<?xml version='1.0' encoding='utf-8'?>
<?grc format='1' created='3.7.10'?>
<flow_graph>
  <timestamp>Fri Jul  1 17:53:00 2016</timestamp>
  <block>
    <key>options</key>
    <param>
      <key>author</key>
      <value>Manolis Surligas (surligas@gmail.com)</value>
    </param>
    <param>
      <key>window_size</key>
      <value>1768,1080</value>
    </param>
    <param>
      <key>category</key>
      <value>Custom</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>description</key>
      <value>SATNOGS transceiver for UPSAT satellite</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(8, 12)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>generate_options</key>
      <value>qt_gui</value>
    </param>
    <param>
      <key>hier_block_src_path</key>
      <value>.:</value>
    </param>
    <param>
      <key>id</key>
      <value>upsat_transceiver_qt</value>
    </param>
    <param>
      <key>max_nouts</key>
      <value>0</value>
    </param>
    <param>
      <key>qt_qss_theme</key>
      <value></value>
    </param>
    <param>
      <key>realtime_scheduling</key>
      <value></value>
    </param>
    <param>
      <key>run_command</key>
      <value>{python} -u {filename}</value>
    </param>
    <param>
      <key>run_options</key>
      <value>prompt</value>
    </param>
    <param>
      <key>run</key>
      <value>True</value>
    </param>
    <param>
      <key>thread_safe_setters</key>
      <value></value>
    </param>
    <param>
      <key>title</key>
      <value>UPSat Transceiver QT</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>FSK baud rate</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1048, 16)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>baud_rate_downlink</value>
    </param>
    <param>
      <key>value</key>
      <value>9600</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>FSK baud rate</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1048, 112)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>baud_rate_uplink</value>
    </param>
    <param>
      <key>value</key>
      <value>1200</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>Decimation factor
for the RX after the
SDR received samples</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(696, 20)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>decimation_rx</value>
    </param>
    <param>
      <key>value</key>
      <value>20</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>The FSK frequency deviation</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(840, 20)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>deviation</value>
    </param>
    <param>
      <key>value</key>
      <value>3.9973e3</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(168, 932)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>first_stage_samp_rate_rx</value>
    </param>
    <param>
      <key>value</key>
      <value>samp_rate_rx / decimation_rx</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(16, 904)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>gaussian_taps</value>
    </param>
    <param>
      <key>value</key>
      <value>filter.firdes.gaussian(1.0, samples_per_symbol_tx, 1.0, 4*samples_per_symbol_tx)</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(168, 1004)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>interp_taps</value>
    </param>
    <param>
      <key>value</key>
      <value>numpy.convolve(numpy.array(gaussian_taps), numpy.array(sq_wave))</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(296, 16)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>modulation_index_downlink</value>
    </param>
    <param>
      <key>value</key>
      <value>deviation / (baud_rate_downlink / 2.0)</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(296, 80)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>modulation_index_uplink</value>
    </param>
    <param>
      <key>value</key>
      <value>deviation / (baud_rate_uplink / 2.0)</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>The RX center frequency
 of the system</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1368, 16)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>rx_frequency</value>
    </param>
    <param>
      <key>value</key>
      <value>435.765e6</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>SDR device 
TX sampling rate</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(752, 900)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>value</key>
      <value>satnogs.hw_rx_settings[rx_sdr_device]['samp_rate']</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>SDR device 
TX sampling rate</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(760, 776)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>samp_rate_tx</value>
    </param>
    <param>
      <key>value</key>
      <value>satnogs.hw_tx_settings[rx_sdr_device]['samp_rate']</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>Samples per FSK symbol.
Should be changed only for better
spectrum mask, or if the resampling
is too great and becomes a bottlneck.</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(472, 12)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>samples_per_symbol_tx</value>
    </param>
    <param>
      <key>value</key>
      <value>4*8</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(16, 984)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>sq_wave</value>
    </param>
    <param>
      <key>value</key>
      <value>(1.0, ) * samples_per_symbol_tx</value>
    </param>
  </block>
  <block>
    <key>variable_low_pass_filter_taps</key>
    <param>
      <key>beta</key>
      <value>6.76</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>cutoff_freq</key>
      <value>20000</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(16, 760)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>gain</key>
      <value>1.0</value>
    </param>
    <param>
      <key>id</key>
      <value>taps</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>width</key>
      <value>60000</value>
    </param>
    <param>
      <key>win</key>
      <value>firdes.WIN_HAMMING</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>The TX center frequency
 of the system</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1216, 16)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>tx_frequency</value>
    </param>
    <param>
      <key>value</key>
      <value>145.835e6</value>
    </param>
  </block>
  <block>
    <key>analog_frequency_modulator_fc</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(792, 232)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>analog_frequency_modulator_fc_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>sensitivity</key>
      <value>(math.pi*modulation_index_uplink) / samples_per_symbol_tx</value>
    </param>
  </block>
  <block>
    <key>analog_quadrature_demod_cf</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(552, 528)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>gain</key>
      <value>((first_stage_samp_rate_rx) / baud_rate_downlink)/(math.pi*modulation_index_downlink)</value>
    </param>
    <param>
      <key>id</key>
      <value>analog_quadrature_demod_cf_0_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
  </block>
  <block>
    <key>analog_sig_source_x</key>
    <param>
      <key>amp</key>
      <value>1</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>freq</key>
      <value>lo_offset </value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(952, 272)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>analog_sig_source_x_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>offset</key>
      <value>0</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_tx</value>
    </param>
    <param>
      <key>waveform</key>
      <value>analog.GR_COS_WAVE</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(272, 756)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>bind_addr</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>0.0.0.0</value>
    </param>
  </block>
  <block>
    <key>blocks_multiply_xx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(832, 352)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>blocks_multiply_xx_0</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>num_inputs</key>
      <value>2</value>
    </param>
    <param>
      <key>vlen</key>
      <value>1</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(272, 844)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>dest_addr</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>127.0.0.1</value>
    </param>
  </block>
  <block>
    <key>digital_binary_slicer_fb</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(944, 528)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>digital_binary_slicer_fb_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
  </block>
  <block>
    <key>digital_clock_recovery_mm_xx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(736, 496)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>gain_mu</key>
      <value>0.175</value>
    </param>
    <param>
      <key>gain_omega</key>
      <value>0.25*0.175*0.175</value>
    </param>
    <param>
      <key>id</key>
      <value>digital_clock_recovery_mm_xx_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>mu</key>
      <value>0.5</value>
    </param>
    <param>
      <key>omega_relative_limit</key>
      <value>0.005</value>
    </param>
    <param>
      <key>omega</key>
      <value>first_stage_samp_rate_rx/baud_rate_downlink</value>
    </param>
    <param>
      <key>type</key>
      <value>float</value>
    </param>
  </block>
  <block>
    <key>freq_xlating_fir_filter_xxx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>center_freq</key>
      <value>lo_offset</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>decim</key>
      <value>decimation_rx</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(304, 504)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>freq_xlating_fir_filter_xxx_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>taps</key>
      <value>taps</value>
    </param>
    <param>
      <key>type</key>
      <value>ccc</value>
    </param>
  </block>
  <block>
    <key>import</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(184, 64)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>import_0</value>
    </param>
    <param>
      <key>import</key>
      <value>import numpy</value>
    </param>
  </block>
  <block>
    <key>import</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(184, 16)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>import_0_0</value>
    </param>
    <param>
      <key>import</key>
      <value>import math</value>
    </param>
  </block>
  <block>
    <key>import</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(184, 112)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>import_0_1</value>
    </param>
    <param>
      <key>import</key>
      <value>from gnuradio import filter</value>
    </param>
  </block>
  <block>
    <key>interp_fir_filter_xxx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(592, 224)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>interp_fir_filter_xxx_0</value>
    </param>
    <param>
      <key>interp</key>
      <value>samples_per_symbol_tx</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>samp_delay</key>
      <value>0</value>
    </param>
    <param>
      <key>taps</key>
      <value>interp_taps</value>
    </param>
    <param>
      <key>type</key>
      <value>fff</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value>To avoid the SDR carrier at the DC
we shift the LO a little further</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(888, 772)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>lo_offset</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>eng_float</value>
    </param>
    <param>
      <key>value</key>
      <value>100e3</value>
    </param>
  </block>
  <block>
    <key>osmosdr_sink</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>ant0</key>
      <value>satnogs.hw_tx_settings[tx_sdr_device]['antenna']</value>
    </param>
    <param>
      <key>bb_gain0</key>
      <value>satnogs.hw_tx_settings[tx_sdr_device]['bb_gain']</value>
    </param>
    <param>
      <key>bw0</key>
      <value>samp_rate_tx</value>
    </param>
    <param>
      <key>corr0</key>
      <value>0</value>
    </param>
    <param>
      <key>freq0</key>
      <value>tx_frequency - lo_offset</value>
    </param>
    <param>
      <key>if_gain0</key>
      <value>satnogs.hw_tx_settings[tx_sdr_device]['if_gain']</value>
    </param>
    <param>
      <key>gain0</key>
      <value>satnogs.hw_tx_settings[tx_sdr_device]['rf_gain']</value>
    </param>
    <param>
      <key>ant10</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain10</key>
      <value>20</value>
    </param>
    <param>
      <key>bw10</key>
      <value>0</value>
    </param>
    <param>
      <key>corr10</key>
      <value>0</value>
    </param>
    <param>
      <key>freq10</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain10</key>
      <value>20</value>
    </param>
    <param>
      <key>gain10</key>
      <value>10</value>
    </param>
    <param>
      <key>ant11</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain11</key>
      <value>20</value>
    </param>
    <param>
      <key>bw11</key>
      <value>0</value>
    </param>
    <param>
      <key>corr11</key>
      <value>0</value>
    </param>
    <param>
      <key>freq11</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain11</key>
      <value>20</value>
    </param>
    <param>
      <key>gain11</key>
      <value>10</value>
    </param>
    <param>
      <key>ant12</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain12</key>
      <value>20</value>
    </param>
    <param>
      <key>bw12</key>
      <value>0</value>
    </param>
    <param>
      <key>corr12</key>
      <value>0</value>
    </param>
    <param>
      <key>freq12</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain12</key>
      <value>20</value>
    </param>
    <param>
      <key>gain12</key>
      <value>10</value>
    </param>
    <param>
      <key>ant13</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain13</key>
      <value>20</value>
    </param>
    <param>
      <key>bw13</key>
      <value>0</value>
    </param>
    <param>
      <key>corr13</key>
      <value>0</value>
    </param>
    <param>
      <key>freq13</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain13</key>
      <value>20</value>
    </param>
    <param>
      <key>gain13</key>
      <value>10</value>
    </param>
    <param>
      <key>ant14</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain14</key>
      <value>20</value>
    </param>
    <param>
      <key>bw14</key>
      <value>0</value>
    </param>
    <param>
      <key>corr14</key>
      <value>0</value>
    </param>
    <param>
      <key>freq14</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain14</key>
      <value>20</value>
    </param>
    <param>
      <key>gain14</key>
      <value>10</value>
    </param>
    <param>
      <key>ant15</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain15</key>
      <value>20</value>
    </param>
    <param>
      <key>bw15</key>
      <value>0</value>
    </param>
    <param>
      <key>corr15</key>
      <value>0</value>
    </param>
    <param>
      <key>freq15</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain15</key>
      <value>20</value>
    </param>
    <param>
      <key>gain15</key>
      <value>10</value>
    </param>
    <param>
      <key>ant16</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain16</key>
      <value>20</value>
    </param>
    <param>
      <key>bw16</key>
      <value>0</value>
    </param>
    <param>
      <key>corr16</key>
      <value>0</value>
    </param>
    <param>
      <key>freq16</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain16</key>
      <value>20</value>
    </param>
    <param>
      <key>gain16</key>
      <value>10</value>
    </param>
    <param>
      <key>ant17</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain17</key>
      <value>20</value>
    </param>
    <param>
      <key>bw17</key>
      <value>0</value>
    </param>
    <param>
      <key>corr17</key>
      <value>0</value>
    </param>
    <param>
      <key>freq17</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain17</key>
      <value>20</value>
    </param>
    <param>
      <key>gain17</key>
      <value>10</value>
    </param>
    <param>
      <key>ant18</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain18</key>
      <value>20</value>
    </param>
    <param>
      <key>bw18</key>
      <value>0</value>
    </param>
    <param>
      <key>corr18</key>
      <value>0</value>
    </param>
    <param>
      <key>freq18</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain18</key>
      <value>20</value>
    </param>
    <param>
      <key>gain18</key>
      <value>10</value>
    </param>
    <param>
      <key>ant19</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain19</key>
      <value>20</value>
    </param>
    <param>
      <key>bw19</key>
      <value>0</value>
    </param>
    <param>
      <key>corr19</key>
      <value>0</value>
    </param>
    <param>
      <key>freq19</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain19</key>
      <value>20</value>
    </param>
    <param>
      <key>gain19</key>
      <value>10</value>
    </param>
    <param>
      <key>ant1</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain1</key>
      <value>20</value>
    </param>
    <param>
      <key>bw1</key>
      <value>0</value>
    </param>
    <param>
      <key>corr1</key>
      <value>0</value>
    </param>
    <param>
      <key>freq1</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain1</key>
      <value>20</value>
    </param>
    <param>
      <key>gain1</key>
      <value>10</value>
    </param>
    <param>
      <key>ant20</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain20</key>
      <value>20</value>
    </param>
    <param>
      <key>bw20</key>
      <value>0</value>
    </param>
    <param>
      <key>corr20</key>
      <value>0</value>
    </param>
    <param>
      <key>freq20</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain20</key>
      <value>20</value>
    </param>
    <param>
      <key>gain20</key>
      <value>10</value>
    </param>
    <param>
      <key>ant21</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain21</key>
      <value>20</value>
    </param>
    <param>
      <key>bw21</key>
      <value>0</value>
    </param>
    <param>
      <key>corr21</key>
      <value>0</value>
    </param>
    <param>
      <key>freq21</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain21</key>
      <value>20</value>
    </param>
    <param>
      <key>gain21</key>
      <value>10</value>
    </param>
    <param>
      <key>ant22</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain22</key>
      <value>20</value>
    </param>
    <param>
      <key>bw22</key>
      <value>0</value>
    </param>
    <param>
      <key>corr22</key>
      <value>0</value>
    </param>
    <param>
      <key>freq22</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain22</key>
      <value>20</value>
    </param>
    <param>
      <key>gain22</key>
      <value>10</value>
    </param>
    <param>
      <key>ant23</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain23</key>
      <value>20</value>
    </param>
    <param>
      <key>bw23</key>
      <value>0</value>
    </param>
    <param>
      <key>corr23</key>
      <value>0</value>
    </param>
    <param>
      <key>freq23</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain23</key>
      <value>20</value>
    </param>
    <param>
      <key>gain23</key>
      <value>10</value>
    </param>
    <param>
      <key>ant24</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain24</key>
      <value>20</value>
    </param>
    <param>
      <key>bw24</key>
      <value>0</value>
    </param>
    <param>
      <key>corr24</key>
      <value>0</value>
    </param>
    <param>
      <key>freq24</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain24</key>
      <value>20</value>
    </param>
    <param>
      <key>gain24</key>
      <value>10</value>
    </param>
    <param>
      <key>ant25</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain25</key>
      <value>20</value>
    </param>
    <param>
      <key>bw25</key>
      <value>0</value>
    </param>
    <param>
      <key>corr25</key>
      <value>0</value>
    </param>
    <param>
      <key>freq25</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain25</key>
      <value>20</value>
    </param>
    <param>
      <key>gain25</key>
      <value>10</value>
    </param>
    <param>
      <key>ant26</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain26</key>
      <value>20</value>
    </param>
    <param>
      <key>bw26</key>
      <value>0</value>
    </param>
    <param>
      <key>corr26</key>
      <value>0</value>
    </param>
    <param>
      <key>freq26</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain26</key>
      <value>20</value>
    </param>
    <param>
      <key>gain26</key>
      <value>10</value>
    </param>
    <param>
      <key>ant27</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain27</key>
      <value>20</value>
    </param>
    <param>
      <key>bw27</key>
      <value>0</value>
    </param>
    <param>
      <key>corr27</key>
      <value>0</value>
    </param>
    <param>
      <key>freq27</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain27</key>
      <value>20</value>
    </param>
    <param>
      <key>gain27</key>
      <value>10</value>
    </param>
    <param>
      <key>ant28</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain28</key>
      <value>20</value>
    </param>
    <param>
      <key>bw28</key>
      <value>0</value>
    </param>
    <param>
      <key>corr28</key>
      <value>0</value>
    </param>
    <param>
      <key>freq28</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain28</key>
      <value>20</value>
    </param>
    <param>
      <key>gain28</key>
      <value>10</value>
    </param>
    <param>
      <key>ant29</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain29</key>
      <value>20</value>
    </param>
    <param>
      <key>bw29</key>
      <value>0</value>
    </param>
    <param>
      <key>corr29</key>
      <value>0</value>
    </param>
    <param>
      <key>freq29</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain29</key>
      <value>20</value>
    </param>
    <param>
      <key>gain29</key>
      <value>10</value>
    </param>
    <param>
      <key>ant2</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain2</key>
      <value>20</value>
    </param>
    <param>
      <key>bw2</key>
      <value>0</value>
    </param>
    <param>
      <key>corr2</key>
      <value>0</value>
    </param>
    <param>
      <key>freq2</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain2</key>
      <value>20</value>
    </param>
    <param>
      <key>gain2</key>
      <value>10</value>
    </param>
    <param>
      <key>ant30</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain30</key>
      <value>20</value>
    </param>
    <param>
      <key>bw30</key>
      <value>0</value>
    </param>
    <param>
      <key>corr30</key>
      <value>0</value>
    </param>
    <param>
      <key>freq30</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain30</key>
      <value>20</value>
    </param>
    <param>
      <key>gain30</key>
      <value>10</value>
    </param>
    <param>
      <key>ant31</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain31</key>
      <value>20</value>
    </param>
    <param>
      <key>bw31</key>
      <value>0</value>
    </param>
    <param>
      <key>corr31</key>
      <value>0</value>
    </param>
    <param>
      <key>freq31</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain31</key>
      <value>20</value>
    </param>
    <param>
      <key>gain31</key>
      <value>10</value>
    </param>
    <param>
      <key>ant3</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain3</key>
      <value>20</value>
    </param>
    <param>
      <key>bw3</key>
      <value>0</value>
    </param>
    <param>
      <key>corr3</key>
      <value>0</value>
    </param>
    <param>
      <key>freq3</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain3</key>
      <value>20</value>
    </param>
    <param>
      <key>gain3</key>
      <value>10</value>
    </param>
    <param>
      <key>ant4</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain4</key>
      <value>20</value>
    </param>
    <param>
      <key>bw4</key>
      <value>0</value>
    </param>
    <param>
      <key>corr4</key>
      <value>0</value>
    </param>
    <param>
      <key>freq4</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain4</key>
      <value>20</value>
    </param>
    <param>
      <key>gain4</key>
      <value>10</value>
    </param>
    <param>
      <key>ant5</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain5</key>
      <value>20</value>
    </param>
    <param>
      <key>bw5</key>
      <value>0</value>
    </param>
    <param>
      <key>corr5</key>
      <value>0</value>
    </param>
    <param>
      <key>freq5</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain5</key>
      <value>20</value>
    </param>
    <param>
      <key>gain5</key>
      <value>10</value>
    </param>
    <param>
      <key>ant6</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain6</key>
      <value>20</value>
    </param>
    <param>
      <key>bw6</key>
      <value>0</value>
    </param>
    <param>
      <key>corr6</key>
      <value>0</value>
    </param>
    <param>
      <key>freq6</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain6</key>
      <value>20</value>
    </param>
    <param>
      <key>gain6</key>
      <value>10</value>
    </param>
    <param>
      <key>ant7</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain7</key>
      <value>20</value>
    </param>
    <param>
      <key>bw7</key>
      <value>0</value>
    </param>
    <param>
      <key>corr7</key>
      <value>0</value>
    </param>
    <param>
      <key>freq7</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain7</key>
      <value>20</value>
    </param>
    <param>
      <key>gain7</key>
      <value>10</value>
    </param>
    <param>
      <key>ant8</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain8</key>
      <value>20</value>
    </param>
    <param>
      <key>bw8</key>
      <value>0</value>
    </param>
    <param>
      <key>corr8</key>
      <value>0</value>
    </param>
    <param>
      <key>freq8</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain8</key>
      <value>20</value>
    </param>
    <param>
      <key>gain8</key>
      <value>10</value>
    </param>
    <param>
      <key>ant9</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain9</key>
      <value>20</value>
    </param>
    <param>
      <key>bw9</key>
      <value>0</value>
    </param>
    <param>
      <key>corr9</key>
      <value>0</value>
    </param>
    <param>
      <key>freq9</key>
      <value>100e6</value>
    </param>
    <param>
      <key>if_gain9</key>
      <value>20</value>
    </param>
    <param>
      <key>gain9</key>
      <value>10</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>args</key>
      <value>satnogs.hw_tx_settings[rx_sdr_device]['dev_arg']</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(544, 312)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>osmosdr_sink_0</value>
    </param>
    <param>
      <key>type</key>
      <value>fc32</value>
    </param>
    <param>
      <key>clock_source0</key>
      <value></value>
    </param>
    <param>
      <key>time_source0</key>
      <value></value>
    </param>
    <param>
      <key>clock_source1</key>
      <value></value>
    </param>
    <param>
      <key>time_source1</key>
      <value></value>
    </param>
    <param>
      <key>clock_source2</key>
      <value></value>
    </param>
    <param>
      <key>time_source2</key>
      <value></value>
    </param>
    <param>
      <key>clock_source3</key>
      <value></value>
    </param>
    <param>
      <key>time_source3</key>
      <value></value>
    </param>
    <param>
      <key>clock_source4</key>
      <value></value>
    </param>
    <param>
      <key>time_source4</key>
      <value></value>
    </param>
    <param>
      <key>clock_source5</key>
      <value></value>
    </param>
    <param>
      <key>time_source5</key>
      <value></value>
    </param>
    <param>
      <key>clock_source6</key>
      <value></value>
    </param>
    <param>
      <key>time_source6</key>
      <value></value>
    </param>
    <param>
      <key>clock_source7</key>
      <value></value>
    </param>
    <param>
      <key>time_source7</key>
      <value></value>
    </param>
    <param>
      <key>nchan</key>
      <value>1</value>
    </param>
    <param>
      <key>num_mboards</key>
      <value>1</value>
    </param>
    <param>
      <key>sample_rate</key>
      <value>samp_rate_tx</value>
    </param>
    <param>
      <key>sync</key>
      <value></value>
    </param>
  </block>
  <block>
    <key>osmosdr_source</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>ant0</key>
      <value>satnogs.hw_rx_settings[rx_sdr_device]['antenna']</value>
    </param>
    <param>
      <key>bb_gain0</key>
      <value>satnogs.hw_rx_settings[rx_sdr_device]['bb_gain']</value>
    </param>
    <param>
      <key>bw0</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>dc_offset_mode0</key>
      <value>0</value>
    </param>
    <param>
      <key>corr0</key>
      <value>0</value>
    </param>
    <param>
      <key>freq0</key>
      <value>rx_frequency - lo_offset</value>
    </param>
    <param>
      <key>gain_mode0</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain0</key>
      <value>satnogs.hw_rx_settings[rx_sdr_device]['if_gain']</value>
    </param>
    <param>
      <key>iq_balance_mode0</key>
      <value>0</value>
    </param>
    <param>
      <key>gain0</key>
      <value>satnogs.hw_rx_settings[rx_sdr_device]['rf_gain']</value>
    </param>
    <param>
      <key>ant10</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain10</key>
      <value>20</value>
    </param>
    <param>
      <key>bw10</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode10</key>
      <value>0</value>
    </param>
    <param>
      <key>corr10</key>
      <value>0</value>
    </param>
    <param>
      <key>freq10</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode10</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain10</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode10</key>
      <value>0</value>
    </param>
    <param>
      <key>gain10</key>
      <value>10</value>
    </param>
    <param>
      <key>ant11</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain11</key>
      <value>20</value>
    </param>
    <param>
      <key>bw11</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode11</key>
      <value>0</value>
    </param>
    <param>
      <key>corr11</key>
      <value>0</value>
    </param>
    <param>
      <key>freq11</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode11</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain11</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode11</key>
      <value>0</value>
    </param>
    <param>
      <key>gain11</key>
      <value>10</value>
    </param>
    <param>
      <key>ant12</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain12</key>
      <value>20</value>
    </param>
    <param>
      <key>bw12</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode12</key>
      <value>0</value>
    </param>
    <param>
      <key>corr12</key>
      <value>0</value>
    </param>
    <param>
      <key>freq12</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode12</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain12</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode12</key>
      <value>0</value>
    </param>
    <param>
      <key>gain12</key>
      <value>10</value>
    </param>
    <param>
      <key>ant13</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain13</key>
      <value>20</value>
    </param>
    <param>
      <key>bw13</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode13</key>
      <value>0</value>
    </param>
    <param>
      <key>corr13</key>
      <value>0</value>
    </param>
    <param>
      <key>freq13</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode13</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain13</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode13</key>
      <value>0</value>
    </param>
    <param>
      <key>gain13</key>
      <value>10</value>
    </param>
    <param>
      <key>ant14</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain14</key>
      <value>20</value>
    </param>
    <param>
      <key>bw14</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode14</key>
      <value>0</value>
    </param>
    <param>
      <key>corr14</key>
      <value>0</value>
    </param>
    <param>
      <key>freq14</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode14</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain14</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode14</key>
      <value>0</value>
    </param>
    <param>
      <key>gain14</key>
      <value>10</value>
    </param>
    <param>
      <key>ant15</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain15</key>
      <value>20</value>
    </param>
    <param>
      <key>bw15</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode15</key>
      <value>0</value>
    </param>
    <param>
      <key>corr15</key>
      <value>0</value>
    </param>
    <param>
      <key>freq15</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode15</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain15</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode15</key>
      <value>0</value>
    </param>
    <param>
      <key>gain15</key>
      <value>10</value>
    </param>
    <param>
      <key>ant16</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain16</key>
      <value>20</value>
    </param>
    <param>
      <key>bw16</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode16</key>
      <value>0</value>
    </param>
    <param>
      <key>corr16</key>
      <value>0</value>
    </param>
    <param>
      <key>freq16</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode16</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain16</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode16</key>
      <value>0</value>
    </param>
    <param>
      <key>gain16</key>
      <value>10</value>
    </param>
    <param>
      <key>ant17</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain17</key>
      <value>20</value>
    </param>
    <param>
      <key>bw17</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode17</key>
      <value>0</value>
    </param>
    <param>
      <key>corr17</key>
      <value>0</value>
    </param>
    <param>
      <key>freq17</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode17</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain17</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode17</key>
      <value>0</value>
    </param>
    <param>
      <key>gain17</key>
      <value>10</value>
    </param>
    <param>
      <key>ant18</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain18</key>
      <value>20</value>
    </param>
    <param>
      <key>bw18</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode18</key>
      <value>0</value>
    </param>
    <param>
      <key>corr18</key>
      <value>0</value>
    </param>
    <param>
      <key>freq18</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode18</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain18</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode18</key>
      <value>0</value>
    </param>
    <param>
      <key>gain18</key>
      <value>10</value>
    </param>
    <param>
      <key>ant19</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain19</key>
      <value>20</value>
    </param>
    <param>
      <key>bw19</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode19</key>
      <value>0</value>
    </param>
    <param>
      <key>corr19</key>
      <value>0</value>
    </param>
    <param>
      <key>freq19</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode19</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain19</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode19</key>
      <value>0</value>
    </param>
    <param>
      <key>gain19</key>
      <value>10</value>
    </param>
    <param>
      <key>ant1</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain1</key>
      <value>20</value>
    </param>
    <param>
      <key>bw1</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode1</key>
      <value>0</value>
    </param>
    <param>
      <key>corr1</key>
      <value>0</value>
    </param>
    <param>
      <key>freq1</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode1</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain1</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode1</key>
      <value>0</value>
    </param>
    <param>
      <key>gain1</key>
      <value>10</value>
    </param>
    <param>
      <key>ant20</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain20</key>
      <value>20</value>
    </param>
    <param>
      <key>bw20</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode20</key>
      <value>0</value>
    </param>
    <param>
      <key>corr20</key>
      <value>0</value>
    </param>
    <param>
      <key>freq20</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode20</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain20</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode20</key>
      <value>0</value>
    </param>
    <param>
      <key>gain20</key>
      <value>10</value>
    </param>
    <param>
      <key>ant21</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain21</key>
      <value>20</value>
    </param>
    <param>
      <key>bw21</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode21</key>
      <value>0</value>
    </param>
    <param>
      <key>corr21</key>
      <value>0</value>
    </param>
    <param>
      <key>freq21</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode21</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain21</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode21</key>
      <value>0</value>
    </param>
    <param>
      <key>gain21</key>
      <value>10</value>
    </param>
    <param>
      <key>ant22</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain22</key>
      <value>20</value>
    </param>
    <param>
      <key>bw22</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode22</key>
      <value>0</value>
    </param>
    <param>
      <key>corr22</key>
      <value>0</value>
    </param>
    <param>
      <key>freq22</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode22</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain22</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode22</key>
      <value>0</value>
    </param>
    <param>
      <key>gain22</key>
      <value>10</value>
    </param>
    <param>
      <key>ant23</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain23</key>
      <value>20</value>
    </param>
    <param>
      <key>bw23</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode23</key>
      <value>0</value>
    </param>
    <param>
      <key>corr23</key>
      <value>0</value>
    </param>
    <param>
      <key>freq23</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode23</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain23</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode23</key>
      <value>0</value>
    </param>
    <param>
      <key>gain23</key>
      <value>10</value>
    </param>
    <param>
      <key>ant24</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain24</key>
      <value>20</value>
    </param>
    <param>
      <key>bw24</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode24</key>
      <value>0</value>
    </param>
    <param>
      <key>corr24</key>
      <value>0</value>
    </param>
    <param>
      <key>freq24</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode24</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain24</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode24</key>
      <value>0</value>
    </param>
    <param>
      <key>gain24</key>
      <value>10</value>
    </param>
    <param>
      <key>ant25</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain25</key>
      <value>20</value>
    </param>
    <param>
      <key>bw25</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode25</key>
      <value>0</value>
    </param>
    <param>
      <key>corr25</key>
      <value>0</value>
    </param>
    <param>
      <key>freq25</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode25</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain25</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode25</key>
      <value>0</value>
    </param>
    <param>
      <key>gain25</key>
      <value>10</value>
    </param>
    <param>
      <key>ant26</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain26</key>
      <value>20</value>
    </param>
    <param>
      <key>bw26</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode26</key>
      <value>0</value>
    </param>
    <param>
      <key>corr26</key>
      <value>0</value>
    </param>
    <param>
      <key>freq26</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode26</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain26</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode26</key>
      <value>0</value>
    </param>
    <param>
      <key>gain26</key>
      <value>10</value>
    </param>
    <param>
      <key>ant27</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain27</key>
      <value>20</value>
    </param>
    <param>
      <key>bw27</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode27</key>
      <value>0</value>
    </param>
    <param>
      <key>corr27</key>
      <value>0</value>
    </param>
    <param>
      <key>freq27</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode27</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain27</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode27</key>
      <value>0</value>
    </param>
    <param>
      <key>gain27</key>
      <value>10</value>
    </param>
    <param>
      <key>ant28</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain28</key>
      <value>20</value>
    </param>
    <param>
      <key>bw28</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode28</key>
      <value>0</value>
    </param>
    <param>
      <key>corr28</key>
      <value>0</value>
    </param>
    <param>
      <key>freq28</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode28</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain28</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode28</key>
      <value>0</value>
    </param>
    <param>
      <key>gain28</key>
      <value>10</value>
    </param>
    <param>
      <key>ant29</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain29</key>
      <value>20</value>
    </param>
    <param>
      <key>bw29</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode29</key>
      <value>0</value>
    </param>
    <param>
      <key>corr29</key>
      <value>0</value>
    </param>
    <param>
      <key>freq29</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode29</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain29</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode29</key>
      <value>0</value>
    </param>
    <param>
      <key>gain29</key>
      <value>10</value>
    </param>
    <param>
      <key>ant2</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain2</key>
      <value>20</value>
    </param>
    <param>
      <key>bw2</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode2</key>
      <value>0</value>
    </param>
    <param>
      <key>corr2</key>
      <value>0</value>
    </param>
    <param>
      <key>freq2</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode2</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain2</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode2</key>
      <value>0</value>
    </param>
    <param>
      <key>gain2</key>
      <value>10</value>
    </param>
    <param>
      <key>ant30</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain30</key>
      <value>20</value>
    </param>
    <param>
      <key>bw30</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode30</key>
      <value>0</value>
    </param>
    <param>
      <key>corr30</key>
      <value>0</value>
    </param>
    <param>
      <key>freq30</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode30</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain30</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode30</key>
      <value>0</value>
    </param>
    <param>
      <key>gain30</key>
      <value>10</value>
    </param>
    <param>
      <key>ant31</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain31</key>
      <value>20</value>
    </param>
    <param>
      <key>bw31</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode31</key>
      <value>0</value>
    </param>
    <param>
      <key>corr31</key>
      <value>0</value>
    </param>
    <param>
      <key>freq31</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode31</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain31</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode31</key>
      <value>0</value>
    </param>
    <param>
      <key>gain31</key>
      <value>10</value>
    </param>
    <param>
      <key>ant3</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain3</key>
      <value>20</value>
    </param>
    <param>
      <key>bw3</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode3</key>
      <value>0</value>
    </param>
    <param>
      <key>corr3</key>
      <value>0</value>
    </param>
    <param>
      <key>freq3</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode3</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain3</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode3</key>
      <value>0</value>
    </param>
    <param>
      <key>gain3</key>
      <value>10</value>
    </param>
    <param>
      <key>ant4</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain4</key>
      <value>20</value>
    </param>
    <param>
      <key>bw4</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode4</key>
      <value>0</value>
    </param>
    <param>
      <key>corr4</key>
      <value>0</value>
    </param>
    <param>
      <key>freq4</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode4</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain4</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode4</key>
      <value>0</value>
    </param>
    <param>
      <key>gain4</key>
      <value>10</value>
    </param>
    <param>
      <key>ant5</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain5</key>
      <value>20</value>
    </param>
    <param>
      <key>bw5</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode5</key>
      <value>0</value>
    </param>
    <param>
      <key>corr5</key>
      <value>0</value>
    </param>
    <param>
      <key>freq5</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode5</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain5</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode5</key>
      <value>0</value>
    </param>
    <param>
      <key>gain5</key>
      <value>10</value>
    </param>
    <param>
      <key>ant6</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain6</key>
      <value>20</value>
    </param>
    <param>
      <key>bw6</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode6</key>
      <value>0</value>
    </param>
    <param>
      <key>corr6</key>
      <value>0</value>
    </param>
    <param>
      <key>freq6</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode6</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain6</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode6</key>
      <value>0</value>
    </param>
    <param>
      <key>gain6</key>
      <value>10</value>
    </param>
    <param>
      <key>ant7</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain7</key>
      <value>20</value>
    </param>
    <param>
      <key>bw7</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode7</key>
      <value>0</value>
    </param>
    <param>
      <key>corr7</key>
      <value>0</value>
    </param>
    <param>
      <key>freq7</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode7</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain7</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode7</key>
      <value>0</value>
    </param>
    <param>
      <key>gain7</key>
      <value>10</value>
    </param>
    <param>
      <key>ant8</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain8</key>
      <value>20</value>
    </param>
    <param>
      <key>bw8</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode8</key>
      <value>0</value>
    </param>
    <param>
      <key>corr8</key>
      <value>0</value>
    </param>
    <param>
      <key>freq8</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode8</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain8</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode8</key>
      <value>0</value>
    </param>
    <param>
      <key>gain8</key>
      <value>10</value>
    </param>
    <param>
      <key>ant9</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain9</key>
      <value>20</value>
    </param>
    <param>
      <key>bw9</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode9</key>
      <value>0</value>
    </param>
    <param>
      <key>corr9</key>
      <value>0</value>
    </param>
    <param>
      <key>freq9</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode9</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain9</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode9</key>
      <value>0</value>
    </param>
    <param>
      <key>gain9</key>
      <value>10</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>args</key>
      <value>satnogs.hw_rx_settings[rx_sdr_device]['dev_arg']</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(64, 440)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>osmosdr_source_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>clock_source0</key>
      <value></value>
    </param>
    <param>
      <key>time_source0</key>
      <value></value>
    </param>
    <param>
      <key>clock_source1</key>
      <value></value>
    </param>
    <param>
      <key>time_source1</key>
      <value></value>
    </param>
    <param>
      <key>clock_source2</key>
      <value></value>
    </param>
    <param>
      <key>time_source2</key>
      <value></value>
    </param>
    <param>
      <key>clock_source3</key>
      <value></value>
    </param>
    <param>
      <key>time_source3</key>
      <value></value>
    </param>
    <param>
      <key>clock_source4</key>
      <value></value>
    </param>
    <param>
      <key>time_source4</key>
      <value></value>
    </param>
    <param>
      <key>clock_source5</key>
      <value></value>
    </param>
    <param>
      <key>time_source5</key>
      <value></value>
    </param>
    <param>
      <key>clock_source6</key>
      <value></value>
    </param>
    <param>
      <key>time_source6</key>
      <value></value>
    </param>
    <param>
      <key>clock_source7</key>
      <value></value>
    </param>
    <param>
      <key>time_source7</key>
      <value></value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>nchan</key>
      <value>1</value>
    </param>
    <param>
      <key>num_mboards</key>
      <value>1</value>
    </param>
    <param>
      <key>type</key>
      <value>fc32</value>
    </param>
    <param>
      <key>sample_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>sync</key>
      <value></value>
    </param>
  </block>
  <block>
    <key>pfb_arb_resampler_xxx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1080, 360)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>pfb_arb_resampler_xxx_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>nfilts</key>
      <value>32</value>
    </param>
    <param>
      <key>rrate</key>
      <value>samp_rate_tx / (baud_rate_uplink * samples_per_symbol_tx)</value>
    </param>
    <param>
      <key>samp_delay</key>
      <value>0</value>
    </param>
    <param>
      <key>atten</key>
      <value>60</value>
    </param>
    <param>
      <key>taps</key>
      <value>firdes.low_pass_2(32, 32, 0.8, 0.1, 60)</value>
    </param>
    <param>
      <key>type</key>
      <value>ccf</value>
    </param>
  </block>
  <block>
    <key>qtgui_freq_sink_x</key>
    <param>
      <key>autoscale</key>
      <value>False</value>
    </param>
    <param>
      <key>average</key>
      <value>1.0</value>
    </param>
    <param>
      <key>axislabels</key>
      <value>True</value>
    </param>
    <param>
      <key>bw</key>
      <value>samp_rate_rx/decimation_rx</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>fc</key>
      <value>0</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>ctrlpanel</key>
      <value>True</value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>fftsize</key>
      <value>1024</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(312, 408)</value>
    </param>
    <param>
      <key>gui_hint</key>
      <value></value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>grid</key>
      <value>True</value>
    </param>
    <param>
      <key>id</key>
      <value>qtgui_freq_sink_x_0</value>
    </param>
    <param>
      <key>legend</key>
      <value>True</value>
    </param>
    <param>
      <key>alpha1</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color1</key>
      <value>"blue"</value>
    </param>
    <param>
      <key>label1</key>
      <value></value>
    </param>
    <param>
      <key>width1</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha10</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color10</key>
      <value>"dark blue"</value>
    </param>
    <param>
      <key>label10</key>
      <value></value>
    </param>
    <param>
      <key>width10</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha2</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color2</key>
      <value>"red"</value>
    </param>
    <param>
      <key>label2</key>
      <value></value>
    </param>
    <param>
      <key>width2</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha3</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color3</key>
      <value>"green"</value>
    </param>
    <param>
      <key>label3</key>
      <value></value>
    </param>
    <param>
      <key>width3</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha4</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color4</key>
      <value>"black"</value>
    </param>
    <param>
      <key>label4</key>
      <value></value>
    </param>
    <param>
      <key>width4</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha5</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color5</key>
      <value>"cyan"</value>
    </param>
    <param>
      <key>label5</key>
      <value></value>
    </param>
    <param>
      <key>width5</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha6</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color6</key>
      <value>"magenta"</value>
    </param>
    <param>
      <key>label6</key>
      <value></value>
    </param>
    <param>
      <key>width6</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha7</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color7</key>
      <value>"yellow"</value>
    </param>
    <param>
      <key>label7</key>
      <value></value>
    </param>
    <param>
      <key>width7</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha8</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color8</key>
      <value>"dark red"</value>
    </param>
    <param>
      <key>label8</key>
      <value></value>
    </param>
    <param>
      <key>width8</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha9</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color9</key>
      <value>"dark green"</value>
    </param>
    <param>
      <key>label9</key>
      <value></value>
    </param>
    <param>
      <key>width9</key>
      <value>1</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>name</key>
      <value>""</value>
    </param>
    <param>
      <key>nconnections</key>
      <value>1</value>
    </param>
    <param>
      <key>showports</key>
      <value>True</value>
    </param>
    <param>
      <key>freqhalf</key>
      <value>True</value>
    </param>
    <param>
      <key>tr_chan</key>
      <value>0</value>
    </param>
    <param>
      <key>tr_level</key>
      <value>0.0</value>
    </param>
    <param>
      <key>tr_mode</key>
      <value>qtgui.TRIG_MODE_FREE</value>
    </param>
    <param>
      <key>tr_tag</key>
      <value>""</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>update_time</key>
      <value>0.01</value>
    </param>
    <param>
      <key>wintype</key>
      <value>firdes.WIN_BLACKMAN_hARRIS</value>
    </param>
    <param>
      <key>label</key>
      <value>Relative Gain</value>
    </param>
    <param>
      <key>ymax</key>
      <value>0</value>
    </param>
    <param>
      <key>ymin</key>
      <value>-140</value>
    </param>
    <param>
      <key>units</key>
      <value>dB</value>
    </param>
  </block>
  <block>
    <key>qtgui_waterfall_sink_x</key>
    <param>
      <key>axislabels</key>
      <value>True</value>
    </param>
    <param>
      <key>bw</key>
      <value>50e3</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>fc</key>
      <value>0</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>fftsize</key>
      <value>1024</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(296, 628)</value>
    </param>
    <param>
      <key>gui_hint</key>
      <value></value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>grid</key>
      <value>False</value>
    </param>
    <param>
      <key>id</key>
      <value>qtgui_waterfall_sink_x_0</value>
    </param>
    <param>
      <key>int_max</key>
      <value>10</value>
    </param>
    <param>
      <key>int_min</key>
      <value>-140</value>
    </param>
    <param>
      <key>legend</key>
      <value>True</value>
    </param>
    <param>
      <key>alpha1</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color1</key>
      <value>0</value>
    </param>
    <param>
      <key>label1</key>
      <value></value>
    </param>
    <param>
      <key>alpha10</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color10</key>
      <value>0</value>
    </param>
    <param>
      <key>label10</key>
      <value></value>
    </param>
    <param>
      <key>alpha2</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color2</key>
      <value>0</value>
    </param>
    <param>
      <key>label2</key>
      <value></value>
    </param>
    <param>
      <key>alpha3</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color3</key>
      <value>0</value>
    </param>
    <param>
      <key>label3</key>
      <value></value>
    </param>
    <param>
      <key>alpha4</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color4</key>
      <value>0</value>
    </param>
    <param>
      <key>label4</key>
      <value></value>
    </param>
    <param>
      <key>alpha5</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color5</key>
      <value>0</value>
    </param>
    <param>
      <key>label5</key>
      <value></value>
    </param>
    <param>
      <key>alpha6</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color6</key>
      <value>0</value>
    </param>
    <param>
      <key>label6</key>
      <value></value>
    </param>
    <param>
      <key>alpha7</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color7</key>
      <value>0</value>
    </param>
    <param>
      <key>label7</key>
      <value></value>
    </param>
    <param>
      <key>alpha8</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color8</key>
      <value>0</value>
    </param>
    <param>
      <key>label8</key>
      <value></value>
    </param>
    <param>
      <key>alpha9</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color9</key>
      <value>0</value>
    </param>
    <param>
      <key>label9</key>
      <value></value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>name</key>
      <value>""</value>
    </param>
    <param>
      <key>nconnections</key>
      <value>1</value>
    </param>
    <param>
      <key>showports</key>
      <value>True</value>
    </param>
    <param>
      <key>freqhalf</key>
      <value>True</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>update_time</key>
      <value>0.10</value>
    </param>
    <param>
      <key>wintype</key>
      <value>firdes.WIN_BLACKMAN_hARRIS</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(168, 756)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>recv_port</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>intx</value>
    </param>
    <param>
      <key>value</key>
      <value>16886</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(648, 900)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>rx_sdr_device</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>usrpb200</value>
    </param>
  </block>
  <block>
    <key>satnogs_ax25_decoder_bm</key>
    <param>
      <key>n_sync_flags</key>
      <value>3</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>descrambling</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1312, 584)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_ax25_decoder_bm_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>max_frame_len</key>
      <value>256</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>promisc</key>
      <value>False</value>
    </param>
    <param>
      <key>addr</key>
      <value>'GND'</value>
    </param>
    <param>
      <key>ssid</key>
      <value>0</value>
    </param>
  </block>
  <block>
    <key>satnogs_multi_format_msg_sink</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1080, 560)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_multi_format_msg_sink_0</value>
    </param>
    <param>
      <key>format</key>
      <value>1</value>
    </param>
  </block>
  <block>
    <key>satnogs_qb50_deframer</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(968, 624)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_qb50_deframer_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>wod_ssid</key>
      <value>0xe</value>
    </param>
  </block>
  <block>
    <key>satnogs_udp_msg_sink</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(728, 672)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_udp_msg_sink_0_0</value>
    </param>
    <param>
      <key>addr</key>
      <value>dest_addr</value>
    </param>
    <param>
      <key>mtu</key>
      <value>1500</value>
    </param>
    <param>
      <key>port</key>
      <value>send_port</value>
    </param>
  </block>
  <block>
    <key>satnogs_udp_msg_sink</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(728, 600)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_udp_msg_sink_0_0_0</value>
    </param>
    <param>
      <key>addr</key>
      <value>dest_addr</value>
    </param>
    <param>
      <key>mtu</key>
      <value>1500</value>
    </param>
    <param>
      <key>port</key>
      <value>wod_port</value>
    </param>
  </block>
  <block>
    <key>satnogs_udp_msg_source</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value>The transmitter can also receive payloads 
from a UDP source. Use netcat or something
similar to produce dynamic payloads.</value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(16, 208)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_udp_msg_source_0</value>
    </param>
    <param>
      <key>addr</key>
      <value>bind_addr</value>
    </param>
    <param>
      <key>mtu</key>
      <value>1500</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>msg_type</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>port</key>
      <value>recv_port</value>
    </param>
  </block>
  <block>
    <key>satnogs_upsat_fsk_frame_encoder</key>
    <param>
      <key>append_crc</key>
      <value>False</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>dest_addr</key>
      <value>ON02GR</value>
    </param>
    <param>
      <key>dest_ssid</key>
      <value>0</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>preamble</key>
      <value>[0x33]*8 </value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(304, 152)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_upsat_fsk_frame_encoder_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>settling_samples</key>
      <value>64</value>
    </param>
    <param>
      <key>msb_first</key>
      <value>True</value>
    </param>
    <param>
      <key>src_addr</key>
      <value>ABCD</value>
    </param>
    <param>
      <key>src_ssid</key>
      <value>0</value>
    </param>
    <param>
      <key>sync_word</key>
      <value>[0x7A, 0x0E]</value>
    </param>
    <param>
      <key>ax_25</key>
      <value>True</value>
    </param>
    <param>
      <key>manchester</key>
      <value>False</value>
    </param>
    <param>
      <key>whitening</key>
      <value>False</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(168, 844)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>send_port</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>intx</value>
    </param>
    <param>
      <key>value</key>
      <value>5022</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(648, 776)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>tx_sdr_device</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>usrpb200</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(552, 780)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>wod_port</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>intx</value>
    </param>
    <param>
      <key>value</key>
      <value>5023</value>
    </param>
  </block>
  <connection>
    <source_block_id>analog_frequency_modulator_fc_0</source_block_id>
    <sink_block_id>pfb_arb_resampler_xxx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>analog_quadrature_demod_cf_0_0</source_block_id>
    <sink_block_id>digital_clock_recovery_mm_xx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>analog_sig_source_x_0</source_block_id>
    <sink_block_id>blocks_multiply_xx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>1</sink_key>
  </connection>
  <connection>
    <source_block_id>blocks_multiply_xx_0</source_block_id>
    <sink_block_id>osmosdr_sink_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>digital_binary_slicer_fb_0</source_block_id>
    <sink_block_id>satnogs_ax25_decoder_bm_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>digital_clock_recovery_mm_xx_0</source_block_id>
    <sink_block_id>digital_binary_slicer_fb_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>freq_xlating_fir_filter_xxx_0</source_block_id>
    <sink_block_id>analog_quadrature_demod_cf_0_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>freq_xlating_fir_filter_xxx_0</source_block_id>
    <sink_block_id>qtgui_freq_sink_x_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>freq_xlating_fir_filter_xxx_0</source_block_id>
    <sink_block_id>qtgui_waterfall_sink_x_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>interp_fir_filter_xxx_0</source_block_id>
    <sink_block_id>analog_frequency_modulator_fc_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>osmosdr_source_0</source_block_id>
    <sink_block_id>freq_xlating_fir_filter_xxx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>pfb_arb_resampler_xxx_0</source_block_id>
    <sink_block_id>blocks_multiply_xx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_ax25_decoder_bm_0</source_block_id>
    <sink_block_id>satnogs_multi_format_msg_sink_0</sink_block_id>
    <source_key>failed_pdu</source_key>
    <sink_key>in</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_ax25_decoder_bm_0</source_block_id>
    <sink_block_id>satnogs_qb50_deframer_0</sink_block_id>
    <source_key>pdu</source_key>
    <sink_key>in</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_qb50_deframer_0</source_block_id>
    <sink_block_id>satnogs_udp_msg_sink_0_0</sink_block_id>
    <source_key>out</source_key>
    <sink_key>in</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_qb50_deframer_0</source_block_id>
    <sink_block_id>satnogs_udp_msg_sink_0_0_0</sink_block_id>
    <source_key>wod</source_key>
    <sink_key>in</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_udp_msg_source_0</source_block_id>
    <sink_block_id>satnogs_upsat_fsk_frame_encoder_0</sink_block_id>
    <source_key>msg</source_key>
    <sink_key>pdu</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_upsat_fsk_frame_encoder_0</source_block_id>
    <sink_block_id>interp_fir_filter_xxx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
</flow_graph>
