<?xml version='1.0' encoding='utf-8'?>
<?grc format='1' created='3.7.11'?>
<flow_graph>
  <timestamp>Thu May  5 00:22:45 2016</timestamp>
  <block>
    <key>options</key>
    <param>
      <key>author</key>
      <value>surligas, cshields, csete</value>
    </param>
    <param>
      <key>window_size</key>
      <value>3000, 3000</value>
    </param>
    <param>
      <key>category</key>
      <value>Custom</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>description</key>
      <value>A generic BPSK demodulation block</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(8, 8)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>generate_options</key>
      <value>no_gui</value>
    </param>
    <param>
      <key>hier_block_src_path</key>
      <value>.:</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_bpsk_demod</value>
    </param>
    <param>
      <key>max_nouts</key>
      <value>0</value>
    </param>
    <param>
      <key>qt_qss_theme</key>
      <value></value>
    </param>
    <param>
      <key>realtime_scheduling</key>
      <value></value>
    </param>
    <param>
      <key>run_command</key>
      <value>{python} -u {filename}</value>
    </param>
    <param>
      <key>run_options</key>
      <value>run</value>
    </param>
    <param>
      <key>run</key>
      <value>True</value>
    </param>
    <param>
      <key>thread_safe_setters</key>
      <value></value>
    </param>
    <param>
      <key>title</key>
      <value>BPSK Generic Demodulation</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1704, 52)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>audio_samp_rate</value>
    </param>
    <param>
      <key>value</key>
      <value>48000</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(845, 985)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>deviation</value>
    </param>
    <param>
      <key>value</key>
      <value>5000</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1704, 260)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>filter_rate</value>
    </param>
    <param>
      <key>value</key>
      <value>250000</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>SDR device 
TX sampling rate</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1704, 460)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>value</key>
      <value>satnogs.hw_rx_settings[rx_sdr_device]['samp_rate']</value>
    </param>
  </block>
  <block>
    <key>variable_low_pass_filter_taps</key>
    <param>
      <key>beta</key>
      <value>6.76</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>cutoff_freq</key>
      <value>100e3</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(48, 716)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>gain</key>
      <value>12.0</value>
    </param>
    <param>
      <key>id</key>
      <value>taps</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>width</key>
      <value>60000</value>
    </param>
    <param>
      <key>win</key>
      <value>firdes.WIN_HAMMING</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1704, 164)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>xlate_filter_taps</value>
    </param>
    <param>
      <key>value</key>
      <value>firdes.low_pass(1, samp_rate_rx, 125000, 25000, firdes.WIN_HAMMING, 6.76)</value>
    </param>
  </block>
  <block>
    <key>analog_agc2_xx</key>
    <param>
      <key>attack_rate</key>
      <value>0.01</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>decay_rate</key>
      <value>0.001</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1472, 60)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>gain</key>
      <value>0.0</value>
    </param>
    <param>
      <key>id</key>
      <value>analog_agc2_xx_0_0</value>
    </param>
    <param>
      <key>max_gain</key>
      <value>65536</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>reference</key>
      <value>0.015</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
  </block>
  <block>
    <key>analog_sig_source_x</key>
    <param>
      <key>amp</key>
      <value>1</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>freq</key>
      <value>cw_offset</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1360, 568)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>analog_sig_source_x_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>offset</key>
      <value>0</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>audio_samp_rate</value>
    </param>
    <param>
      <key>waveform</key>
      <value>analog.GR_COS_WAVE</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(398, 1065)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>antenna</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>satnogs.not_set_antenna</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(311, 1065)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>bb_gain</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>eng_float</value>
    </param>
    <param>
      <key>value</key>
      <value>satnogs.not_set_rx_bb_gain</value>
    </param>
  </block>
  <block>
    <key>rational_resampler_xxx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>decim</key>
      <value>125</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>fbw</key>
      <value>0</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(992, 268)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>blks2_rational_resampler_xxx_1</value>
    </param>
    <param>
      <key>interp</key>
      <value>24</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>taps</key>
      <value>[]</value>
    </param>
    <param>
      <key>type</key>
      <value>ccc</value>
    </param>
  </block>
  <block>
    <key>blocks_complex_to_real</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1016, 504)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>blocks_complex_to_real_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>vlen</key>
      <value>1</value>
    </param>
  </block>
  <block>
    <key>blocks_multiply_xx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1216, 488)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>blocks_multiply_xx_0</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>num_inputs</key>
      <value>2</value>
    </param>
    <param>
      <key>vlen</key>
      <value>1</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value>The CW offset shifts the carrier from 0 Hz to a
frequency that corresponds to the CW audio
tone. This tone is typically 500-800 Hz.</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1360, 684)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>cw_offset</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>eng_float</value>
    </param>
    <param>
      <key>value</key>
      <value>1500</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(696, 1068)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>decoded_data_file_path</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>/tmp/.satnogs/data/data</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(63, 1065)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>dev_args</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>satnogs.not_set_dev_args</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(64, 984)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>doppler_correction_per_sec</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>intx</value>
    </param>
    <param>
      <key>value</key>
      <value>20</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(472, 1068)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>enable_iq_dump</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>intx</value>
    </param>
    <param>
      <key>value</key>
      <value>0</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(534, 985)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>file_path</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>test.ogg</value>
    </param>
  </block>
  <block>
    <key>freq_xlating_fir_filter_xxx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>center_freq</key>
      <value>lo_offset</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>decim</key>
      <value>int(samp_rate_rx/filter_rate)</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(680, 268)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>freq_xlating_fir_filter_xxx_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>taps</key>
      <value>xlate_filter_taps</value>
    </param>
    <param>
      <key>type</key>
      <value>ccc</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(231, 1065)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>if_gain</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>eng_float</value>
    </param>
    <param>
      <key>value</key>
      <value>satnogs.not_set_rx_if_gain</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(592, 1068)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>iq_file_path</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>/tmp/iq.dat</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value>To avoid the SDR carrier at the DC
we shift the LO a little further</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1704, 324)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>lo_offset</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>eng_float</value>
    </param>
    <param>
      <key>value</key>
      <value>100e3</value>
    </param>
  </block>
  <block>
    <key>low_pass_filter</key>
    <param>
      <key>beta</key>
      <value>6.76</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>cutoff_freq</key>
      <value>2000</value>
    </param>
    <param>
      <key>decim</key>
      <value>1</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>type</key>
      <value>fir_filter_ccf</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1256, 36)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>gain</key>
      <value>1</value>
    </param>
    <param>
      <key>id</key>
      <value>low_pass_filter_0</value>
    </param>
    <param>
      <key>interp</key>
      <value>1</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>audio_samp_rate</value>
    </param>
    <param>
      <key>width</key>
      <value>1000</value>
    </param>
    <param>
      <key>win</key>
      <value>firdes.WIN_HAMMING</value>
    </param>
  </block>
  <block>
    <key>osmosdr_source</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>ant0</key>
      <value>satnogs.handle_rx_antenna(rx_sdr_device, antenna)</value>
    </param>
    <param>
      <key>bb_gain0</key>
      <value>satnogs.handle_rx_bb_gain(rx_sdr_device, bb_gain)</value>
    </param>
    <param>
      <key>bw0</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>dc_offset_mode0</key>
      <value>2</value>
    </param>
    <param>
      <key>corr0</key>
      <value>ppm</value>
    </param>
    <param>
      <key>freq0</key>
      <value>rx_freq - lo_offset</value>
    </param>
    <param>
      <key>gain_mode0</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain0</key>
      <value>satnogs.handle_rx_if_gain(rx_sdr_device, if_gain)</value>
    </param>
    <param>
      <key>iq_balance_mode0</key>
      <value>0</value>
    </param>
    <param>
      <key>gain0</key>
      <value>satnogs.handle_rx_rf_gain(rx_sdr_device, rf_gain)</value>
    </param>
    <param>
      <key>ant10</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain10</key>
      <value>20</value>
    </param>
    <param>
      <key>bw10</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode10</key>
      <value>0</value>
    </param>
    <param>
      <key>corr10</key>
      <value>0</value>
    </param>
    <param>
      <key>freq10</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode10</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain10</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode10</key>
      <value>0</value>
    </param>
    <param>
      <key>gain10</key>
      <value>10</value>
    </param>
    <param>
      <key>ant11</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain11</key>
      <value>20</value>
    </param>
    <param>
      <key>bw11</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode11</key>
      <value>0</value>
    </param>
    <param>
      <key>corr11</key>
      <value>0</value>
    </param>
    <param>
      <key>freq11</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode11</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain11</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode11</key>
      <value>0</value>
    </param>
    <param>
      <key>gain11</key>
      <value>10</value>
    </param>
    <param>
      <key>ant12</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain12</key>
      <value>20</value>
    </param>
    <param>
      <key>bw12</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode12</key>
      <value>0</value>
    </param>
    <param>
      <key>corr12</key>
      <value>0</value>
    </param>
    <param>
      <key>freq12</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode12</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain12</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode12</key>
      <value>0</value>
    </param>
    <param>
      <key>gain12</key>
      <value>10</value>
    </param>
    <param>
      <key>ant13</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain13</key>
      <value>20</value>
    </param>
    <param>
      <key>bw13</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode13</key>
      <value>0</value>
    </param>
    <param>
      <key>corr13</key>
      <value>0</value>
    </param>
    <param>
      <key>freq13</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode13</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain13</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode13</key>
      <value>0</value>
    </param>
    <param>
      <key>gain13</key>
      <value>10</value>
    </param>
    <param>
      <key>ant14</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain14</key>
      <value>20</value>
    </param>
    <param>
      <key>bw14</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode14</key>
      <value>0</value>
    </param>
    <param>
      <key>corr14</key>
      <value>0</value>
    </param>
    <param>
      <key>freq14</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode14</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain14</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode14</key>
      <value>0</value>
    </param>
    <param>
      <key>gain14</key>
      <value>10</value>
    </param>
    <param>
      <key>ant15</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain15</key>
      <value>20</value>
    </param>
    <param>
      <key>bw15</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode15</key>
      <value>0</value>
    </param>
    <param>
      <key>corr15</key>
      <value>0</value>
    </param>
    <param>
      <key>freq15</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode15</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain15</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode15</key>
      <value>0</value>
    </param>
    <param>
      <key>gain15</key>
      <value>10</value>
    </param>
    <param>
      <key>ant16</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain16</key>
      <value>20</value>
    </param>
    <param>
      <key>bw16</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode16</key>
      <value>0</value>
    </param>
    <param>
      <key>corr16</key>
      <value>0</value>
    </param>
    <param>
      <key>freq16</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode16</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain16</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode16</key>
      <value>0</value>
    </param>
    <param>
      <key>gain16</key>
      <value>10</value>
    </param>
    <param>
      <key>ant17</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain17</key>
      <value>20</value>
    </param>
    <param>
      <key>bw17</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode17</key>
      <value>0</value>
    </param>
    <param>
      <key>corr17</key>
      <value>0</value>
    </param>
    <param>
      <key>freq17</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode17</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain17</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode17</key>
      <value>0</value>
    </param>
    <param>
      <key>gain17</key>
      <value>10</value>
    </param>
    <param>
      <key>ant18</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain18</key>
      <value>20</value>
    </param>
    <param>
      <key>bw18</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode18</key>
      <value>0</value>
    </param>
    <param>
      <key>corr18</key>
      <value>0</value>
    </param>
    <param>
      <key>freq18</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode18</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain18</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode18</key>
      <value>0</value>
    </param>
    <param>
      <key>gain18</key>
      <value>10</value>
    </param>
    <param>
      <key>ant19</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain19</key>
      <value>20</value>
    </param>
    <param>
      <key>bw19</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode19</key>
      <value>0</value>
    </param>
    <param>
      <key>corr19</key>
      <value>0</value>
    </param>
    <param>
      <key>freq19</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode19</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain19</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode19</key>
      <value>0</value>
    </param>
    <param>
      <key>gain19</key>
      <value>10</value>
    </param>
    <param>
      <key>ant1</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain1</key>
      <value>20</value>
    </param>
    <param>
      <key>bw1</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode1</key>
      <value>0</value>
    </param>
    <param>
      <key>corr1</key>
      <value>0</value>
    </param>
    <param>
      <key>freq1</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode1</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain1</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode1</key>
      <value>0</value>
    </param>
    <param>
      <key>gain1</key>
      <value>10</value>
    </param>
    <param>
      <key>ant20</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain20</key>
      <value>20</value>
    </param>
    <param>
      <key>bw20</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode20</key>
      <value>0</value>
    </param>
    <param>
      <key>corr20</key>
      <value>0</value>
    </param>
    <param>
      <key>freq20</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode20</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain20</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode20</key>
      <value>0</value>
    </param>
    <param>
      <key>gain20</key>
      <value>10</value>
    </param>
    <param>
      <key>ant21</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain21</key>
      <value>20</value>
    </param>
    <param>
      <key>bw21</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode21</key>
      <value>0</value>
    </param>
    <param>
      <key>corr21</key>
      <value>0</value>
    </param>
    <param>
      <key>freq21</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode21</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain21</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode21</key>
      <value>0</value>
    </param>
    <param>
      <key>gain21</key>
      <value>10</value>
    </param>
    <param>
      <key>ant22</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain22</key>
      <value>20</value>
    </param>
    <param>
      <key>bw22</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode22</key>
      <value>0</value>
    </param>
    <param>
      <key>corr22</key>
      <value>0</value>
    </param>
    <param>
      <key>freq22</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode22</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain22</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode22</key>
      <value>0</value>
    </param>
    <param>
      <key>gain22</key>
      <value>10</value>
    </param>
    <param>
      <key>ant23</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain23</key>
      <value>20</value>
    </param>
    <param>
      <key>bw23</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode23</key>
      <value>0</value>
    </param>
    <param>
      <key>corr23</key>
      <value>0</value>
    </param>
    <param>
      <key>freq23</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode23</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain23</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode23</key>
      <value>0</value>
    </param>
    <param>
      <key>gain23</key>
      <value>10</value>
    </param>
    <param>
      <key>ant24</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain24</key>
      <value>20</value>
    </param>
    <param>
      <key>bw24</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode24</key>
      <value>0</value>
    </param>
    <param>
      <key>corr24</key>
      <value>0</value>
    </param>
    <param>
      <key>freq24</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode24</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain24</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode24</key>
      <value>0</value>
    </param>
    <param>
      <key>gain24</key>
      <value>10</value>
    </param>
    <param>
      <key>ant25</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain25</key>
      <value>20</value>
    </param>
    <param>
      <key>bw25</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode25</key>
      <value>0</value>
    </param>
    <param>
      <key>corr25</key>
      <value>0</value>
    </param>
    <param>
      <key>freq25</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode25</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain25</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode25</key>
      <value>0</value>
    </param>
    <param>
      <key>gain25</key>
      <value>10</value>
    </param>
    <param>
      <key>ant26</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain26</key>
      <value>20</value>
    </param>
    <param>
      <key>bw26</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode26</key>
      <value>0</value>
    </param>
    <param>
      <key>corr26</key>
      <value>0</value>
    </param>
    <param>
      <key>freq26</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode26</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain26</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode26</key>
      <value>0</value>
    </param>
    <param>
      <key>gain26</key>
      <value>10</value>
    </param>
    <param>
      <key>ant27</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain27</key>
      <value>20</value>
    </param>
    <param>
      <key>bw27</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode27</key>
      <value>0</value>
    </param>
    <param>
      <key>corr27</key>
      <value>0</value>
    </param>
    <param>
      <key>freq27</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode27</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain27</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode27</key>
      <value>0</value>
    </param>
    <param>
      <key>gain27</key>
      <value>10</value>
    </param>
    <param>
      <key>ant28</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain28</key>
      <value>20</value>
    </param>
    <param>
      <key>bw28</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode28</key>
      <value>0</value>
    </param>
    <param>
      <key>corr28</key>
      <value>0</value>
    </param>
    <param>
      <key>freq28</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode28</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain28</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode28</key>
      <value>0</value>
    </param>
    <param>
      <key>gain28</key>
      <value>10</value>
    </param>
    <param>
      <key>ant29</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain29</key>
      <value>20</value>
    </param>
    <param>
      <key>bw29</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode29</key>
      <value>0</value>
    </param>
    <param>
      <key>corr29</key>
      <value>0</value>
    </param>
    <param>
      <key>freq29</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode29</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain29</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode29</key>
      <value>0</value>
    </param>
    <param>
      <key>gain29</key>
      <value>10</value>
    </param>
    <param>
      <key>ant2</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain2</key>
      <value>20</value>
    </param>
    <param>
      <key>bw2</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode2</key>
      <value>0</value>
    </param>
    <param>
      <key>corr2</key>
      <value>0</value>
    </param>
    <param>
      <key>freq2</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode2</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain2</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode2</key>
      <value>0</value>
    </param>
    <param>
      <key>gain2</key>
      <value>10</value>
    </param>
    <param>
      <key>ant30</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain30</key>
      <value>20</value>
    </param>
    <param>
      <key>bw30</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode30</key>
      <value>0</value>
    </param>
    <param>
      <key>corr30</key>
      <value>0</value>
    </param>
    <param>
      <key>freq30</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode30</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain30</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode30</key>
      <value>0</value>
    </param>
    <param>
      <key>gain30</key>
      <value>10</value>
    </param>
    <param>
      <key>ant31</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain31</key>
      <value>20</value>
    </param>
    <param>
      <key>bw31</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode31</key>
      <value>0</value>
    </param>
    <param>
      <key>corr31</key>
      <value>0</value>
    </param>
    <param>
      <key>freq31</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode31</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain31</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode31</key>
      <value>0</value>
    </param>
    <param>
      <key>gain31</key>
      <value>10</value>
    </param>
    <param>
      <key>ant3</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain3</key>
      <value>20</value>
    </param>
    <param>
      <key>bw3</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode3</key>
      <value>0</value>
    </param>
    <param>
      <key>corr3</key>
      <value>0</value>
    </param>
    <param>
      <key>freq3</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode3</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain3</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode3</key>
      <value>0</value>
    </param>
    <param>
      <key>gain3</key>
      <value>10</value>
    </param>
    <param>
      <key>ant4</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain4</key>
      <value>20</value>
    </param>
    <param>
      <key>bw4</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode4</key>
      <value>0</value>
    </param>
    <param>
      <key>corr4</key>
      <value>0</value>
    </param>
    <param>
      <key>freq4</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode4</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain4</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode4</key>
      <value>0</value>
    </param>
    <param>
      <key>gain4</key>
      <value>10</value>
    </param>
    <param>
      <key>ant5</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain5</key>
      <value>20</value>
    </param>
    <param>
      <key>bw5</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode5</key>
      <value>0</value>
    </param>
    <param>
      <key>corr5</key>
      <value>0</value>
    </param>
    <param>
      <key>freq5</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode5</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain5</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode5</key>
      <value>0</value>
    </param>
    <param>
      <key>gain5</key>
      <value>10</value>
    </param>
    <param>
      <key>ant6</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain6</key>
      <value>20</value>
    </param>
    <param>
      <key>bw6</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode6</key>
      <value>0</value>
    </param>
    <param>
      <key>corr6</key>
      <value>0</value>
    </param>
    <param>
      <key>freq6</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode6</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain6</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode6</key>
      <value>0</value>
    </param>
    <param>
      <key>gain6</key>
      <value>10</value>
    </param>
    <param>
      <key>ant7</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain7</key>
      <value>20</value>
    </param>
    <param>
      <key>bw7</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode7</key>
      <value>0</value>
    </param>
    <param>
      <key>corr7</key>
      <value>0</value>
    </param>
    <param>
      <key>freq7</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode7</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain7</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode7</key>
      <value>0</value>
    </param>
    <param>
      <key>gain7</key>
      <value>10</value>
    </param>
    <param>
      <key>ant8</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain8</key>
      <value>20</value>
    </param>
    <param>
      <key>bw8</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode8</key>
      <value>0</value>
    </param>
    <param>
      <key>corr8</key>
      <value>0</value>
    </param>
    <param>
      <key>freq8</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode8</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain8</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode8</key>
      <value>0</value>
    </param>
    <param>
      <key>gain8</key>
      <value>10</value>
    </param>
    <param>
      <key>ant9</key>
      <value></value>
    </param>
    <param>
      <key>bb_gain9</key>
      <value>20</value>
    </param>
    <param>
      <key>bw9</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offset_mode9</key>
      <value>0</value>
    </param>
    <param>
      <key>corr9</key>
      <value>0</value>
    </param>
    <param>
      <key>freq9</key>
      <value>100e6</value>
    </param>
    <param>
      <key>gain_mode9</key>
      <value>False</value>
    </param>
    <param>
      <key>if_gain9</key>
      <value>20</value>
    </param>
    <param>
      <key>iq_balance_mode9</key>
      <value>0</value>
    </param>
    <param>
      <key>gain9</key>
      <value>10</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>args</key>
      <value>satnogs.handle_rx_dev_args(rx_sdr_device, dev_args)</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(15, 359)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>osmosdr_source_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>clock_source0</key>
      <value></value>
    </param>
    <param>
      <key>time_source0</key>
      <value></value>
    </param>
    <param>
      <key>clock_source1</key>
      <value></value>
    </param>
    <param>
      <key>time_source1</key>
      <value></value>
    </param>
    <param>
      <key>clock_source2</key>
      <value></value>
    </param>
    <param>
      <key>time_source2</key>
      <value></value>
    </param>
    <param>
      <key>clock_source3</key>
      <value></value>
    </param>
    <param>
      <key>time_source3</key>
      <value></value>
    </param>
    <param>
      <key>clock_source4</key>
      <value></value>
    </param>
    <param>
      <key>time_source4</key>
      <value></value>
    </param>
    <param>
      <key>clock_source5</key>
      <value></value>
    </param>
    <param>
      <key>time_source5</key>
      <value></value>
    </param>
    <param>
      <key>clock_source6</key>
      <value></value>
    </param>
    <param>
      <key>time_source6</key>
      <value></value>
    </param>
    <param>
      <key>clock_source7</key>
      <value></value>
    </param>
    <param>
      <key>time_source7</key>
      <value></value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>nchan</key>
      <value>1</value>
    </param>
    <param>
      <key>num_mboards</key>
      <value>1</value>
    </param>
    <param>
      <key>type</key>
      <value>fc32</value>
    </param>
    <param>
      <key>sample_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>sync</key>
      <value></value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(773, 985)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>ppm</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>intx</value>
    </param>
    <param>
      <key>value</key>
      <value>0</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(159, 1065)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>rf_gain</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>eng_float</value>
    </param>
    <param>
      <key>value</key>
      <value>satnogs.not_set_rx_rf_gain</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(351, 985)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>rigctl_port</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>intx</value>
    </param>
    <param>
      <key>value</key>
      <value>4532</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(446, 985)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>rx_freq</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>eng_float</value>
    </param>
    <param>
      <key>value</key>
      <value>100e6</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(231, 985)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>rx_sdr_device</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>usrpb200</value>
    </param>
  </block>
  <block>
    <key>satnogs_coarse_doppler_correction_cc</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(368, 404)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_coarse_doppler_correction_cc_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>sampling_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>target_freq</key>
      <value>rx_freq</value>
    </param>
  </block>
  <block>
    <key>satnogs_doppler_correction_cc</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>corrections_per_sec</key>
      <value>1000</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>0</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(360, 248)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_doppler_correction_cc_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>sampling_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>target_freq</key>
      <value>rx_freq</value>
    </param>
  </block>
  <block>
    <key>satnogs_iq_sink</key>
    <param>
      <key>append</key>
      <value>False</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>filename</key>
      <value>iq_file_path</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1272, 372)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_iq_sink_0</value>
    </param>
    <param>
      <key>scale</key>
      <value>32767</value>
    </param>
    <param>
      <key>status</key>
      <value>enable_iq_dump</value>
    </param>
  </block>
  <block>
    <key>satnogs_ogg_encoder</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>filename</key>
      <value>file_path</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(680, 472)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_ogg_encoder_0</value>
    </param>
    <param>
      <key>quality</key>
      <value>1.0</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>audio_samp_rate</value>
    </param>
  </block>
  <block>
    <key>satnogs_tcp_rigctl_msg_source</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(16, 204)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_tcp_rigctl_msg_source_0</value>
    </param>
    <param>
      <key>addr</key>
      <value>"127.0.0.1"</value>
    </param>
    <param>
      <key>mtu</key>
      <value>1500</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>mode</key>
      <value>False</value>
    </param>
    <param>
      <key>port</key>
      <value>rigctl_port</value>
    </param>
    <param>
      <key>interval</key>
      <value>1000/doppler_correction_per_sec</value>
    </param>
  </block>
  <block>
    <key>satnogs_waterfall_sink</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>center_freq</key>
      <value>0.0</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>fft_size</key>
      <value>1024</value>
    </param>
    <param>
      <key>filename</key>
      <value>waterfall_file_path</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1408, 248)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_waterfall_sink_0</value>
    </param>
    <param>
      <key>mode</key>
      <value>1</value>
    </param>
    <param>
      <key>pps</key>
      <value>10</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>audio_samp_rate</value>
    </param>
  </block>
  <block>
    <key>parameter</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(638, 985)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>waterfall_file_path</value>
    </param>
    <param>
      <key>label</key>
      <value></value>
    </param>
    <param>
      <key>short_id</key>
      <value></value>
    </param>
    <param>
      <key>type</key>
      <value>string</value>
    </param>
    <param>
      <key>value</key>
      <value>/tmp/waterfall.dat</value>
    </param>
  </block>
  <connection>
    <source_block_id>analog_agc2_xx_0_0</source_block_id>
    <sink_block_id>blocks_multiply_xx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>1</sink_key>
  </connection>
  <connection>
    <source_block_id>analog_sig_source_x_0</source_block_id>
    <sink_block_id>blocks_multiply_xx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>blks2_rational_resampler_xxx_1</source_block_id>
    <sink_block_id>low_pass_filter_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>blks2_rational_resampler_xxx_1</source_block_id>
    <sink_block_id>satnogs_iq_sink_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>blks2_rational_resampler_xxx_1</source_block_id>
    <sink_block_id>satnogs_waterfall_sink_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>blocks_complex_to_real_0</source_block_id>
    <sink_block_id>satnogs_ogg_encoder_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>blocks_multiply_xx_0</source_block_id>
    <sink_block_id>blocks_complex_to_real_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>freq_xlating_fir_filter_xxx_0</source_block_id>
    <sink_block_id>blks2_rational_resampler_xxx_1</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>low_pass_filter_0</source_block_id>
    <sink_block_id>analog_agc2_xx_0_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>osmosdr_source_0</source_block_id>
    <sink_block_id>satnogs_coarse_doppler_correction_cc_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_coarse_doppler_correction_cc_0</source_block_id>
    <sink_block_id>freq_xlating_fir_filter_xxx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_doppler_correction_cc_0</source_block_id>
    <sink_block_id>freq_xlating_fir_filter_xxx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_tcp_rigctl_msg_source_0</source_block_id>
    <sink_block_id>satnogs_coarse_doppler_correction_cc_0</sink_block_id>
    <source_key>freq</source_key>
    <sink_key>freq</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_tcp_rigctl_msg_source_0</source_block_id>
    <sink_block_id>satnogs_doppler_correction_cc_0</sink_block_id>
    <source_key>freq</source_key>
    <sink_key>freq</sink_key>
  </connection>
</flow_graph>
