(footprint "nixie-psu" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61F55CBA)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 1.04 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e48a6dbb-0186-478f-89ca-2b7d9be30d0a)
  )
  (fp_text value "nixie-psu" (at 0 2.54 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp af36a7ae-483b-4079-9462-5af26d2d70e1)
  )
  (fp_text user "+5v" (at 16.51 7.62 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 19b20a97-95e2-4911-afd8-59df7b96360d)
  )
  (fp_text user "0V" (at -17.78 -1.27 90 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 85b19495-2934-4533-adb8-9c3c042cc78f)
  )
  (fp_text user "HV" (at 16.51 5.08 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp a0799125-eff5-45de-880f-94813122f402)
  )
  (fp_text user "+12v" (at -20.32 -1.27 90 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp ee6b3d60-3bbd-4a29-a849-627d3930506c)
  )
  (fp_text user "Gnd" (at 16.51 2.54 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fdcb0ba4-7b26-48ef-889a-469b94893a2a)
  )
  (fp_rect (start -22.86 -8.89) (end 24.13 10.16) (layer "F.SilkS") (width 0.15) (fill none) (tstamp 45150f23-0936-481b-905a-44e2450d8e93))
  (pad "1" thru_hole roundrect (at -20.32 -5.08) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp 74ff62f8-7957-4107-9faa-0c13155c07b8))
  (pad "2" thru_hole oval (at -17.78 -5.08) (size 1.5 2.5) (drill 0.8) (layers *.Cu *.Mask) (tstamp 0a357a05-6f3a-4d9f-b86a-181414f80afa))
  (pad "3" thru_hole oval (at 20.32 7.62) (size 2.5 1.5) (drill 0.8) (layers *.Cu *.Mask) (tstamp f4ab63e1-3925-41dc-a1f7-6999d61e9230))
  (pad "4" thru_hole oval (at 20.32 5.08) (size 2.5 1.5) (drill 0.8) (layers *.Cu *.Mask) (tstamp b59108b3-f696-4533-b652-a46f91427701))
  (pad "5" thru_hole roundrect (at 20.32 2.54) (size 2.5 1.5) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25) (tstamp e74daf6f-0af2-4246-8e18-886bf91aefe4))
)
