(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(Q1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "GND")
  (net 5 "Net-(Q2-Pad2)")
  (net 6 "Net-(L1-Pad2)")
  (net 7 "RF")
  (net 8 "Net-(C5-Pad2)")
  (net 9 "Net-(C9-Pad1)")
  (net 10 "Net-(C13-Pad1)")
  (net 11 "Net-(R7-Pad2)")
  (net 12 "Net-(C10-Pad1)")
  (net 13 "Net-(C14-Pad1)")
  (net 14 "ADC_Q")
  (net 15 "ADC_I")
  (net 16 "Net-(C21-Pad1)")
  (net 17 "A_OUT")
  (net 18 "ADC_MIC")
  (net 19 "Net-(J8-Pad1)")
  (net 20 "CLK0")
  (net 21 "Net-(U1-Pad2)")
  (net 22 "CLK1")
  (net 23 "Net-(U1-Pad4)")
  (net 24 "Net-(U1-Pad5)")
  (net 25 "Net-(U1-Pad11)")
  (net 26 "BIAS_PWM")
  (net 27 "+5V")
  (net 28 "+12V")
  (net 29 "unconnected-(U3-Pad3)")
  (net 30 "unconnected-(U3-Pad4)")
  (net 31 "unconnected-(U3-Pad5)")
  (net 32 "unconnected-(U3-Pad6)")
  (net 33 "unconnected-(U3-Pad7)")
  (net 34 "Net-(C2-Pad2)")
  (net 35 "Net-(C24-Pad2)")
  (net 36 "Net-(R20-Pad1)")
  (net 37 "Net-(C23-Pad1)")
  (net 38 "Net-(R22-Pad1)")
  (net 39 "Net-(C17-Pad2)")
  (net 40 "Net-(R11-Pad2)")
  (net 41 "Net-(C17-Pad1)")
  (net 42 "SDA_PLL")
  (net 43 "SCL_PLL")
  (net 44 "RX_EN")
  (net 45 "unconnected-(U6-Pad7)")
  (net 46 "unconnected-(U6-Pad11)")
  (net 47 "unconnected-(U6-Pad12)")
  (net 48 "SDA_DISP")
  (net 49 "SCL_DISP")
  (net 50 "unconnected-(U6-Pad21)")
  (net 51 "unconnected-(U6-Pad22)")
  (net 52 "unconnected-(U6-Pad30)")
  (net 53 "+3.3V")
  (net 54 "unconnected-(U6-Pad37)")
  (net 55 "Net-(J6-Pad3)")
  (net 56 "Net-(C16-Pad1)")
  (net 57 "Net-(R9-Pad2)")
  (net 58 "Net-(C16-Pad2)")
  (net 59 "Net-(C4-Pad1)")
  (net 60 "Net-(C11-Pad1)")
  (net 61 "Net-(C21-Pad2)")
  (net 62 "CLK2")
  (net 63 "Net-(J6-Pad2)")
  (net 64 "Net-(J6-Pad4)")
  (net 65 "Net-(J6-Pad5)")
  (net 66 "unconnected-(U6-Pad5)")
  (net 67 "unconnected-(U6-Pad6)")
  (net 68 "unconnected-(U6-Pad34)")
  (net 69 "unconnected-(U6-Pad33)")
  (net 70 "unconnected-(U6-Pad8)")
  (net 71 "unconnected-(U6-Pad32)")
  (net 72 "unconnected-(U6-Pad9)")
  (net 73 "unconnected-(U6-Pad10)")
  (net 74 "unconnected-(U6-Pad28)")
  (net 75 "unconnected-(U6-Pad27)")
  (net 76 "unconnected-(U6-Pad24)")
  (net 77 "unconnected-(U6-Pad17)")
  (net 78 "unconnected-(U6-Pad23)")

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 0629cab6-3ecd-4d24-b3c7-424a14a328b7)
    (at 63.5 115.57 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/833d276f-89a9-412e-87b1-93b00a5538d1")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 19aa4ee1-fec3-424c-95df-19f4f5c8d816)
    )
    (fp_text value "10n" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cf88e525-449d-4fb1-948c-10d2d9114601)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp f1d7bc4f-eeb4-4fef-aeed-c807364d9a1c)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 643fff21-af42-4ef7-8733-9c73ec575ed4))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp c6dbc4b1-d837-4260-b6e4-0b91aa5fce92))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 0ffa7e70-bb5e-43f0-9c88-b0fe8a64b644))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1d067892-b626-4028-9ffc-7704b838c858))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 320c1959-4c93-41c4-a33d-36de480e2957))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 9409d7a9-75d8-42dd-bb20-1304ee9e5579))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 22df7f7e-c709-4f7b-8258-b1a61cda41cf))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 575c8014-6ed8-4330-9339-b7ce9a4f4fb7))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 6f985817-ba77-43a5-b77b-fdcee3b64a2c))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp f3554d68-cbe7-40c7-8670-1056a5e205f1))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "RF") (pintype "passive") (tstamp 29e9d713-005b-40ff-a6ce-ee66e9d9e145))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)") (pintype "passive") (tstamp fdd4ba2a-1667-411e-ae49-5360a1746782))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 06ef5dac-6f88-43ab-9b1a-66059e2f36b9)
    (at 187.705 45.115)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/fe85fe77-cb6e-4948-b019-a4b17f90c189")
    (attr exclude_from_pos_files)
    (fp_text reference "TP13" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 473e075a-2333-4d74-8b61-7514b748222a)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d7d04cfe-1d20-4c69-9bee-9900b85a221f)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a40b8b27-cea3-43d7-9fa9-7e28786c9ace)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp ac870ee9-46cb-4295-a264-36ce5d6dd751))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp f73181fe-5f57-401a-b245-d8509c033f51))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "ADC_MIC") (pinfunction "1") (pintype "passive") (tstamp b29b1f5e-ac61-4a11-8e85-799c5bc48c3a))
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 0dca2ee4-5238-4bd4-a6db-59d342ae0fc4)
    (at 172.955 52.285)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/54ccf1a8-1e61-46c2-8235-d4d34dc5e106")
    (attr exclude_from_pos_files)
    (fp_text reference "TP11" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0cc38e8e-091a-4936-8834-5040eb041094)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aada3a87-be0c-4ef3-8493-44b3d8b2a19a)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 135b03eb-67de-4e85-9289-ed3dd3bc3ff6)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 6735bb54-cf92-4852-8990-c1fd90c5f82b))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp a7e62d5e-1e29-4ecd-97b9-765fc674d77b))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(C21-Pad1)") (pinfunction "1") (pintype "passive") (tstamp 969e865c-6ae7-41f4-8289-39381f51b89e))
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 20a9412a-1080-42e1-8c1f-3be340d362d3)
    (at 79.815 92.075)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/761c6b0e-6a7d-4b86-bffb-d3b36ea17fb2")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp eb96ac6d-6083-4d37-a081-816699140787)
    )
    (fp_text value "100" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fe75d0cc-456e-4fac-8e89-3fb1025e5cfe)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 39fc929f-9ce2-4e36-a7ab-36f3c402d5fd)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 0faafc19-a4b2-4b53-941f-f18b4b8d69d4))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 64f89687-999b-44d7-8989-62721c995597))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 09a65a0c-044b-43fd-bd17-9c2aa5a93ced))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2af2dd7c-8fd8-4e07-9761-d3763926d50c))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp c842520c-e1a3-422c-865a-985871e22b18))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp c9336b05-3bf0-4f0a-8137-82359f8d5c68))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 1c3ca8d0-3b16-48f7-a3b5-21145dcff766))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 7ce6b4fd-d94f-4a34-aa74-b739aa7656b1))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 8acb2828-f46b-4a28-98a5-dfdb6164b9ee))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 9e43c38e-af39-4a5b-bd08-28db7a3779da))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C14-Pad1)") (pintype "passive") (tstamp 66b3d282-7bd7-4502-a39f-1cde6cbc994a))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(R9-Pad2)") (pintype "passive") (tstamp b2f7dc97-9bdd-43a5-9ab3-6939ad6b99a2))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 21233baa-b8c7-4692-aa08-973259c6ac82)
    (at 275.22 36.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/79775c20-159a-44c3-adb0-8e946e8616e3")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 36d80f86-ccc9-4fdc-a491-a988e61b47bf)
    )
    (fp_text value "33pF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ed96dade-3814-4e3e-b8c1-44b785ffd451)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 3a6a5a1e-6e0e-4081-b314-3617e0032e46)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 3b325e3b-2b88-45bb-a24d-e8672562a8b9))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 6516f8bc-2c21-4dfa-80da-e31bca7c9999))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 719de35c-80b0-47d5-b70f-b8809dee18ce))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 7ad17669-91dd-4782-b1dc-341215486979))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 84e33ee1-99a7-4b81-a07b-5ca1560e4ceb))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp f51e42dd-ff3d-4a39-832a-2e8fddd57542))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 2a11398d-23a4-46c2-b179-617accd7f550))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 5409bcdf-b434-4b27-9246-167c81181b92))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 6475daf3-9d23-48ac-a6b2-e02c82772fb8))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp fda868d2-5f6d-43b4-9d59-bea973343cf1))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C5-Pad2)") (pintype "passive") (tstamp cc676b96-e999-4fd1-bf2e-ae6866bcac0b))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp d287178a-f65f-4178-9d8e-c3f13674e937))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 277ff9b5-13f3-423a-9101-1d522e7c6dd8)
    (at 86.995 93.0675 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/dd09c7eb-b6e0-4e6f-8244-c9bbec0b94fa")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1e4fb22f-16b9-4a80-88b1-cf2d40e933ed)
    )
    (fp_text value "82k" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9cf9ba19-2920-4073-ad91-1024ce31d755)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 1146080b-f74e-4942-9f1b-dc73211bdd0b)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 7d11be81-87f1-49e3-9238-c2291c332a54))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 7f104ba8-8424-4863-a8ab-4a9852034635))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 6e2a1ca1-20c5-43b4-acd4-260f26d1adc0))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 836bc690-d42f-448d-9478-803f734d5e7f))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 99226c6b-7451-48d2-a312-b4f5397b9e8e))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp d775cfd8-f919-481e-a246-586f3202b7c6))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 5940424d-d637-412e-93ae-b9a63b45fbbc))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 6f5d5c49-04b6-4352-a630-728107ce05bf))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 79584832-e191-4c64-9f06-19a2447b90a9))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp fa96486f-a2f9-4e4c-99d1-22e79c51b939))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(C17-Pad1)") (pintype "passive") (tstamp b11deb7f-c86f-4f0e-8d08-6be78bc3e5c0))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(C17-Pad2)") (pintype "passive") (tstamp fac78ee4-51cf-46d3-9a1e-5188c795e5ed))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 35bd1c74-bf2c-4361-98e8-7b9e1dda3389)
    (at 101.8775 86.36)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/f300a717-9890-4131-8316-c152763d998c")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b14ff658-bda8-4a0f-8698-95c0483b3fbf)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 56a4fec8-c024-4882-91e1-96c3518f63b1)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 7b1fb2b9-06b2-4cca-8791-56f4f9e2070d)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 1a090648-775e-43cb-8745-34607af4fe50))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 7de53142-e558-46ca-a974-17e3059c52a6))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4fd12a5a-ace2-4049-9081-a6190b9d2ba5))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 5d0c0511-2423-4ffc-981c-315ea03169ff))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp b9bb7e48-21ad-417b-93f8-67eca2331649))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp bf6eb881-42ab-4eba-b95b-d0f9fee45b50))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 70e58da1-f263-4937-a017-9a93e1477dde))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 7d9eae5c-727e-48f5-9ffc-04c19fcef8e1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp c2803b36-ba5c-4b5c-a29c-5f3b3e21b5a1))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp d3906278-f4e9-4948-83da-44674067ee7a))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "ADC_Q") (pintype "passive") (tstamp 43947645-903a-436c-af7c-90852645526d))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "+3.3V") (pintype "passive") (tstamp 61c8a4e3-44e3-496f-bbba-e4a07ae550e9))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 36c508b2-11e7-4792-9bd3-ffd745416782)
    (at 257.82 42.97)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/71eb7282-1fff-4f62-93ee-0c261d2d8b88")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ebac3eff-ef03-4312-a1b9-d9074a16402a)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c52e908a-704c-40d5-b7e9-b37538f645d1)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 1b256d1b-6717-4239-a428-42f8ba0aeb8c)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 1f63e667-7bcd-451a-9480-fc3493b19dfd))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp ea5f38c5-e7d1-4dc3-82ed-4be9eb724f95))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 83417671-bd3e-4fd2-aaf3-44caf4b4ba08))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp bff9b048-e962-462b-84c1-087d186eac74))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp df7a20fb-5707-4f15-90ff-1241345d675a))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp e6f9863e-960f-4d36-949a-4334e20c799d))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 22a65f5d-0e0a-4980-ae45-e746384606a0))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 316c6bae-3619-497e-ac4e-29e38b962ae0))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 6bb6f887-e5d3-40d3-940d-898cd5c2ccaa))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp c083e600-8854-4e72-afd2-e9b57abc104d))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "+3.3V") (pintype "passive") (tstamp 35af084b-6775-434a-96d0-c6cb66c47561))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C21-Pad1)") (pintype "passive") (tstamp e972612a-98b2-4991-9cc6-b430d4674503))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp 36cc157a-bce9-4cdb-9109-7b4b61290438)
    (at 92.71 62.23 -90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/5ba7b60f-1246-410b-bf81-0cc77535d0d9")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 89aeb4ca-0cc4-457f-af0d-c769c54a5891)
    )
    (fp_text value "Si5351 Breakout" (at 0 17.57 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f4fdf6d3-753d-4b7f-b52d-4f55b98f03d4)
    )
    (fp_text user "${REFERENCE}" (at 0 7.62) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 24011ac7-70f2-4a66-94e0-1fbe8427c2f9)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 1c11451e-0534-4fa9-9202-4390fc7c1d15))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 2ed023a3-93c2-4646-977e-599fc4133d26))
    (fp_line (start 1.33 1.27) (end 1.33 16.57) (layer "F.SilkS") (width 0.12) (tstamp 791d5700-833f-453f-95f1-a3f1303f22ab))
    (fp_line (start -1.33 16.57) (end 1.33 16.57) (layer "F.SilkS") (width 0.12) (tstamp 88d6fb48-acec-4165-93d9-9c37d2d4078f))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 8b94e541-cf86-4058-81ec-12d8d3c5fe37))
    (fp_line (start -1.33 1.27) (end -1.33 16.57) (layer "F.SilkS") (width 0.12) (tstamp 9fa2a635-941b-4266-b793-7059b67bdf6b))
    (fp_line (start -1.8 17.05) (end 1.8 17.05) (layer "F.CrtYd") (width 0.05) (tstamp 6a0e9ee5-9c0c-4747-93d1-fe75f576aeac))
    (fp_line (start 1.8 17.05) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 978f6034-874f-45cb-9b07-80a96530f267))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp dbb54577-123b-46f9-b124-1bbe9d7eda9b))
    (fp_line (start -1.8 -1.8) (end -1.8 17.05) (layer "F.CrtYd") (width 0.05) (tstamp ebbe7021-fd76-429c-91d1-88618a749f20))
    (fp_line (start -1.27 16.51) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 4468ace7-a2c7-41c0-9f5a-5c3e2a37177a))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 6e6ed998-8be6-4ad5-b9e1-da16484f3382))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 8ba6c8f2-979d-490c-8d36-ddf1b60023f4))
    (fp_line (start 1.27 16.51) (end -1.27 16.51) (layer "F.Fab") (width 0.1) (tstamp b686437a-cf7b-47c5-9ce9-e93915f619a4))
    (fp_line (start 1.27 -1.27) (end 1.27 16.51) (layer "F.Fab") (width 0.1) (tstamp b73f1aa5-2b7c-4c2a-bebc-34becf7859fc))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "+5V") (pinfunction "Pin_1") (pintype "passive") (tstamp bf50265b-052c-47e3-9acb-ce82f4af29b9))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp a76e4d76-e898-4c59-bf19-8dc725ae6840))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "SDA_PLL") (pinfunction "Pin_3") (pintype "passive") (tstamp a96b013b-44ef-4767-b055-c73a1edcd52d))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "SCL_PLL") (pinfunction "Pin_4") (pintype "passive") (tstamp 8f64f1d1-3fc2-4319-9325-ad5fdc074108))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "CLK0") (pinfunction "Pin_5") (pintype "passive") (tstamp a3d7f6e8-6f17-40c6-b407-77c5369aa2e1))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "CLK1") (pinfunction "Pin_6") (pintype "passive") (tstamp c7ff0e3f-bd2b-4ee7-aa9c-f1608048980c))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "CLK2") (pinfunction "Pin_7") (pintype "passive") (tstamp 40363e81-d142-4518-87ea-594f59c100d6))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 3eb0b384-c237-46c6-8721-1d4e4a0847ec)
    (at 68.58 104.14)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/1f4f4b35-e2e4-4a87-9b42-940dea6eb805")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b3886352-7261-4172-babb-09f8fad97c23)
    )
    (fp_text value "1k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dd64aa83-51a4-4e50-800e-0a6b1aef23f8)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp f1d463f3-6c25-4429-bc3b-76cf32dee0b1)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 96feb37e-7638-427b-9ebd-2796cc1f658f))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp e0c6feca-bbc6-4d12-861f-4ff32a872203))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2c4831d0-5696-4787-83e1-6b76da745c97))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 512033c7-ec27-4ba7-ae27-ec3d9d513859))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 776ec86f-80cd-4488-883a-3ef83f6890b1))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp e099641c-f16f-44a1-9576-3727bc81ac51))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 11e0d462-7619-4380-a81a-fa78962cc841))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 9f161a73-a728-4ca8-bbb3-cf128b1471d6))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp c42bf61a-5c60-4e22-9906-2e876962aac0))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp f5e7e06e-dd1e-43cc-a014-9b29e741701f))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)") (pintype "passive") (tstamp 1a2cf7a0-8a93-4654-9549-68611d992572))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 17383c55-702d-4f3e-9542-dc0d0f53b531))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SO-8_5.3x6.2mm_P1.27mm" (layer "F.Cu")
    (tedit 5EA5315B) (tstamp 401001fb-236c-4a11-81e4-4047a990eca1)
    (at 93.0275 93.345)
    (descr "SO, 8 Pin (https://www.ti.com/lit/ml/msop001a/msop001a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/320c4831-d108-487d-b58c-c68d935468be")
    (attr smd)
    (fp_text reference "U5" (at 0 -4.05) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a644e554-85ba-446c-a234-6952ca1b1d5c)
    )
    (fp_text value "TL072" (at 0 4.05) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2aac78db-c0db-4460-9650-b6d3e0e257a3)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 89849b53-cccd-4b3b-8121-3d898e78baa9)
    )
    (fp_line (start -2.76 -3.21) (end -2.76 -2.465) (layer "F.SilkS") (width 0.12) (tstamp 2568a3c6-86df-4141-9a2b-bd079affbef0))
    (fp_line (start -2.76 -2.465) (end -4.45 -2.465) (layer "F.SilkS") (width 0.12) (tstamp 852f172f-77c1-415b-934a-51cff1f769ab))
    (fp_line (start 2.76 -3.21) (end 2.76 -2.465) (layer "F.SilkS") (width 0.12) (tstamp 906f9b2a-d8ac-44cc-8e8f-6c9c8d3286ee))
    (fp_line (start 0 3.21) (end -2.76 3.21) (layer "F.SilkS") (width 0.12) (tstamp a71ed525-ff4b-4c56-a2d9-c163c7577d45))
    (fp_line (start 0 -3.21) (end -2.76 -3.21) (layer "F.SilkS") (width 0.12) (tstamp b4904339-ddfc-4696-b53d-eca9bd5a248a))
    (fp_line (start 0 3.21) (end 2.76 3.21) (layer "F.SilkS") (width 0.12) (tstamp ba570ee4-f981-4fa9-a29e-946e1b5dd23e))
    (fp_line (start -2.76 3.21) (end -2.76 2.465) (layer "F.SilkS") (width 0.12) (tstamp bd9940e4-f299-4a2a-b9ba-58c09acef591))
    (fp_line (start 2.76 3.21) (end 2.76 2.465) (layer "F.SilkS") (width 0.12) (tstamp cd9f6b31-2aa5-4a62-ac0a-03524d98b491))
    (fp_line (start 0 -3.21) (end 2.76 -3.21) (layer "F.SilkS") (width 0.12) (tstamp ff83fa10-a1f0-4728-889a-4f9ed9f3bcda))
    (fp_line (start -4.7 3.35) (end 4.7 3.35) (layer "F.CrtYd") (width 0.05) (tstamp 12774e97-35b7-4fc4-863f-a7404bd3e368))
    (fp_line (start -4.7 -3.35) (end -4.7 3.35) (layer "F.CrtYd") (width 0.05) (tstamp 4c329e82-69b9-4860-af6c-761dae09a992))
    (fp_line (start 4.7 -3.35) (end -4.7 -3.35) (layer "F.CrtYd") (width 0.05) (tstamp 9021278d-61e4-42a9-bf6d-df8a88a5bd80))
    (fp_line (start 4.7 3.35) (end 4.7 -3.35) (layer "F.CrtYd") (width 0.05) (tstamp b07d879f-98b7-4755-b93d-3b9a16d9b73a))
    (fp_line (start -2.65 3.1) (end -2.65 -2.1) (layer "F.Fab") (width 0.1) (tstamp 020a6f7c-7c17-4b99-8cdf-ab611253e5d7))
    (fp_line (start -2.65 -2.1) (end -1.65 -3.1) (layer "F.Fab") (width 0.1) (tstamp 1dbd6adc-3a98-4202-b6d7-e557ecc92426))
    (fp_line (start -1.65 -3.1) (end 2.65 -3.1) (layer "F.Fab") (width 0.1) (tstamp 40ccc18b-9b81-40ea-952c-9b80879a50ec))
    (fp_line (start 2.65 -3.1) (end 2.65 3.1) (layer "F.Fab") (width 0.1) (tstamp 45bca654-a242-4cb4-99c1-34efb4e07762))
    (fp_line (start 2.65 3.1) (end -2.65 3.1) (layer "F.Fab") (width 0.1) (tstamp 6400d3e6-ac65-4125-918e-f759d20c0ce7))
    (pad "1" smd roundrect (at -3.5 -1.905) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(C17-Pad2)") (pintype "output") (tstamp d0ffa6be-9815-4379-8af4-3a2593245bef))
    (pad "2" smd roundrect (at -3.5 -0.635) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(R11-Pad2)") (pinfunction "-") (pintype "input") (tstamp a45cd5d5-09a9-47ae-8d16-0a5db461dd1c))
    (pad "3" smd roundrect (at -3.5 0.635) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(C17-Pad1)") (pinfunction "+") (pintype "input") (tstamp fcb7535f-375c-40e5-b176-c36934bdb107))
    (pad "4" smd roundrect (at -3.5 1.905) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "V-") (pintype "power_in") (tstamp 25c22036-b816-4502-b5ff-ceae9e0d9460))
    (pad "5" smd roundrect (at 3.5 1.905) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(C16-Pad1)") (pinfunction "+") (pintype "input") (tstamp bb8eff83-84e0-41ef-bfa8-dc987f48a927))
    (pad "6" smd roundrect (at 3.5 0.635) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(R9-Pad2)") (pinfunction "-") (pintype "input") (tstamp 3ae118a3-0427-4d3f-a418-41075c36e381))
    (pad "7" smd roundrect (at 3.5 -0.635) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C16-Pad2)") (pintype "output") (tstamp d0341964-5050-4d12-b77a-2420b2a28e71))
    (pad "8" smd roundrect (at 3.5 -1.905) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pinfunction "V+") (pintype "power_in") (tstamp 58c4d62c-d545-430e-9c5c-e18a6224e659))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_5.3x6.2mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (tedit 5A1C1810) (tstamp 422dee9b-db2f-4a0b-b401-ec85e3907ff3)
    (at 53.6225 118.11 180)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/d843298c-7b40-49e3-8b56-6492e06c6d78")
    (attr smd)
    (fp_text reference "J2" (at -3.96 -3 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e40cb945-e25d-465a-b7f8-32aa836161a5)
    )
    (fp_text value "Conn_Coaxial" (at 5 6) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f28f051-d9f2-49ac-b20c-4cba76df02da)
    )
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 220ed610-cd8f-40ca-b044-a702bf190bf2)
    )
    (fp_line (start -3.71 0.25) (end -3.21 0) (layer "F.SilkS") (width 0.12) (tstamp 8ac9d345-f102-4662-88dd-103eff1ce6ce))
    (fp_line (start -3.71 -0.25) (end -3.71 0.25) (layer "F.SilkS") (width 0.12) (tstamp 96313b1e-3aa0-4f41-9704-7cf0104c78f5))
    (fp_line (start -3.21 0) (end -3.71 -0.25) (layer "F.SilkS") (width 0.12) (tstamp d5560b68-5c2c-4aaf-8544-e1e3ee1679b2))
    (fp_line (start -3.04 5.58) (end -3.04 -5.58) (layer "B.CrtYd") (width 0.05) (tstamp 014cdbde-7952-4cd4-9020-cd1c2136ccf7))
    (fp_line (start 14.47 5.58) (end -3.04 5.58) (layer "B.CrtYd") (width 0.05) (tstamp 425142ff-38f1-4464-9ea6-3c1267e4286c))
    (fp_line (start 14.47 -5.58) (end 14.47 5.58) (layer "B.CrtYd") (width 0.05) (tstamp 53265d08-3d01-4b70-b370-35338b88554b))
    (fp_line (start 14.47 -5.58) (end -3.04 -5.58) (layer "B.CrtYd") (width 0.05) (tstamp 9272de79-ac3f-492e-98e9-0a53a667d08f))
    (fp_line (start -3.04 5.58) (end -3.04 -5.58) (layer "F.CrtYd") (width 0.05) (tstamp 4c0450bf-caca-4292-813b-ff93b461b34f))
    (fp_line (start 14.47 5.58) (end -3.04 5.58) (layer "F.CrtYd") (width 0.05) (tstamp 56d9dac6-d992-4eb5-9ea8-d9f1adc9cb61))
    (fp_line (start 14.47 -5.58) (end -3.04 -5.58) (layer "F.CrtYd") (width 0.05) (tstamp 760b31fd-34a8-44cd-bf49-135ee6e8b2a5))
    (fp_line (start 14.47 -5.58) (end 14.47 5.58) (layer "F.CrtYd") (width 0.05) (tstamp 766b4c31-b9d3-41ee-baf8-49ce4157942f))
    (fp_line (start -1.91 3.81) (end -1.91 5.08) (layer "F.Fab") (width 0.1) (tstamp 0ea8dec6-1be6-41a9-91c7-6ea3df379fcc))
    (fp_line (start 3.54 0) (end 2.54 0.75) (layer "F.Fab") (width 0.1) (tstamp 2059631f-053e-469b-9c6c-5ee17396eb79))
    (fp_line (start -1.91 5.08) (end 4.445 5.08) (layer "F.Fab") (width 0.1) (tstamp 269bded2-9a03-4a80-bef7-72d9cb6c3d51))
    (fp_line (start 4.445 -3.81) (end 4.445 -5.08) (layer "F.Fab") (width 0.1) (tstamp 2850c3ce-2d9a-4c4a-a9eb-72f125b17d6a))
    (fp_line (start 2.54 3.81) (end -1.91 3.81) (layer "F.Fab") (width 0.1) (tstamp 45ef5429-d47f-4c25-88c1-ec7110068f96))
    (fp_line (start 13.97 3.81) (end 4.445 3.81) (layer "F.Fab") (width 0.1) (tstamp 557b1e17-8e4a-4c1d-b8ad-ebb48ba78893))
    (fp_line (start -1.91 -5.08) (end -1.91 -3.81) (layer "F.Fab") (width 0.1) (tstamp 69e6a3fb-f47e-4e95-9a57-30d080250016))
    (fp_line (start 4.445 5.08) (end 4.445 3.81) (layer "F.Fab") (width 0.1) (tstamp 986179e1-ec59-45f1-8c3c-4b465d83d42f))
    (fp_line (start 2.54 -0.75) (end 3.54 0) (layer "F.Fab") (width 0.1) (tstamp bd97ea20-889c-4f95-b50c-cc2776860839))
    (fp_line (start 4.445 -3.81) (end 13.97 -3.81) (layer "F.Fab") (width 0.1) (tstamp cef3a31d-ed07-4618-8136-5bd719f968e0))
    (fp_line (start 13.97 -3.81) (end 13.97 3.81) (layer "F.Fab") (width 0.1) (tstamp dc077055-3b62-459d-9d2b-d2969678474a))
    (fp_line (start -1.91 -3.81) (end 2.54 -3.81) (layer "F.Fab") (width 0.1) (tstamp dc2134af-2dc5-4222-920b-bce14ebc647b))
    (fp_line (start -1.91 -5.08) (end 4.445 -5.08) (layer "F.Fab") (width 0.1) (tstamp f1134a11-8a16-44c4-8d82-b5b7f2ba6810))
    (fp_line (start 2.54 -3.81) (end 2.54 3.81) (layer "F.Fab") (width 0.1) (tstamp f1baa158-c05a-4b1f-9269-6e1308625875))
    (pad "1" smd rect (at 0 0 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "RF") (pinfunction "In") (pintype "passive") (tstamp 3bd5ffc8-d254-420d-9443-2ae59391c1ed))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive") (tstamp 06d113f4-ebd2-4a5f-9947-1f5d43e80a2f))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive") (tstamp 1ab3ea2d-5466-48bf-9d5c-02660067f964))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive") (tstamp 746ca96d-709d-4e27-8fca-33934f5caebc))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "GND") (pinfunction "Ext") (pintype "passive") (tstamp 796c78d6-6436-422d-83cc-5b3b16204cdf))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 4256b676-1fd8-4322-9a31-177914a201f9)
    (at 74.295 95.885)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/c587351e-3452-4e4d-abc8-c6ab30116b05")
    (attr exclude_from_pos_files)
    (fp_text reference "TP7" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 50378532-dad9-42e9-af75-0589782b7fee)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4e37ad4c-8c1a-4ad8-a1ac-5171554041af)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 22172758-eb63-4090-b03f-e7bad64f70cd)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 63a8e8d3-bae1-4f8c-99e4-cb5d27027e9e))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 961fbda7-8655-456b-92c2-65f51e9ee014))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(C10-Pad1)") (pinfunction "1") (pintype "passive") (tstamp fcf5fbcd-cc61-43ab-b6df-9264d0c12361))
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 460e8000-67a5-4344-98f1-9d91e63751ed)
    (at 262.17 45.48)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/290f5cee-e4e3-4179-8496-0a76066ba45e")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7aa6fd2d-eff9-4d3e-9486-0cbe5f539d83)
    )
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9df73c53-cc48-4c25-8497-a15bd16c409d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp d58f4b67-e084-4299-9d46-310f39193133)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 4d1400a6-e509-4fa8-961f-399199f756f5))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp c2782193-9fca-42d2-a53f-4703e519770c))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 41598a19-1844-4f7e-a444-9263508dbee0))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 425a8b40-bb9b-4d3e-9679-03b7a452600f))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 8242347c-63f5-4391-87f7-1389d7924687))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp a2744eaf-fe94-4d39-a539-4982de2e935f))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 1e60518b-e08a-4398-8e18-9d3af6067c7f))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 8fb381e9-a6f7-4dc2-b747-905531a1d809))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp ca6f8a39-26aa-4e4c-9af0-8d69d9789415))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp fdfe87df-ab0f-4113-8fd6-7f6d28ecc188))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pintype "passive") (tstamp 6852fbe2-f7f8-412c-a50a-262a6fc161b4))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 644de180-3594-4528-bd01-0481f3efc0e0))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 49877285-ea14-4e94-a7e6-bb160f94448d)
    (at 59.69 118.11)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/b70f7648-1fc4-427e-8330-05076e91e9a5")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 111c4281-6447-46b2-8e98-2c7921b28298)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5a3d37d4-a5c0-4e2c-b962-21a5e127de57)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 25a60434-5a69-44a9-9fc6-98defeaba970)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp b9c2f322-33cc-4b84-a7dd-7af8c19b04f4))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 8c291be1-ad1d-4ee5-9572-911f6beeb4b5))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "RF") (pinfunction "1") (pintype "passive") (tstamp 65982a9b-fc98-48d8-8c45-7a6f941a12de))
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 530a56ef-2056-4fe9-ae0e-0aca7b2d5d01)
    (at 68.58 91.2125 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/a0eb4f95-47b6-4203-9351-21b1ca735303")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 385b7b3f-7fc5-4da1-a350-9e5c9d64431e)
    )
    (fp_text value "470nF" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5ddc4414-8581-484a-af30-e5847e584265)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp b5d7ae87-2fa0-4fa8-aac8-bc2eadf8931d)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 8c6f2a97-6d22-4726-9579-5363ae75fbbe))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp c516f4a8-53e3-41dd-9039-40ce82f3d2db))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 00875486-82fe-4c37-bd7c-60f8157eb6e8))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 19584ed3-05ea-4511-aa73-2660fe519383))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 3aa6d88d-6db7-4abf-ad03-b350b3be5651))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp cb5927a3-e69e-4087-94bf-93d33bcf6d80))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 01410bc7-925d-45d4-8947-bc0e42eb8056))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 2f109e64-70af-4f1b-aaf4-5afe489c224c))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 73c173d7-69ec-4382-9049-cf107216b8cf))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp d2dc0a47-0fb6-4245-8756-f09853e1bdc6))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C14-Pad1)") (pintype "passive") (tstamp 52e0d502-d21b-4c40-b5c1-014be89f48b0))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp cae6cd36-2791-4ca8-a56e-8adb4326689b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (tedit 5A02FF81) (tstamp 531e8a94-19a3-4da5-b234-fa3344348c30)
    (at 91.44 118.11 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/48f7dd9a-c82f-45b8-ac87-2e2d54dcfb3b")
    (attr through_hole)
    (fp_text reference "Q2" (at 2.54 -3.56) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 41f40c19-0ee3-422c-90e6-1c708a822451)
    )
    (fp_text value "BS170" (at 2.54 2.79) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 494b8529-bf2c-4c85-9d87-46472916a6a9)
    )
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8c45b0fd-1fcc-41e9-bf5e-e0fbe250f5e6)
    )
    (fp_line (start 0.74 1.85) (end 4.34 1.85) (layer "F.SilkS") (width 0.12) (tstamp f744e060-ffc5-46d8-a6b2-31b2a5dee488))
    (fp_arc (start 4.864184 1.122795) (mid 4.633903 1.509328) (end 4.34 1.85) (layer "F.SilkS") (width 0.12) (tstamp 210d5e5a-df25-4487-af30-c9d3b8975a0d))
    (fp_arc (start 0.74 1.85) (mid 0.446097 1.509328) (end 0.215816 1.122795) (layer "F.SilkS") (width 0.12) (tstamp 27aa8c47-9174-49f4-916c-4e2950834643))
    (fp_arc (start 2.54 -2.6) (mid 3.936979 -2.192818) (end 4.8964 -1.098807) (layer "F.SilkS") (width 0.12) (tstamp 699bf6e1-dbe0-493e-a5ac-a85eed401ef8))
    (fp_arc (start 0.1836 -1.098807) (mid 1.143021 -2.192817) (end 2.54 -2.6) (layer "F.SilkS") (width 0.12) (tstamp f3a4431e-cb61-4e05-b508-f44f6f5831e9))
    (fp_line (start 6.09 2.01) (end 6.09 -2.73) (layer "F.CrtYd") (width 0.05) (tstamp 10bbbd3c-9b54-47be-a4aa-d811b1783083))
    (fp_line (start -1.01 -2.73) (end -1.01 2.01) (layer "F.CrtYd") (width 0.05) (tstamp 70147ff8-2fe3-4f8a-9184-4c822064e98f))
    (fp_line (start 6.09 2.01) (end -1.01 2.01) (layer "F.CrtYd") (width 0.05) (tstamp 9b255483-db19-48e8-8781-4e0e0638ea6f))
    (fp_line (start -1.01 -2.73) (end 6.09 -2.73) (layer "F.CrtYd") (width 0.05) (tstamp ba4d2f7c-cb7f-42d3-9b13-c5cc2ad08724))
    (fp_line (start 0.8 1.75) (end 4.3 1.75) (layer "F.Fab") (width 0.1) (tstamp 2b1fbb5c-36cc-48a0-a7dd-d3a613e55810))
    (fp_arc (start 0.786375 1.753625) (mid 0.248779 -0.949055) (end 2.54 -2.48) (layer "F.Fab") (width 0.1) (tstamp 8fd43d74-6913-49fe-8ee1-d94615c20598))
    (fp_arc (start 2.54 -2.48) (mid 4.831221 -0.949055) (end 4.293625 1.753625) (layer "F.Fab") (width 0.1) (tstamp 9c979ac5-7aa1-4d35-b36f-7c594ceb26cd))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "D") (pintype "passive") (tstamp b444fc24-d6ab-491c-bb25-b5de8101a56e))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(Q2-Pad2)") (pinfunction "G") (pintype "input") (tstamp 10095cbd-7c48-4b42-b176-821b6244d95b))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(L1-Pad2)") (pinfunction "S") (pintype "passive") (tstamp 35e4d8a7-724b-428d-9e6a-66ef8e7574dc))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 54fa75e8-4eb6-450e-816a-995f15df106e)
    (at 257.82 45.48)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/cb4352a4-d4d3-4f53-9df1-91940ee58c7f")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f3baf79-df7c-4ab3-8d52-74e46d70c5f6)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f059ed45-bef6-4974-8ff4-ab3c790ae316)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 688da539-5d1f-44c3-b7a2-4bcb9d1ef158)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 3017ff17-3d76-4996-8fea-eaab0c2ec923))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp f7a76f54-0e02-473d-9f2f-a1939ef27402))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 07a599c8-7821-4bd6-899b-c64b77c6de59))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 11163ac5-6ccd-4e12-b24c-c76c305e44e8))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1d0d6c6c-b070-420e-b883-4b78bfc6657a))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 3457e963-b017-442f-a98b-78d601b8fccb))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 39ddd324-e08b-4ff8-85b4-26e7254ff3ab))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 4683328e-047c-4ab9-a728-694cc011e0df))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp dbe00d53-d0b3-4e9e-9ca3-dc941ca37354))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp fef23bf7-f824-43c0-8065-0255def8abc2))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(C4-Pad1)") (pintype "passive") (tstamp c11a7cbd-e623-476f-9d56-a345224e7f74))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp ae5afebc-56a6-4151-a0ca-e4bef57b8a8d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 551f15ba-d55d-432e-ad38-45ae80fcc3ba)
    (at 276.86 26.76)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/d653b5f7-c93d-4d7f-826b-06ec0575606f")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 10397562-7a49-42de-a3a9-20d9111d0343)
    )
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2afcac3b-8634-4fc1-8667-38d3beca9b15)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 902c3f8a-39f3-4628-a636-44e20f983382)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 357cc1d9-dca2-44e8-8da1-ac0ebd50a97d))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp c781b03f-2a9c-40c6-ba08-d7cbf3688981))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 0b3336f9-1588-4c48-bd38-f4de08152639))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 71df043f-de6c-4522-8e55-08f44bb0915c))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 756ca6bc-8d90-418a-9c9f-3d2706719295))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp aa9b0268-311d-4560-8943-843a139e0442))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 4f9fa616-78dc-40a8-a48f-a1700e60c518))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 5a14a18c-34cf-4887-bcce-f8c232698b6c))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 5cbfcc66-d28c-4ac6-895f-43650412ae88))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp b6f030bf-5029-4dbc-a018-32e0d94393f7))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "+12V") (pintype "passive") (tstamp cd5de800-e407-45a0-b21e-169167df32f0))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp e23e1600-3a01-44c4-b07a-96e15ebe67d7))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "F.Cu")
    (tedit 5A02FF81) (tstamp 58dd59c9-695e-4a1f-9038-e81651a9b5a0)
    (at 63.5 109.22 90)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/47ea9ae3-60da-4f61-9e7f-aad481ba9199")
    (attr through_hole)
    (fp_text reference "Q1" (at 2.54 -3.56 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cdb53d7b-c2bb-4ef7-8115-cbe5cfec81eb)
    )
    (fp_text value "BS170" (at 2.54 2.79 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0e37d2ab-6124-4fef-885e-9a0f599f839e)
    )
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp adee262e-cddd-4885-8847-b912fd513027)
    )
    (fp_line (start 0.74 1.85) (end 4.34 1.85) (layer "F.SilkS") (width 0.12) (tstamp 49c3e69e-a6fe-451c-afef-075edca5f8f5))
    (fp_arc (start 2.54 -2.6) (mid 3.936979 -2.192818) (end 4.8964 -1.098807) (layer "F.SilkS") (width 0.12) (tstamp 0996d588-1439-424c-a033-0347b6828065))
    (fp_arc (start 0.74 1.85) (mid 0.446097 1.509328) (end 0.215816 1.122795) (layer "F.SilkS") (width 0.12) (tstamp 20bcd22f-b770-4040-9e59-de5ea3ad6a9c))
    (fp_arc (start 4.864184 1.122795) (mid 4.633903 1.509328) (end 4.34 1.85) (layer "F.SilkS") (width 0.12) (tstamp ad2312ca-3fab-42d8-84bf-6f9f16818403))
    (fp_arc (start 0.1836 -1.098807) (mid 1.143021 -2.192817) (end 2.54 -2.6) (layer "F.SilkS") (width 0.12) (tstamp ee21e596-0cf8-4aa1-9ca2-51020c753817))
    (fp_line (start -1.01 -2.73) (end -1.01 2.01) (layer "F.CrtYd") (width 0.05) (tstamp 16effc11-6bd1-44f1-925d-9dd0fa8dc588))
    (fp_line (start 6.09 2.01) (end 6.09 -2.73) (layer "F.CrtYd") (width 0.05) (tstamp 5a867f97-7d9d-4003-aab7-ccf60c05ad81))
    (fp_line (start 6.09 2.01) (end -1.01 2.01) (layer "F.CrtYd") (width 0.05) (tstamp 905ca73c-b2e2-485b-a0b9-a4abd670f2f3))
    (fp_line (start -1.01 -2.73) (end 6.09 -2.73) (layer "F.CrtYd") (width 0.05) (tstamp 9a9843b3-1ce9-4521-bf43-a51eebce0507))
    (fp_line (start 0.8 1.75) (end 4.3 1.75) (layer "F.Fab") (width 0.1) (tstamp a0bd9b6d-b8ee-476b-9b62-237a1228b72d))
    (fp_arc (start 2.54 -2.48) (mid 4.831221 -0.949055) (end 4.293625 1.753625) (layer "F.Fab") (width 0.1) (tstamp 43c1d036-4caf-421c-a9fb-7c775fd46392))
    (fp_arc (start 0.786375 1.753625) (mid 0.248779 -0.949055) (end 2.54 -2.48) (layer "F.Fab") (width 0.1) (tstamp 523048e3-0b7d-4474-ae34-b671f79ae17e))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)") (pinfunction "D") (pintype "passive") (tstamp 5b059f07-327d-44ca-8010-d22cb6ae8156))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(Q1-Pad2)") (pinfunction "G") (pintype "input") (tstamp 84f271e5-d15b-4a73-a619-08d71cc18994))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)") (pinfunction "S") (pintype "passive") (tstamp 81b7b8ce-fb9f-4072-b8eb-88792a4f18c4))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 62ec3fe7-32ea-4649-b0a7-0320ea1af7dc)
    (at 79.815 97.79)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/92850843-265a-4fa0-8012-65263508320a")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 056255e1-f620-46f3-b1f5-feb1c77a9c6c)
    )
    (fp_text value "100" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f0169b5d-077a-441b-87df-440839bfd06d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 31d5aba3-c487-419f-8c1d-0c832b425f03)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 86607f0c-28ea-4174-9905-b67a971de2b1))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp f27a2395-9a41-4dea-b615-d7a739bdfb42))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 014ea8e0-6470-42fd-ab1e-ef7a3e9ecc85))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 32b8d40c-3d00-45e3-b13e-45b41810c7de))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 77901e5c-5fbf-46ac-8f8f-08df8e0e6053))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp d224f319-49b6-4037-8c64-2db16e577608))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 44898c87-e4f8-4c37-8c99-66ac2e51d642))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 835f8fa3-a68a-42fe-9ec8-9fb5ac07eb15))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp c0da17d6-0f0e-49c5-8862-d8a1fca21646))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp de331dea-fd11-446c-b973-ea020cbbaea3))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C13-Pad1)") (pintype "passive") (tstamp ec853611-8186-4f01-ba1b-9523799f62b7))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(C16-Pad1)") (pintype "passive") (tstamp 82b3f100-e4ac-4b20-8fa5-395720f90e47))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 6521df07-7c1e-4146-95e9-9a1993cf896d)
    (at 74.295 92.075)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/b7278322-9a8f-42cd-bde5-534fe674d54d")
    (attr exclude_from_pos_files)
    (fp_text reference "TP8" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp af91baae-7f1e-4acf-b5d6-3c8ff1e12a90)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5e7d4c7b-6b2d-4279-ba88-68cf234301ea)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ad90f7f-8e68-4a32-ade3-b60d1a68a566)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 2b874c16-7aaf-4010-bd3d-4b6d6256f0a7))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 23c79fb4-b676-42cb-abfa-36a1e33d3eec))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(C14-Pad1)") (pinfunction "1") (pintype "passive") (tstamp cae234b2-da47-472b-af3b-2065d2491e44))
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp 677f2749-d521-4ebf-9121-f20ae95c7929)
    (at 140.335 109.855 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/f0c15d61-df3b-4019-903f-824ef526c8ec")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5fc0cbc4-553c-4d8a-8c71-91764348963f)
    )
    (fp_text value "Conn_01x06" (at 0 15.03) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 43037a3a-4825-4572-bf49-20f54657c90b)
    )
    (fp_text user "${REFERENCE}" (at 0 6.35 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 59f95545-ea22-4a0c-9485-4bc1a4965cd8)
    )
    (fp_line (start -1.33 14.03) (end 1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp 08db5aee-4b2d-4a78-9c4a-098e60c8ef43))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 21d2ca1d-f2bc-4832-8ad3-a8601c5fc522))
    (fp_line (start 1.33 1.27) (end 1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp 2a753afb-aa9b-4bac-a442-b7f08d134e58))
    (fp_line (start -1.33 1.27) (end -1.33 14.03) (layer "F.SilkS") (width 0.12) (tstamp 80dda8c9-0575-434f-b54e-327ee128c0c1))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 85b4ac61-c4e9-4c72-bef8-6accb77b88b2))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp f3750fb9-ed33-4ed8-a320-eecffd9072ec))
    (fp_line (start -1.8 -1.8) (end -1.8 14.5) (layer "F.CrtYd") (width 0.05) (tstamp 623a15c0-28d5-4346-9501-4b6b329e8213))
    (fp_line (start 1.8 14.5) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 73c81e45-0f71-4281-8b79-854a794142c4))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 8ec01beb-253a-47b9-9ce1-7fb93b0d9de1))
    (fp_line (start -1.8 14.5) (end 1.8 14.5) (layer "F.CrtYd") (width 0.05) (tstamp d455ef9c-5cae-4da7-9285-dfef272418c3))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 2cd72d7d-3ea3-423c-aad5-e75cfad536c9))
    (fp_line (start 1.27 -1.27) (end 1.27 13.97) (layer "F.Fab") (width 0.1) (tstamp 3c00a87a-a194-4f6f-95f9-38538c656cb5))
    (fp_line (start 1.27 13.97) (end -1.27 13.97) (layer "F.Fab") (width 0.1) (tstamp 77dd4ce2-145a-459b-940a-05f36c6ae562))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 84260d3d-1ccd-461e-a6c8-c8226d0f957e))
    (fp_line (start -1.27 13.97) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp f0a6de05-23f9-45fd-ae0c-66efa47ac408))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3.3V") (pinfunction "Pin_1") (pintype "passive") (tstamp 7439e615-4b9a-4cc7-b86a-17a26b98f541))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J6-Pad2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 1e0a2b04-dc24-4966-a2c5-ae96259451be))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J6-Pad3)") (pinfunction "Pin_3") (pintype "passive") (tstamp 208a4d8b-033c-4298-81c0-e52f2ae3799e))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J6-Pad4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 585ab4c1-beb5-4318-8106-ff73f4dc7a84))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J6-Pad5)") (pinfunction "Pin_5") (pintype "passive") (tstamp 73ad1f7b-0014-437c-abc4-14332bc0f160))
    (pad "6" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_6") (pintype "passive") (tstamp 0e611232-3db8-4d26-88f9-39e00b7c4424))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 6a077694-f530-4f3e-8e7b-77506ac7ccd7)
    (at 181.405 50.325)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/e7fbc2de-0189-45e5-b74f-fb82ed66d6bb")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6097eaff-d3bd-46c0-a13c-a928ad4fe226)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f03fa0d-2d01-41c2-b3a7-54e88c917680)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 662258c4-eaef-49b3-bbf6-f0e49701b867)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 27f27b2d-6e19-457a-9b7a-f85b2da26b1c))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp ac656105-e87c-491b-8747-f6ba843d2755))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad2)") (pinfunction "1") (pintype "passive") (tstamp 7214354a-0189-4b2e-b73d-7eea29d7e764))
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 6c1c4501-bb9f-4fe5-96d5-9916578527a2)
    (at 169.405 55.765)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/833696ee-4c8b-44c8-98c5-4175cea98397")
    (attr exclude_from_pos_files)
    (fp_text reference "TP14" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6700ea60-dff3-4f21-b4c3-f6052b7f200f)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 08b5e5f5-2aea-43c0-a155-8f29091f2cbb)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9f3fe211-bcc6-422f-9fc8-d0cd52369fd0)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 92312c1d-21a5-4e0e-9751-1c34d78cd361))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp c5ff5de9-5e9b-4432-88cd-dc35888f8d95))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(J8-Pad1)") (pinfunction "1") (pintype "passive") (tstamp a379a877-6d4b-44d6-890f-3b4407d8c2a8))
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 6e8093b8-7940-433a-a513-b92bc9601080)
    (at 285.31 24.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/3c71e5a4-0ca4-47e5-82b1-6ccf2164b794")
    (attr smd)
    (fp_text reference "R25" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6e79463b-2393-4c0c-8061-7ffb55039894)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a195e9c-bb63-467c-b9f2-0fcc16027505)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 4689bde9-9c59-41bf-8b89-833205474a93)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 219a876b-28cc-4518-bb0d-b31a811231c9))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp fbf84df4-ab6a-470a-9454-80d4475b66a5))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 9bf5588c-94e5-4c20-b489-d43bb2079e44))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp cb623c70-b424-44a8-998b-d9957c82c1e8))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ece816f3-45d2-48ba-996d-b7c63a1ad07b))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp f5a39bb6-f4c5-4d90-8ab1-db2b89fbb239))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 08ade1bd-fdd4-4d67-a54e-35f4c83f33a4))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 26cab796-c2d4-4d75-afc6-a42d4a8f5b91))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 61f00c5f-ef31-46e5-863f-f26565c4d537))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 7201c473-39da-4f43-ad6e-6b18fbfc9ed4))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "ADC_MIC") (pintype "passive") (tstamp 315cae37-7456-41e8-a414-e540297626fa))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp aa30afd9-0879-4cdb-88f9-b6c12b6c11b1))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 6ea6100a-514d-4fc0-944f-1bbe9f660acb)
    (at 63.5 100.33 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/9f13b748-2b60-4f81-82e4-e15c75e258e5")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 85944811-c1ff-48e4-b7b3-e224d2baa079)
    )
    (fp_text value "10n" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 12f6a38e-06d8-4882-86a4-9d6d92cff5ed)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp d1e7e8e6-2f4c-41ff-8099-116bca3c23e5)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 0676c7d6-6785-46c1-8d45-62d6576b475d))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 6a65efcb-e2a1-41c9-9595-5b9947906971))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2b85a518-a387-4eb4-a0d1-2d3842a288f5))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp ae6777b0-da5d-41d0-bf09-e72067bd76e2))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp ba546c72-40e6-43d8-a7d4-b46c7295c501))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp d9fbe022-dc0a-43b6-8f4a-990611e014cd))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 0c396afa-80d0-4366-a472-19aef76ff721))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 180166e5-ce2b-4eac-978d-bf893d1f3f9d))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 5c1be2ef-ff17-4129-ae48-1afa82064e2a))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp f52d47fd-2ce2-4821-b5fd-f75e4cc5c085))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)") (pintype "passive") (tstamp 62089237-d8ae-4082-a099-f8bc9655054e))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(C2-Pad2)") (pintype "passive") (tstamp 79949e84-2011-4bfa-ac9e-00aeed3f8a0b))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 6f8d286e-6f80-4fcf-9ed8-7aad37033c00)
    (at 99.695 89.9425 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/45b975fe-aa6f-49a2-8a53-24c78009161d")
    (attr smd)
    (fp_text reference "C20" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6488777b-45c0-4cd5-bf9e-5e5325d53ae5)
    )
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 51719653-c318-4e62-841d-c0fd85b11857)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp afe07e24-c49c-433b-9e79-4245cd2079d3)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 608e843d-9f0f-4ea8-b9ae-adba9300dbb4))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp e8c01941-9958-4eb4-a52c-c6836b643f76))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2414c0a6-2520-46e0-800c-9ec5fdd154c8))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 260e479b-bb56-454a-b9ad-32a9823c1936))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 5c7bf924-9fc3-4de6-a4d8-cc251e1adce3))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 88b6349a-1718-466d-a29b-a387813de7a7))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 2656fccc-cd71-4b07-9e96-c3cc47ddc768))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 5c49f945-fe76-4b4e-9a68-7b934d192b33))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp a1cec721-9fa7-4de6-a4e0-deb68aab4f10))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp dc826d12-f741-43dd-8034-8d1ae3be49f0))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C16-Pad2)") (pintype "passive") (tstamp 3482eddd-44e6-4838-a6ab-3cf09a6f4252))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "ADC_Q") (pintype "passive") (tstamp 6950874a-1bb8-4021-8bb3-22ba398416a0))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 707097ab-622d-4fdb-b6b2-2f5b394d7b2f)
    (at 84.8125 86.36)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/1efd5fbc-7190-4326-af49-e4dfb1a28279")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d7873c67-7a5c-4de5-b13a-64a614a050ab)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e290d50d-7f2b-422b-8281-8d43b88e4506)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 499658ba-ed0a-44da-9155-2a6b9203ac5b)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 5ea10003-ba71-4301-ba82-4a0dedc82300))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp f7468c52-1cc2-432a-8ceb-bf2511f7ee18))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 30b5c727-4f2a-4636-9180-e5234bb1c20e))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4990898a-ee52-48d5-bcf8-feadfd5260bd))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 52a374dd-7ba3-4f37-8e78-b74e84e9dc7d))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 78205040-ebff-4b3a-9bbb-412745cb07b6))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 7b6f6609-1bb5-418f-8c88-3965384eb27b))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 9ddef8b1-2230-48fa-82c8-94f3f6e72963))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp da5c69db-404b-4a0c-81b7-80f9c6119b17))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp e15a7570-e5ba-4847-abf9-5c9add376e48))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 2ef5144c-96cc-417d-8574-b56f6f2916aa))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "ADC_I") (pintype "passive") (tstamp 15d14d87-131a-4e9d-98b9-cd4d8b9f67fa))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 732f19f6-d00c-4e2d-9372-6b077da111db)
    (at 270.87 41.14)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/57dac42a-f3ac-4966-87b5-6689856dcd62")
    (attr smd)
    (fp_text reference "R20" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5d25cb78-5469-439d-9abf-8dfbe629c48f)
    )
    (fp_text value "R" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 52fe7e02-6ce4-4009-b997-e3ae47230e84)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp da1c9748-e2e5-4a03-99b7-3bae34027103)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 11952494-e007-4610-a1cf-46544f0a9cfa))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp f84b76dc-16c1-42cd-8e53-7b04c81a786e))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 06db64b9-dcff-43a8-8181-d25b42021966))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2cb86e95-ad5a-4d85-8469-659b5f9a8d56))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 96658833-1c65-4d97-b465-c0be302125e5))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp e78e3293-6339-4b60-844f-6ca992041e1d))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 53c1fef2-4a79-45de-a500-59b576d4c307))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp b63d8fb9-c79f-4ba6-8bb5-aa04da1e1383))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp d9e7ca1a-8556-45ae-bf2f-672b92a80ac8))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp dbe4b9bc-6afe-48dd-92b3-9e952055e576))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(R20-Pad1)") (pintype "passive") (tstamp c3fd582d-4d59-4e8b-b54a-6b9f60b40688))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 6514d276-8fee-487d-a122-96d2eb79e417))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 73da02ed-a842-4288-9b7b-8ea8a7372ae7)
    (at 72.39 118.11)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/b859695c-305e-412f-9997-70574aa5daa4")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dc4bac14-cbfd-43e2-9542-2f69229c2a80)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4205a307-ada4-40f0-a83d-c0abe354edce)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 690db441-2b4f-4194-ab2c-b65e9c5a16aa)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp beeccd52-6ce1-48c3-8265-c068f56354e2))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 6c7922db-b9ca-481e-9774-901f6b98006a))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(C5-Pad2)") (pinfunction "1") (pintype "passive") (tstamp 63fa9047-54f2-4cf1-999b-37db4709357d))
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 74365e57-42a8-49f2-8637-1e093da87ece)
    (at 191.255 45.115)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/027b58d6-ef15-4661-a26f-869219e5c685")
    (attr exclude_from_pos_files)
    (fp_text reference "TP10" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 051b8832-53bf-462d-8948-b574e9c3dd5b)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cb429374-a78f-45aa-bc16-20415550a02e)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec984e62-288c-475d-b264-f1bb83848b55)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 9656163f-db34-4455-9e2c-781ae349e49b))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp f35c9e98-2977-45d2-858d-7315f8478349))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "ADC_I") (pinfunction "1") (pintype "passive") (tstamp 29295fad-29ff-459a-8d99-6a38293d229f))
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 74676e39-a661-4c16-b3b4-6e917f15546c)
    (at 79.815 93.98)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/29da3f52-2263-4697-8e3b-ddd68d736da1")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c4b9df8b-d272-49bf-af15-d421c444b0b1)
    )
    (fp_text value "100" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4fb97daa-c28a-44ba-9972-e8b0397c6e00)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp cffc79a5-0188-4f10-bdcf-66091aa87c6c)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp b6d763d8-2b49-4550-8b22-88abf15f33f5))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp c05591e0-5be3-4aa9-a8a4-ede68594e897))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4c5b1147-ebad-4270-a0cc-1747b0e35073))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp bb15f912-a214-4724-ad81-f82235b2158e))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp cf57edd1-23d6-4329-bcf3-7f5342d6f149))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp e8f5b2bc-63c6-4517-89be-815e3a62eba7))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 27f6f384-93fb-4587-9db3-7b8cf9b23956))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 5a67cf65-b921-4d23-9c2c-818b3cf39e4a))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 5c1532de-df4c-4344-89ec-181cc26cb06b))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp edbdf52f-4749-4d37-89aa-1ddb83323de0))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C9-Pad1)") (pintype "passive") (tstamp 54b379cc-a044-4e85-bd05-935098e227e4))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(C17-Pad1)") (pintype "passive") (tstamp b1791cdd-67e0-41bb-b23c-5959490a1e68))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 78049738-bbe5-4dcf-8b75-ccd0a6b38ad5)
    (at 266.52 36.12)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/f07fbfdc-2c54-4944-9771-bdb86d69bcda")
    (attr smd)
    (fp_text reference "C22" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5b8e6c27-202b-4493-81bd-85e542bdd4d3)
    )
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c0844e89-afa5-4d63-8bfd-5a32844d5007)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp bc37f9b2-6211-4e9a-937d-9abdcb821c1f)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp b5d08304-1510-4c54-a953-ffd369909606))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp cd050ce7-19be-43c9-9df8-73d330e79cc1))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 9944a4d6-5f59-489f-808b-aeef3197c05a))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ce957270-1354-4fb0-b244-fdd02492f380))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ed60296b-3ec2-4504-b342-727e8f2ebc8f))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp f065b322-c3e1-42a8-aa3e-e12b11f4617f))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 29f7fd98-3539-4745-bc17-6c6328258a23))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 993b350f-2dc9-42fd-b2c4-fe710204d313))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp a7709469-0bfc-4e3e-9384-d90f1be49419))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp d9b8a91b-6029-47cf-be59-fdfaefca0fa2))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "A_OUT") (pintype "passive") (tstamp d1be6602-4cc2-47e4-815e-28ae590143f2))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 696f537b-edca-4c3c-9e51-738ffd681888))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 78ea853f-f358-48ed-91fa-d75002cd3e59)
    (at 276.86 29.27)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/14edbb8b-7f66-4705-a035-ee92c4235ee4")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 81529994-5687-4fe8-a799-8146db9b1f6c)
    )
    (fp_text value "R" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 720ca5d3-6508-47b0-9cf8-edcb31121939)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 7748130e-8811-4f29-b7eb-aae2432d95b3)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 4e3a6a02-f65e-4699-8659-abdf301ad192))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp bb9f3e14-4916-464c-a883-f06fcca96f25))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 06186c7a-f83d-4670-a28e-4cd93a782c15))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp b70c292f-286d-433f-a25e-6d1d73840fe2))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp e326965e-d64c-44d4-8af7-0e452c930166))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp e76c2e1c-5db5-47de-a39f-90e35baf69e5))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 1d4c84cc-f24e-4e53-9afa-df8882c98b6f))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 324ec640-4af4-4632-a91e-27d9c30640bd))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 7b11b708-f404-4e97-9afa-dee3a10ed02d))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp b9dcaaf0-2d83-45bb-a860-90a4f4b86dda))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J8-Pad1)") (pintype "passive") (tstamp 46913879-0265-4ab0-8d3a-12488ff1bbc4))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R22-Pad1)") (pintype "passive") (tstamp befd5316-e55c-4548-94b9-09a9eb707b45))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 802ccb87-2625-4761-b7df-4338be6aa370)
    (at 68.58 71.12 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/7f7b20d4-5662-47c8-b579-df063fb58657")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 55d46bfa-ce00-4b34-b45c-7cbd9ee6032a)
    )
    (fp_text value "10n" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3873865d-650f-4bfd-b284-006a8164baeb)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp b34ae0a7-ba07-4409-a232-9055730f05ad)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 836721dc-aa36-4c06-b80c-318f7c0c1c06))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp b029beeb-69e8-4d4b-8e88-c71caed009c4))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4674d3e7-9954-42c9-8473-115e13d7c25b))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 496dde3b-1357-4afd-9181-05dc9e373ac7))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 75fc7515-e86a-4a4e-8be8-f9269b74e74a))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp da6853ab-ba75-4d5a-9f2a-b0523c36dfe7))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 1715295e-7a4a-485e-9c4a-0b1851459314))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 3921a3e5-9e4a-4c29-b8cb-61ce1d114148))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 485d1598-e629-404c-b774-c50bb140c2f7))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp f16954bb-e4c8-47df-a310-bdadb6fa88a8))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(C11-Pad1)") (pintype "passive") (tstamp 301dc38f-9334-495a-ac3a-84ec6d6b7094))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp ef3591fb-0f27-4140-a030-1602c97b4f77))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 821c8605-4785-4732-a359-7a1ace8b0ce6)
    (at 68.58 98.6525 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/631537e3-30d1-4583-b0db-8b3d1047adc7")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5c5675a8-5c4e-4af1-ba86-d951ceb3b5a3)
    )
    (fp_text value "470nF" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp db06f2db-2419-4703-b611-d50001e89f09)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 43629765-86b7-4564-8f53-4f6afd9bf4e3)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 373f1f6a-ca0c-471c-8e05-586f7717abcf))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 5d820e43-840d-42c6-819b-ef5b8052512f))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 0ed6d8e6-1953-4deb-8d94-0ec152362456))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 8aa0b3ae-d87c-4ac9-9099-03e10af63ecc))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp bd79cacc-4c90-42cf-bb9c-016665a719db))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ee642e12-4ab3-4f97-af3c-c9228b808ef3))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 0b2496cb-ddf6-48e1-b55f-c661369e0e99))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 40dd69c3-3f1f-45b4-a5f6-9052a4ceeee8))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp d2241b7a-def3-4127-bf3d-b9d21e83ad9b))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp dc9cea1c-782d-4afd-8d6a-a156ecd1ae49))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C13-Pad1)") (pintype "passive") (tstamp 56a64c9a-3394-4ded-bf99-4f9978d0a404))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 1f6023f2-1bb2-4dd0-aca9-904ad140ac9e))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 8715d684-f216-4adf-9c96-f3669872d409)
    (at 172.955 48.735)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/6972dc38-e9f7-4819-9953-6877597d7e08")
    (attr exclude_from_pos_files)
    (fp_text reference "TP9" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 28db49fa-b923-4b2d-bf69-c0bc085a8838)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 96a35969-0cee-4dfb-987d-527c90c96b73)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5b76cb78-43e0-4f0a-bb77-afa648720855)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 2969916c-2e1a-44f3-9806-fb1003165a50))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 6535cc4d-b0fd-4655-bd87-86769b10b62a))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "ADC_Q") (pinfunction "1") (pintype "passive") (tstamp 51141a00-b6f6-4626-aadb-087c6d649d93))
  )

  (footprint "Package_SO:SO-8_5.3x6.2mm_P1.27mm" (layer "F.Cu")
    (tedit 5EA5315B) (tstamp 88008a53-0e0c-4d45-82e6-c7c531942e6a)
    (at 122.555 118.11 180)
    (descr "SO, 8 Pin (https://www.ti.com/lit/ml/msop001a/msop001a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/6cdd0ef3-b2cf-48ed-ba70-6dc5cabe3f8a")
    (attr smd)
    (fp_text reference "U4" (at 0 -4.05) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 74145d38-f41c-4a27-ae28-7bf68f74fa4a)
    )
    (fp_text value "TL072" (at 0 4.05) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5ad5c300-243e-4e22-ab9a-569200593713)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c190c540-2747-48b2-9c03-598ad536e63b)
    )
    (fp_line (start 0 3.21) (end 2.76 3.21) (layer "F.SilkS") (width 0.12) (tstamp 41a497a4-ea4c-495f-b7d4-ceebcbb79512))
    (fp_line (start 2.76 3.21) (end 2.76 2.465) (layer "F.SilkS") (width 0.12) (tstamp 71bde90f-cec7-4a38-9e1a-ffb758b46ce8))
    (fp_line (start -2.76 3.21) (end -2.76 2.465) (layer "F.SilkS") (width 0.12) (tstamp 74bfd584-91d9-4ec7-a335-82f5d80d59ed))
    (fp_line (start -2.76 -3.21) (end -2.76 -2.465) (layer "F.SilkS") (width 0.12) (tstamp 84d73f2a-4c25-4b38-ab56-45f5f5510e74))
    (fp_line (start 0 -3.21) (end 2.76 -3.21) (layer "F.SilkS") (width 0.12) (tstamp c0652664-be27-4ace-99a9-3ba4fca9d4d3))
    (fp_line (start 0 3.21) (end -2.76 3.21) (layer "F.SilkS") (width 0.12) (tstamp cd6cd805-d311-4603-b010-5c509fa0c3b7))
    (fp_line (start 0 -3.21) (end -2.76 -3.21) (layer "F.SilkS") (width 0.12) (tstamp dec492b7-0532-4f7d-a747-6490a9b41a1e))
    (fp_line (start -2.76 -2.465) (end -4.45 -2.465) (layer "F.SilkS") (width 0.12) (tstamp e5ca21c2-e959-432a-9237-f0e9645fa0d0))
    (fp_line (start 2.76 -3.21) (end 2.76 -2.465) (layer "F.SilkS") (width 0.12) (tstamp ea3ec051-f549-418c-965a-3d04ccd38895))
    (fp_line (start 4.7 3.35) (end 4.7 -3.35) (layer "F.CrtYd") (width 0.05) (tstamp 869e6bc9-6790-4f23-b433-32ce32486fa8))
    (fp_line (start -4.7 3.35) (end 4.7 3.35) (layer "F.CrtYd") (width 0.05) (tstamp 960f0ef4-e780-4717-982d-d6b3d92b9298))
    (fp_line (start 4.7 -3.35) (end -4.7 -3.35) (layer "F.CrtYd") (width 0.05) (tstamp 9d7eb146-8798-4833-969c-aa31eb6541e9))
    (fp_line (start -4.7 -3.35) (end -4.7 3.35) (layer "F.CrtYd") (width 0.05) (tstamp bc5da3db-b740-47db-bcbf-0ccd871b04c1))
    (fp_line (start 2.65 3.1) (end -2.65 3.1) (layer "F.Fab") (width 0.1) (tstamp 0936bfe1-dd36-49ec-ad8f-97f306e1d856))
    (fp_line (start -2.65 -2.1) (end -1.65 -3.1) (layer "F.Fab") (width 0.1) (tstamp 1f6e875e-5fc7-4f14-ba34-d341f42c5fb8))
    (fp_line (start 2.65 -3.1) (end 2.65 3.1) (layer "F.Fab") (width 0.1) (tstamp 226b28ea-fc74-4535-8b0a-3cdeadfb6b92))
    (fp_line (start -2.65 3.1) (end -2.65 -2.1) (layer "F.Fab") (width 0.1) (tstamp 348d1ad7-264c-4d60-8f8b-a89303a4b8d8))
    (fp_line (start -1.65 -3.1) (end 2.65 -3.1) (layer "F.Fab") (width 0.1) (tstamp c9d70c70-eb60-4173-9c6a-b0ca95ffd388))
    (pad "1" smd roundrect (at -3.5 -1.905 180) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(C24-Pad2)") (pintype "output") (tstamp 3248fa04-dd46-4568-a7f5-c432153ba3b7))
    (pad "2" smd roundrect (at -3.5 -0.635 180) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(R20-Pad1)") (pinfunction "-") (pintype "input") (tstamp 21e258f6-5200-4a8a-a5a3-503696eff56c))
    (pad "3" smd roundrect (at -3.5 0.635 180) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C21-Pad1)") (pinfunction "+") (pintype "input") (tstamp 96ca71fe-6b4e-4a15-ad7b-8426ad259a75))
    (pad "4" smd roundrect (at -3.5 1.905 180) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "V-") (pintype "power_in") (tstamp ce98f720-32f8-4b30-a305-1f705632938d))
    (pad "5" smd roundrect (at 3.5 1.905 180) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(C23-Pad1)") (pinfunction "+") (pintype "input") (tstamp 5ac375d5-42ea-4e2e-9ee2-82a810c551d0))
    (pad "6" smd roundrect (at 3.5 0.635 180) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R22-Pad1)") (pinfunction "-") (pintype "input") (tstamp 8318e3ad-d561-40a1-99ba-5df8f335d995))
    (pad "7" smd roundrect (at 3.5 -0.635 180) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J8-Pad1)") (pintype "output") (tstamp 1754da7d-23fd-495c-a48b-7b10003ad01e))
    (pad "8" smd roundrect (at 3.5 -1.905 180) (size 1.9 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pinfunction "V+") (pintype "power_in") (tstamp 2cae82aa-2831-4c54-9547-9ed3acd60780))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_5.3x6.2mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32) (tstamp 894a4f50-6b3b-4d24-beb7-8cafeacb630c)
    (at 60.325 94.615)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/a503b3cd-99c6-4fd0-8010-d2670b698c92")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.45) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f525d49-674a-4be8-a834-a20253268ef1)
    )
    (fp_text value "FST3253" (at 0 3.45) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ce1f2d18-d438-405b-9e3c-e5b823a0207b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6b88f4e9-2883-4ff2-a3d3-357bcfcf0d57)
    )
    (fp_line (start 0 2.735) (end 2.2 2.735) (layer "F.SilkS") (width 0.12) (tstamp 3d900104-5f82-49da-817d-115a61ef4e36))
    (fp_line (start 0 -2.735) (end 2.2 -2.735) (layer "F.SilkS") (width 0.12) (tstamp 55d455bc-5c29-4738-9db4-88e7e707c707))
    (fp_line (start 0 2.735) (end -2.2 2.735) (layer "F.SilkS") (width 0.12) (tstamp 7ec53ca0-3c30-4f28-86db-a73aed0e485c))
    (fp_line (start 0 -2.735) (end -3.6 -2.735) (layer "F.SilkS") (width 0.12) (tstamp bf8e52ae-cb3e-4973-8e8c-98c7bfecf0e9))
    (fp_line (start -3.85 -2.75) (end -3.85 2.75) (layer "F.CrtYd") (width 0.05) (tstamp 4e2e65ce-3d58-47f5-8ab2-d8b7a0f22576))
    (fp_line (start -3.85 2.75) (end 3.85 2.75) (layer "F.CrtYd") (width 0.05) (tstamp 7bf9ea66-f159-420d-970b-e9775745e570))
    (fp_line (start 3.85 2.75) (end 3.85 -2.75) (layer "F.CrtYd") (width 0.05) (tstamp 92f3359e-b1c1-4979-b4f2-92341c428f0e))
    (fp_line (start 3.85 -2.75) (end -3.85 -2.75) (layer "F.CrtYd") (width 0.05) (tstamp a42dbf2e-9c09-4353-98cb-14a96f3f8fc2))
    (fp_line (start -1.2 -2.5) (end 2.2 -2.5) (layer "F.Fab") (width 0.1) (tstamp 03a14bc6-f59c-4d3d-a284-ffde521cd4c9))
    (fp_line (start 2.2 -2.5) (end 2.2 2.5) (layer "F.Fab") (width 0.1) (tstamp 2efef6b7-1cca-4095-94ee-202ed4162d24))
    (fp_line (start -2.2 -1.5) (end -1.2 -2.5) (layer "F.Fab") (width 0.1) (tstamp 6a595e45-2244-4b4b-ab07-f94fd17446a4))
    (fp_line (start 2.2 2.5) (end -2.2 2.5) (layer "F.Fab") (width 0.1) (tstamp 6c0b29ec-5f10-4d85-a386-3d5513423ef6))
    (fp_line (start -2.2 2.5) (end -2.2 -1.5) (layer "F.Fab") (width 0.1) (tstamp c50f1493-b8aa-4a63-904d-9e3f0b04fd8a))
    (pad "1" smd roundrect (at -2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "OE1") (pintype "input") (tstamp 6a69148c-22e4-41b4-869c-27a71324a357))
    (pad "2" smd roundrect (at -2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U1-Pad4)") (pinfunction "S1") (pintype "input") (tstamp 9cd2dc52-00e5-4482-9c89-8ae3860a6435))
    (pad "3" smd roundrect (at -2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "unconnected-(U3-Pad3)") (pinfunction "1B4") (pintype "bidirectional") (tstamp de70bdcb-1296-462b-a277-fda651e257e6))
    (pad "4" smd roundrect (at -2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "unconnected-(U3-Pad4)") (pinfunction "1B3") (pintype "bidirectional") (tstamp c6621b9a-52cd-41de-99b7-728591f63ead))
    (pad "5" smd roundrect (at -2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "unconnected-(U3-Pad5)") (pinfunction "1B2") (pintype "bidirectional") (tstamp b8caa9e8-7315-4fe2-9eff-e5df052c92b6))
    (pad "6" smd roundrect (at -2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "unconnected-(U3-Pad6)") (pinfunction "1B1") (pintype "bidirectional") (tstamp ac1f946d-b65b-4847-beab-a39de84699b6))
    (pad "7" smd roundrect (at -2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "unconnected-(U3-Pad7)") (pinfunction "1A") (pintype "bidirectional") (tstamp b60f8798-dcfa-4e43-9f65-c30fedaea8c4))
    (pad "8" smd roundrect (at -2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 5b2b1ea8-a9e1-4624-9b86-5d0d7ffc21f4))
    (pad "9" smd roundrect (at 2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(C2-Pad2)") (pinfunction "2A") (pintype "bidirectional") (tstamp 4d1fca27-1a49-43a7-a547-343a76087d23))
    (pad "10" smd roundrect (at 2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C13-Pad1)") (pinfunction "2B1") (pintype "bidirectional") (tstamp 35e5936f-4f66-4998-9067-37b81654d6aa))
    (pad "11" smd roundrect (at 2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C10-Pad1)") (pinfunction "2B2") (pintype "bidirectional") (tstamp b63b85d4-1da1-401e-a9ed-2c4c9d2c5483))
    (pad "12" smd roundrect (at 2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C9-Pad1)") (pinfunction "2B3") (pintype "bidirectional") (tstamp 679ca417-5b3c-4f72-8941-cf1295af0c1c))
    (pad "13" smd roundrect (at 2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C14-Pad1)") (pinfunction "2B4") (pintype "bidirectional") (tstamp 8a0939f9-396b-4787-8585-702d7bb8abd0))
    (pad "14" smd roundrect (at 2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U1-Pad2)") (pinfunction "S0") (pintype "input") (tstamp 71afb966-005b-414d-8c3a-138eebc64c96))
    (pad "15" smd roundrect (at 2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "OE2") (pintype "input") (tstamp 6c60be9e-33e8-4ad7-b27a-b9553b644f26))
    (pad "16" smd roundrect (at 2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pinfunction "Vcc") (pintype "power_in") (tstamp 71e80b0a-7f42-4464-82de-7e41a350950c))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp 8968e0ab-f1cc-49f0-aa14-fae752530993)
    (at 252.66 35.06)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/94ce4825-95fd-4633-b329-0306541a42e6")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp efd7ae76-9784-470c-9327-f2331865da15)
    )
    (fp_text value "Conn_01x02" (at 0 4.87) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fde719e8-2791-431e-8e70-0a08f6d5d9d0)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3fc5de42-2119-40d9-bb78-05d36871e5f6)
    )
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 32683bd7-2bd7-415b-b712-5b22192821f1))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 467ac2f6-d231-4767-9416-d0548cefa266))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 827d62e7-9eab-42d5-adb1-3898e8b5d718))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 8712f5f5-a347-4af6-b6af-7133e1a74a2a))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp ee00ab05-3c12-402e-946b-fe010df73b84))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp fbf9e6b2-b8bb-4ee9-a6bc-a9bc23a655be))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 0a9f2d16-88f3-410a-88a1-3b04e430864c))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp 2670c399-7c40-4d1c-a16f-c330ac9bc069))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp bbb06d3b-aab1-4c69-bbfc-1090f9ae55b1))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp c72782d0-2e68-4e2a-98cf-a5cf9e536302))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 21edb6e9-b7d4-426a-b987-763af4baf707))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 2ca64fdb-2f69-4c74-a93e-55f75f7c0396))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 61ae99af-e5be-43c5-aed2-a1ecbb84a4ee))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 885ead3a-3c99-469d-9b13-dc25c69c698e))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp b89ebf1e-6202-43e4-aa0f-b0b372d3b491))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp a400fbc2-1a1d-469e-a79e-baafc93c41c0))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp 8f6db1fb-0f14-404f-82c6-92e1aa0a6b00))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 8c3f5df5-e258-4eb1-a074-eddccbec495d)
    (at 97.5125 86.36)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/225542d5-6269-4bf9-98f0-1c752917767b")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 56663246-e68a-48f8-bccc-7a718bd5e454)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 96737448-dad8-410c-80f2-2582c6f2b76a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 1ed79f0a-c34e-4f3f-acfe-9ee9656df48e)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 249a8116-455d-457e-8df1-c6a5b40bdd10))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 24b25d0a-450f-48c2-b1d8-be99375d784b))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 6ad4a4aa-595f-429e-8ee1-dfbcb7818259))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 8f640a8d-88cd-4271-9882-6bf7f947bd79))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp e504d5a8-53ac-456c-bf4f-8a532288d4ce))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp f997d275-5d4d-4cf3-83fd-2e892c7bfa7b))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 0616184a-b3f7-4e31-85e8-b795f63b5f59))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 0dd217b7-0bd0-4660-956d-2fc8c863870b))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp a3892367-9d3e-4c7e-b304-67d26b5e14db))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp aaf037a6-3990-4c62-8588-49deb59a3e15))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 6c179a83-1f96-4cf5-95aa-02d642e48024))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "ADC_Q") (pintype "passive") (tstamp 732dcd44-9dad-4650-a531-7e489bf55572))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 8c89493e-5485-495c-b0a9-ba235c827132)
    (at 280.96 21.74)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/b3c56fe3-4408-419b-ace2-007df43715cb")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7111e111-2cf9-4ebc-bc7a-d7188171e476)
    )
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cff0fd0d-3113-4e03-b215-1d339111dbbd)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 640964ad-1b95-4c28-8721-3a15e089b809)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 238e2f42-3e05-4be9-ad05-8a6f15ea873e))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp f4fee6cd-7e50-412d-95f4-48ad385c2534))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1565a4cd-3f9d-4d6e-87ca-ce09b2aaf889))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 5ce056ec-55e7-4834-a2bd-7296a5205089))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 7703788b-dfee-405c-890c-033f81cd985a))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp feb2de40-c5f7-4f20-9e6b-842958b83950))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 0f815b82-bce8-430e-ba16-d3e333459677))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 4f295dbf-6507-4517-bf95-b4f7599c6964))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 5da31e88-973f-43bb-b3cc-590508478279))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 9db7eb4d-b2ab-4606-b0ef-61c01b316690))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pintype "passive") (tstamp 843503a4-a637-46db-bea6-d8bee72803a2))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 2b2d5e1c-8ed8-465b-ac7a-18d2d0a75317))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 8cda0868-01b2-45c1-b72d-ff1e6456d349)
    (at 262.17 40.46)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/d228e31f-fcc2-4af2-8e99-be28df2928c9")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 91188ec0-6b72-490c-85e7-14f0518138a1)
    )
    (fp_text value "R" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8785bf8c-d288-41f2-8c00-2109bf530b17)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 0e9b1124-f899-4cd4-8244-2fcb40721c14)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp e71155ac-a028-4e25-a25d-316cb5ee471e))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp ed4f21f3-0709-4b20-ab0b-cafd9d345391))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 026330ae-be51-42c2-adcc-7b07257fd787))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2ce1d18c-6baa-40ae-a98a-b08cd2b99b14))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 470d755c-5bff-4301-907b-c1521f54b6cb))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp ae5b0120-efce-4d76-b7b8-7a4f28c529da))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 3e11fd3b-db4c-4556-87ca-6af8c71633bc))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp c1ba6ef0-e5f8-4d60-b03f-df5177da60fe))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp ddccafd8-303c-41bb-8114-57e76b3d3790))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp e0a19e4b-c2c9-4f4c-b239-77ec5ff99bc8))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(C24-Pad2)") (pintype "passive") (tstamp 28b3d2e5-987f-4a0b-9beb-46e7d193858c))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(R20-Pad1)") (pintype "passive") (tstamp 84df48fc-fedd-4864-88df-ec6522a2138a))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_Elec_5x5.8" (layer "F.Cu")
    (tedit 5BC8D926) (tstamp 90d29924-27cf-4bdc-aa2c-cfb0163709be)
    (at 133.985 117.475)
    (descr "SMD capacitor, aluminum electrolytic nonpolar, 5.0x5.8mm")
    (tags "capacitor electrolyic nonpolar")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/f8daa350-01af-4818-9687-b1a76402565c")
    (attr smd)
    (fp_text reference "C21" (at 0 -3.7) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2619c9c5-22ca-4d81-af7d-769fff5a0b77)
    )
    (fp_text value "10uF" (at 0 3.7) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c91e1110-28de-4883-a2c9-5a751f924992)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1884cd18-e500-4f4a-87ce-4b1718ef8a04)
    )
    (fp_line (start 2.76 -2.76) (end 2.76 -1.06) (layer "F.SilkS") (width 0.12) (tstamp 1d5affe2-c0dc-4acb-88c4-a757ccd6b63d))
    (fp_line (start -2.76 -1.695563) (end -1.695563 -2.76) (layer "F.SilkS") (width 0.12) (tstamp 279e9bd0-2ff5-4e43-8e8a-d395d952ed2a))
    (fp_line (start -2.76 -1.695563) (end -2.76 -1.06) (layer "F.SilkS") (width 0.12) (tstamp 45a423ff-4ec8-4647-84d0-77a375c98bb0))
    (fp_line (start -1.695563 2.76) (end 2.76 2.76) (layer "F.SilkS") (width 0.12) (tstamp 600fbc69-a8b4-4606-9031-4f2b3464d72a))
    (fp_line (start 2.76 2.76) (end 2.76 1.06) (layer "F.SilkS") (width 0.12) (tstamp 77e74dcf-91c8-4e8a-82b6-b66528a755e0))
    (fp_line (start -2.76 1.695563) (end -2.76 1.06) (layer "F.SilkS") (width 0.12) (tstamp a04db535-82fe-449f-a799-a41d494edf3e))
    (fp_line (start -1.695563 -2.76) (end 2.76 -2.76) (layer "F.SilkS") (width 0.12) (tstamp d8335d4f-7b80-4484-ab28-17ccba17c39c))
    (fp_line (start -2.76 1.695563) (end -1.695563 2.76) (layer "F.SilkS") (width 0.12) (tstamp f859d87b-6312-41b9-9c4a-d309657b5c50))
    (fp_line (start 3.7 1.05) (end 2.9 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 03b6e381-3b43-453b-938f-8f4ad4345f9d))
    (fp_line (start -2.9 -1.05) (end -3.7 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 0a65d34b-2fce-43b3-a612-6877307da6a0))
    (fp_line (start -1.75 2.9) (end 2.9 2.9) (layer "F.CrtYd") (width 0.05) (tstamp 2590b7c4-7c4b-47a0-aa4c-a2f1b1003047))
    (fp_line (start 2.9 1.05) (end 2.9 2.9) (layer "F.CrtYd") (width 0.05) (tstamp 3684900d-54fe-4f66-9800-13d4cc9079f2))
    (fp_line (start -3.7 -1.05) (end -3.7 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 40297eef-ca8c-420d-90a1-40cdd9b44694))
    (fp_line (start -3.7 1.05) (end -2.9 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 4805c586-2154-4b06-99c4-158a9add01e1))
    (fp_line (start -2.9 1.05) (end -2.9 1.75) (layer "F.CrtYd") (width 0.05) (tstamp 7e14d6d4-0dd0-430b-b163-f643c1a68546))
    (fp_line (start -2.9 -1.75) (end -2.9 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 88a717cb-0608-4eee-ac68-b457d5188f18))
    (fp_line (start 2.9 -2.9) (end 2.9 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 88d23264-58e1-462a-be51-17834e0566a1))
    (fp_line (start -1.75 -2.9) (end 2.9 -2.9) (layer "F.CrtYd") (width 0.05) (tstamp 8900e141-a3c7-4ea1-bca0-a7afa8ca0304))
    (fp_line (start -2.9 -1.75) (end -1.75 -2.9) (layer "F.CrtYd") (width 0.05) (tstamp 90e73330-c94b-420d-8751-c9ef66c47de4))
    (fp_line (start 2.9 -1.05) (end 3.7 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp b86a467e-7f3c-4b61-ba8c-d5ccb1f44ca1))
    (fp_line (start -2.9 1.75) (end -1.75 2.9) (layer "F.CrtYd") (width 0.05) (tstamp d8b87c72-6d9e-491b-a281-4538cdd35a7d))
    (fp_line (start 3.7 -1.05) (end 3.7 1.05) (layer "F.CrtYd") (width 0.05) (tstamp eca457a3-b1c9-447d-9a4b-c0590deee59b))
    (fp_line (start -2.65 -1.65) (end -1.65 -2.65) (layer "F.Fab") (width 0.1) (tstamp 12d6ac60-763c-48cd-bd79-32f36119bd63))
    (fp_line (start -2.65 -1.65) (end -2.65 1.65) (layer "F.Fab") (width 0.1) (tstamp 155ffa8a-23e6-4ce0-b326-009d3cf21095))
    (fp_line (start -1.65 -2.65) (end 2.65 -2.65) (layer "F.Fab") (width 0.1) (tstamp 2b93f6a5-e9a3-4a6a-9abe-38b2f33548b8))
    (fp_line (start -1.65 2.65) (end 2.65 2.65) (layer "F.Fab") (width 0.1) (tstamp 68355bac-1d64-48f9-a5d4-767ea5bf37f6))
    (fp_line (start 2.65 -2.65) (end 2.65 2.65) (layer "F.Fab") (width 0.1) (tstamp 77ae6004-c341-4650-8358-b6ff44235afd))
    (fp_line (start -2.65 1.65) (end -1.65 2.65) (layer "F.Fab") (width 0.1) (tstamp 7c1583bd-fb72-47f9-9f50-2d41fbd57e45))
    (fp_circle (center 0 0) (end 2.5 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp e0dbeec9-6fde-4566-82b6-dd08b849862f))
    (pad "1" smd roundrect (at -2.0625 0) (size 2.775 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 16 "Net-(C21-Pad1)") (pintype "passive") (tstamp f43655df-ddd0-4600-a6ad-a290db946786))
    (pad "2" smd roundrect (at 2.0625 0) (size 2.775 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 61 "Net-(C21-Pad2)") (pintype "passive") (tstamp d2c25c10-9395-4c43-a52f-70f81949fb28))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_5x5.8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 93220888-551a-447d-be7b-3391b00f34bf)
    (at 89.1775 86.36)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/bc2784ba-2ca3-46d6-bd88-6cd6586f4b68")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d896908a-eeee-4737-854d-f0e7323481df)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dca5c326-4af5-49ad-93d0-aaa4f31a20c7)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 7bc3586d-5f5c-41b6-9a49-8a26c5a60921)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp b03d683d-c906-46b0-b07d-b5bdd122a8ee))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp f2eec877-06d6-4332-9365-7f474cd3f373))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 18561a51-093d-42f7-a10d-105ed44ecbff))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 753b6da3-2dd6-4ae8-9358-6f0d8aec4a7f))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp b9903362-d007-4dcd-9a45-115354a84687))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp e605b749-ee87-4cca-baea-02162befbd91))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 3adb0e64-b375-4248-a0e6-98c17a5f416d))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 45e7e0f8-a678-4820-aa7c-e03a81229352))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 737b57b4-0d6d-4b4f-924b-f9bd2d78e647))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 876f992b-1736-40f9-bf90-f7b50e96770a))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "ADC_I") (pintype "passive") (tstamp ae12ee9e-795e-44de-a499-10b4916d4924))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "+3.3V") (pintype "passive") (tstamp e25a3244-50c4-499e-aa04-5b5d5386ecaa))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (tedit 5A02FF57) (tstamp 9560cf52-9007-480c-bfed-8ded709b90f0)
    (at 181.005 40.875)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/d1b8d41b-5450-4bfb-9842-7caa66998b0e")
    (attr smd)
    (fp_text reference "U2" (at 0 -4.5) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f6a3527-7de3-427b-9003-c6f1b3c9ce5b)
    )
    (fp_text value "LM1117-5.0" (at 0 4.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bd8dcd78-fec4-47fc-ba7b-d8bd93c09a61)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.12)))
      (tstamp 964fddd5-fa89-45aa-947f-2fef62e31589)
    )
    (fp_line (start 1.91 3.41) (end 1.91 2.15) (layer "F.SilkS") (width 0.12) (tstamp 02a75c3e-3c34-43fd-9b51-9870b58bea7c))
    (fp_line (start 1.91 -3.41) (end 1.91 -2.15) (layer "F.SilkS") (width 0.12) (tstamp 07cdb9d5-5521-4e7b-b681-852541dba473))
    (fp_line (start -4.1 -3.41) (end 1.91 -3.41) (layer "F.SilkS") (width 0.12) (tstamp c3f6a81b-261c-4de6-8cfc-31edb4cc627c))
    (fp_line (start -1.85 3.41) (end 1.91 3.41) (layer "F.SilkS") (width 0.12) (tstamp d2a8b3f9-2710-47cb-9aba-30883a7c808e))
    (fp_line (start -4.4 3.6) (end 4.4 3.6) (layer "F.CrtYd") (width 0.05) (tstamp 3047dc51-7eb4-4c4c-bf14-f7830621fb2d))
    (fp_line (start -4.4 -3.6) (end -4.4 3.6) (layer "F.CrtYd") (width 0.05) (tstamp 746cfd9c-6b80-46a2-a8db-e35cda9cf502))
    (fp_line (start 4.4 -3.6) (end -4.4 -3.6) (layer "F.CrtYd") (width 0.05) (tstamp 7af28f9c-2834-490e-bdab-d2a9292f1af3))
    (fp_line (start 4.4 3.6) (end 4.4 -3.6) (layer "F.CrtYd") (width 0.05) (tstamp d2bbc0f3-2173-49f1-aa43-89ca25abab4e))
    (fp_line (start 1.85 -3.35) (end 1.85 3.35) (layer "F.Fab") (width 0.1) (tstamp 01cf65ab-b988-4e65-860d-c9e67fdfd184))
    (fp_line (start -1.85 3.35) (end 1.85 3.35) (layer "F.Fab") (width 0.1) (tstamp 615f9809-bf86-406e-a252-e74efb23bda4))
    (fp_line (start -1.85 -2.35) (end -0.85 -3.35) (layer "F.Fab") (width 0.1) (tstamp 8685eb08-570b-4f02-acdf-43c0e901325f))
    (fp_line (start -0.85 -3.35) (end 1.85 -3.35) (layer "F.Fab") (width 0.1) (tstamp 976f26a7-7a10-41d6-898f-3b28a7a8b4a0))
    (fp_line (start -1.85 -2.35) (end -1.85 3.35) (layer "F.Fab") (width 0.1) (tstamp eba63a2c-8832-41d9-a8c8-3c53f9ffad65))
    (pad "1" smd rect (at -3.15 -2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 86705ddb-bf53-4196-a80c-d4c86d04ee2e))
    (pad "2" smd rect (at 3.15 0) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "+5V") (pinfunction "VO") (pintype "power_out") (tstamp 1d2c2148-744d-4dfb-954b-b49fc3212d8d))
    (pad "2" smd rect (at -3.15 0) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "+5V") (pinfunction "VO") (pintype "power_out") (tstamp e909e30d-78be-4d1a-b40c-0ca9035b791d))
    (pad "3" smd rect (at -3.15 2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "+12V") (pinfunction "VI") (pintype "power_in") (tstamp 971e3361-7a3c-4f83-b91c-523fda7ba63e))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 97bc7790-e9f2-4856-9193-89781eb5e34c)
    (at 276.61 24.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/a83b7602-8e87-401f-b4d8-36ac7fef5180")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 84358d3e-823e-45fc-9b70-8e45df3294ba)
    )
    (fp_text value "1k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 01c53d5b-0354-47c5-9f6e-736fb989919e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 7934d710-b5ac-4280-8e44-f5b9a65ff32a)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 48011078-5698-4cef-829b-a8247d8f26a6))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp c22e7c6e-32ff-4def-a9ba-3a0b8a28681b))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 19242e93-373c-4100-90d9-9c3a38064cc7))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2e294b02-0e02-4e29-8ee7-03929ae8d621))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp b2f3b435-1291-46ee-b7af-b83f6bbf6c10))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ec1f2712-1ffe-4820-a6e3-6e1b807ebb35))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 031f16e3-6fe5-4452-8c0b-6b21f719c838))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 72addbd5-66f4-4b98-9b3a-f0e01a7eedd1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 7bb21e55-dfb8-4b1b-8f6e-d609c7da2550))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp b13ced13-f4af-47ad-8706-4a757c12bb3f))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(C4-Pad1)") (pintype "passive") (tstamp 3de2e410-c1b7-4d64-9efd-75ce2694d554))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(C2-Pad2)") (pintype "passive") (tstamp 7d75486d-9e73-45d3-a091-a867c1d30ed5))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp 9be498ff-6246-440e-b3af-426636ff4847)
    (at 192.055 52.215)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/ab7815a5-9823-4972-8e94-c9593ee3ecf2")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 83f2a8f5-610b-46ea-b9ea-328f5265d66b)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp adf462ba-db02-4e19-b00c-1f246072c795)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5777d36a-e50a-4550-ba86-0491e7d0abdb)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 4ad145cd-e8d4-47da-98a3-a116c8bc372a))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp bb434b38-9a98-4dc3-b9e2-5c114184b690))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(Q2-Pad2)") (pinfunction "1") (pintype "passive") (tstamp 027d2174-6e63-466c-ba7c-963eb1a86a34))
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 9e17fd82-736a-441f-9e43-85e0a19bb8ce)
    (at 276.86 31.78)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/3709931b-d43a-40ae-ac68-40dbdd450997")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ac3f526d-d40c-424b-9269-04cfea5da33e)
    )
    (fp_text value "R" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 34d73b19-bfdc-4cc9-bb3b-c0b32a3d0288)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 3779975f-e514-4caa-a94b-c10d2d263cff)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 27bc9bcb-fcf7-41fe-8e8f-4ea207b92d8f))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp f624171f-d146-4395-a90a-971699b1090e))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 636569d8-2172-40f4-9695-ec304c641a33))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp a8139a14-1d8b-4c42-bd82-5079b674d8d1))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp dd0a6376-f871-4eda-8eb9-e87d8c05319b))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp fee80253-7145-4d8a-9b8b-665e19108a7b))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 23760749-e917-43f3-b98e-a967a3d14bfb))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp a650ba41-ab9a-4118-b800-0d80000b7a95))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp e855429a-4b2b-4ee2-a2e0-1b9e85fda0b9))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp e88155f8-15e5-44c4-a3ba-7ffca55418ff))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R22-Pad1)") (pintype "passive") (tstamp d1070d4e-2831-4943-9bcd-163b57a0ac03))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 2cffd7eb-18dc-4518-b209-d1c7cc6163b6))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp 9fd6f0a4-803a-4fbb-9ffb-d405a1b71e68)
    (at 285.31 21.74)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/4352184d-3c35-4a4f-8bc7-9aa8a5d14a9b")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a4cb203c-5fcc-4719-ac75-f7b2eda001f4)
    )
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0a0a3d2-bfdf-4b74-a3e1-89af063b287b)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 8f087cc8-89c0-4c78-891d-b6b83a87ebe2)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 4155c687-4731-4a3c-87b9-31c451765863))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 89640891-0e02-4f80-a8f1-655415f83fdd))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 056e50a0-a081-4a7d-b3fe-e1afb06f79ec))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 06068ae8-8aff-4fae-b954-7b684d290b58))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp e1d89da9-9e81-4002-953f-1c99b50166db))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp e3927b59-3d5d-4809-aa74-7e1c9663aa8f))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 02e3e9a6-1ade-4dbe-9c10-0708dfee9d8b))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 10765a3a-b65e-4258-a693-305549d4040b))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 4a90172f-1669-49ce-841e-5c4549b6da0f))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp de0e996c-594d-423a-b867-668b45b817f8))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(C4-Pad1)") (pintype "passive") (tstamp 0a050b19-1f90-4579-8a8a-ac7474d628bc))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp a2439564-622e-47cb-a90e-6bf9b2d4bbf1))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp a096ded7-9981-4ced-ac10-19b0b9515c1b)
    (at 268.16 31.1)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/c1df0342-7fb9-4dd8-a5a2-5fd700d58f43")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 14cf8d7f-5881-4ddc-abf0-4e5abde4b130)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp edfac2b7-b04e-4a86-bd39-e8feb3aee2f2)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 88db622e-5f73-4b22-b31f-6821511f765e)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp bc0cc1ce-145c-4618-9850-4403fa781220))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp bc0e4250-0393-40e4-9124-40c1ec5d189f))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 065efd75-8029-4963-b1d3-0632c4d8bb7f))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 33257184-2bfe-420c-a4c1-a5a0e27e2667))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 3eec7584-7c0a-41fc-9fba-535d0b5908e2))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 57d43c84-4cd8-46d9-9182-1d5a83c76009))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 59cff25e-8f29-4d55-afc3-eb68fd7e68b5))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 8bc288c1-a97f-4f48-999c-78ad26aebf33))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp f0400165-c5d6-4fed-b818-3f3fd3371298))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp fa4a0d80-6837-4f2f-bba1-73471afcf55f))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(C11-Pad1)") (pintype "passive") (tstamp 2f4ffd88-b8f4-424b-94a0-efccded0302e))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(R7-Pad2)") (pintype "passive") (tstamp 826d1720-5951-482a-bf31-f926831a7b91))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp a8074302-b68a-49c0-980e-54c33e35fd18)
    (at 272.51 31.1)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/cab1b378-7c23-47dc-9e53-f05413dcb39b")
    (attr smd)
    (fp_text reference "R24" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f8f722e9-bbbc-4193-b431-4bb9a2f49643)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0b898197-30d4-4b89-b5ad-872df28e42c7)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp a7289345-e5d0-476e-b7bf-f6cb2e0f4b82)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 4c7db5ae-bb68-433f-bad8-6c0011d994c6))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp eb343dd6-072e-4398-91d2-3023f2d64421))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 10f7b619-154a-49c1-9432-479716b80c4d))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 21047409-6e26-46ce-909f-8ccaa1931248))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2c0a12d1-50e3-4053-85f2-4d3f3cbb791f))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp dd0d2a0d-1cd6-4010-89e7-f2caa4f9a364))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 3b779f69-002f-4f1d-a8af-cdb57d401b83))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 64fb7300-8e79-4e04-a834-cd45b8c48ecd))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp a61d9670-3cb7-469c-ae5a-59abf8f3a17c))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp d5b8eabd-d92b-48d8-9afc-2920dc94b5e9))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "+3.3V") (pintype "passive") (tstamp 3b6ec5e9-d617-43c4-bce4-a1740ca94416))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "ADC_MIC") (pintype "passive") (tstamp 27a46da4-20ec-4660-a3ae-f8ed3935f002))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp aae18fdb-c2a0-49d6-b534-5231c0861070)
    (at 248.01 35.06)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/6ff947c0-ac3f-43c6-accb-a30a25c98fda")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp de405a2d-5611-4ab0-b9c9-6f7153ae3a47)
    )
    (fp_text value "Conn_01x02" (at 0 4.87) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b9935f94-12c6-45f6-89e3-8acf7a1f66d8)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9883ee71-df69-43bd-ab6c-2fce61c76a6d)
    )
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 331a51cb-c8f9-4e39-b698-9407e604855b))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 4e3bf19a-f3be-47de-960f-d4abd1b2e20e))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp b13f70d5-5c24-4420-ae44-12aa609297ca))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp ccf58dff-7050-4808-b4e6-6b20e85d55d0))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp d1dbed8f-3fb6-4850-8781-c51157e283d2))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp ef7ade8d-655c-4772-a890-8f941fcd3415))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp 2bfbe4a5-6e7e-4f8e-a314-2bedd9087c79))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 2eb55fef-b08d-42fb-93aa-3fefcc8a0c17))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 925e833a-ebf6-4c0e-8c8f-a0a85819f793))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp b1a5b1ab-31f1-4839-8a26-e0a2b130216d))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 09625107-fe54-4609-853b-75d63b00847a))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 0bdc5ef5-b0e7-40aa-978d-bf38dbf913f1))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 3f67813f-d4de-4276-bb02-7829f0ed2cfa))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp aed472dd-7d76-4b02-9367-808e87dcd0d7))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp ce32f92f-80bd-4bfc-a514-b48ccf923ac1))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp d6d6715b-8689-4ae3-a589-fea312faca3e))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "+12V") (pinfunction "Pin_2") (pintype "passive") (tstamp cdd2aa48-101c-4a6f-be3d-5778ac7dd82a))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp ae939f47-48ec-4d11-b5ee-d683dd1eb74a)
    (at 270.87 38.63)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/4138b77b-788b-46a9-a533-fae3b5df1c3c")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1f629ca7-8a42-4f65-9878-7f73971563c0)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4931c613-6093-42c7-9e46-21cee8b503d8)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp ae1a5948-8b8d-4f44-a4a0-0cac3fff0f2f)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 2d371cab-b296-4bad-959f-64fe9adb87b3))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 69d3e37a-bf05-456f-8693-b96434f585d4))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 305314c8-f8e6-4116-8dfa-5144f3ffeaa6))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 4ef6d7c3-69a5-4d05-a9a3-b581981b9df0))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 82829a71-13be-4d25-8b82-ee1288aabcc1))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp d793515e-342a-4aa0-bc0d-b275d6d0b84b))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 053c8ccc-4430-4c73-a4fc-a34966219d78))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 05ca0289-3199-43b9-a777-9115cf637f88))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 5c6c40ce-0d66-4e69-bf28-909dcba00a4c))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 71cfd421-36da-4ca8-8d1c-a9d4ab86571b))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C21-Pad1)") (pintype "passive") (tstamp ff9a2f5c-1e7b-428a-b48a-7a1f779c4d06))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 9d47b6cc-4aad-446e-a4d1-25b102540d49))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp b1a4a496-0d59-4ee9-ba10-bf379fa50676)
    (at 243.36 22.81)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/15f0b9d9-df93-44c9-a2f4-9296065f4b26")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c6e95c87-25af-4724-b974-8626e8c999f6)
    )
    (fp_text value "Conn_01x04" (at 0 9.95) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 26a16648-e7e8-443d-902e-44a20c8d139c)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 06adb7e5-6884-4684-8230-ad742a0053fe)
    )
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 19ce9658-8fe2-4e7d-bf88-978ce3efae9a))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 5b6be021-d63f-4a93-9797-6f4b1a0b1d6e))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 6761e91f-f736-482d-969f-8c4b9f01d3ba))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp ca553fd1-7ec0-454c-97e7-434f6725ab30))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp ec7f33c2-9da5-4a1a-98b2-1b1d271d5f1f))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp eec6191d-385e-49b7-859d-90fb67dcd2e9))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 316ab5ed-c17f-484b-a154-57ffb460f876))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 3d7dfd12-2092-46c3-9e46-523f72f225f2))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 9d48a373-beba-42c9-8d44-8b248cb74bf0))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp d5d9b379-d649-4ead-a875-5b11a39bcfc0))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 34387fb6-329a-44e2-95e1-dc1fab545a51))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 60491b48-0985-402d-8561-3c19f207b3e0))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 669978b6-01c8-481e-a54d-16ccf67938a9))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp cb29f7f2-4213-4210-a262-c0fef7fa8f40))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp f0412629-fae4-4c07-9d99-cbdecf4d62a4))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive") (tstamp 4b4de77d-f9df-4454-801d-aedcecb0fb17))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "SCL_DISP") (pinfunction "Pin_2") (pintype "passive") (tstamp 298df274-b72c-4700-8f09-bdf0a2aba235))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "SDA_DISP") (pinfunction "Pin_3") (pintype "passive") (tstamp 62b72a33-1190-436a-afd0-834ed52b6ec1))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3.3V") (pinfunction "Pin_4") (pintype "passive") (tstamp db8281b6-ef43-4aa9-9a8e-6ab8fa3efcb1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp b55cca33-99d9-421e-9736-5ec07d9bfaf4)
    (at 99.695 93.6225 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/8c6919d4-8ebe-4194-ba85-cf0142e9216c")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ebc7ddc5-dd4b-4ab7-8e68-be3b7b56b53b)
    )
    (fp_text value "82k" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6de0685d-7d8a-4718-a849-bc18f8449e85)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp cfb7b2d8-88c8-424e-8515-bac0a29a8b9c)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 2cd3e5ef-ca20-438f-839d-81efdbcab90a))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 2e55015c-7854-423a-88ee-fce6cba4a8e8))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 08e1b7a8-b5cc-4c56-b665-0a5864a73bc1))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 60017dbf-25d4-4981-a3f9-7271e6ee577e))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 91127f4d-e7f8-4126-ab05-5cf61a0e6cc0))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp bc3d2438-f561-4742-a0d9-4744ff7cd9a2))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 55cee63d-17e1-4ad2-a6d7-b4b1244a6dbc))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 630d7bf4-b807-47c0-823b-0fc65f5415f6))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 723db50c-062d-42ae-b9c5-783849f8f3b1))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 95d833e3-2de2-4d77-80c9-7c990bca101c))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(C16-Pad1)") (pintype "passive") (tstamp ab74d42f-a0c7-4157-b279-8da5a51b4742))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C16-Pad2)") (pintype "passive") (tstamp f9e17920-9875-499c-b665-fa76e5e0fc0f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_Elec_5x5.8" (layer "F.Cu")
    (tedit 5BC8D926) (tstamp bf60e285-c6d0-4e2f-92dc-bc9d87d163a4)
    (at 111.76 116.205 180)
    (descr "SMD capacitor, aluminum electrolytic nonpolar, 5.0x5.8mm")
    (tags "capacitor electrolyic nonpolar")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/35c37a5f-63a8-4b9d-bf93-c93bdfe6cd66")
    (attr smd)
    (fp_text reference "C23" (at 0 -3.7) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e15553a3-5e4b-4ffb-abb1-57c925efbe1f)
    )
    (fp_text value "10uF" (at 0 3.7) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2144bd94-11b1-40d1-95f2-904f19fb09fb)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 08e0c03a-27b3-4047-a711-0bc6dc2a6d93)
    )
    (fp_line (start -2.76 1.695563) (end -2.76 1.06) (layer "F.SilkS") (width 0.12) (tstamp 0405cf34-b641-4816-87a5-e5dc3a353461))
    (fp_line (start -1.695563 -2.76) (end 2.76 -2.76) (layer "F.SilkS") (width 0.12) (tstamp 54f4b796-f06b-469b-a19b-04c7219240bd))
    (fp_line (start -2.76 1.695563) (end -1.695563 2.76) (layer "F.SilkS") (width 0.12) (tstamp 67009c46-c8f4-4403-8aaa-df438d831080))
    (fp_line (start 2.76 2.76) (end 2.76 1.06) (layer "F.SilkS") (width 0.12) (tstamp 7f70bef2-91ac-4b43-a418-46c6722c7959))
    (fp_line (start 2.76 -2.76) (end 2.76 -1.06) (layer "F.SilkS") (width 0.12) (tstamp 9db7892c-0fe5-468f-90fb-36c72bc9d8e5))
    (fp_line (start -1.695563 2.76) (end 2.76 2.76) (layer "F.SilkS") (width 0.12) (tstamp ab25194f-2e54-4009-a3ff-c1c6ac68bd05))
    (fp_line (start -2.76 -1.695563) (end -2.76 -1.06) (layer "F.SilkS") (width 0.12) (tstamp ab25ada2-3d0c-421f-a622-46a6c141af18))
    (fp_line (start -2.76 -1.695563) (end -1.695563 -2.76) (layer "F.SilkS") (width 0.12) (tstamp ecbadf3d-e728-4e46-b0d3-a1154f1edf8d))
    (fp_line (start 2.9 -1.05) (end 3.7 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 239ee258-e74e-4810-ad8c-d3931403aa86))
    (fp_line (start -2.9 -1.75) (end -2.9 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 51fb96e8-804e-413e-ba72-d79406c12de7))
    (fp_line (start -3.7 1.05) (end -2.9 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 5ab53550-571c-471c-8ab6-4afbad1cd888))
    (fp_line (start 3.7 1.05) (end 2.9 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 850e0366-7b7e-4c88-b36b-d6a32bf9d8fb))
    (fp_line (start 2.9 1.05) (end 2.9 2.9) (layer "F.CrtYd") (width 0.05) (tstamp a76aed77-3ff7-4f7d-966e-19f413ed7497))
    (fp_line (start -2.9 -1.05) (end -3.7 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp bd8df726-3a86-4748-8c1a-a64fdb4b360e))
    (fp_line (start -2.9 1.05) (end -2.9 1.75) (layer "F.CrtYd") (width 0.05) (tstamp bdad84fb-3918-4b90-bedd-5691b60e8ace))
    (fp_line (start 2.9 -2.9) (end 2.9 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp c7d9e0fa-d2b2-4534-9f48-bd7d4ecae974))
    (fp_line (start -2.9 -1.75) (end -1.75 -2.9) (layer "F.CrtYd") (width 0.05) (tstamp cdf0f046-db3f-4213-b17c-594f934b8ca9))
    (fp_line (start -3.7 -1.05) (end -3.7 1.05) (layer "F.CrtYd") (width 0.05) (tstamp d76f2016-70fe-4afc-8db1-909056028a68))
    (fp_line (start -1.75 2.9) (end 2.9 2.9) (layer "F.CrtYd") (width 0.05) (tstamp d914c5c7-e7cf-46d2-9096-99b173293dec))
    (fp_line (start 3.7 -1.05) (end 3.7 1.05) (layer "F.CrtYd") (width 0.05) (tstamp def7e0f1-a059-450e-a8b2-a30a3d2f9589))
    (fp_line (start -1.75 -2.9) (end 2.9 -2.9) (layer "F.CrtYd") (width 0.05) (tstamp edac4882-a24b-480a-91ea-9d8f6f0faf60))
    (fp_line (start -2.9 1.75) (end -1.75 2.9) (layer "F.CrtYd") (width 0.05) (tstamp fecda349-8613-4d66-896d-026a8746831b))
    (fp_line (start -1.65 2.65) (end 2.65 2.65) (layer "F.Fab") (width 0.1) (tstamp 38883051-525a-4fa9-990b-411a0da6d45d))
    (fp_line (start 2.65 -2.65) (end 2.65 2.65) (layer "F.Fab") (width 0.1) (tstamp 87fd59e0-3ff3-429d-965a-0443ac4e9c5e))
    (fp_line (start -2.65 -1.65) (end -2.65 1.65) (layer "F.Fab") (width 0.1) (tstamp aa81c5d7-3851-477e-a2a8-9b89cbfc6872))
    (fp_line (start -2.65 -1.65) (end -1.65 -2.65) (layer "F.Fab") (width 0.1) (tstamp b2a3b35e-6170-4316-b185-fccc22c026da))
    (fp_line (start -1.65 -2.65) (end 2.65 -2.65) (layer "F.Fab") (width 0.1) (tstamp e44c43d2-1fb5-43cb-84da-ae3bafa71dfd))
    (fp_line (start -2.65 1.65) (end -1.65 2.65) (layer "F.Fab") (width 0.1) (tstamp e80ab0e7-a80d-4526-ae1c-bf5343d148df))
    (fp_circle (center 0 0) (end 2.5 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 68cd1b32-9bb0-47a2-9625-3674eeac41c7))
    (pad "1" smd roundrect (at -2.0625 0 180) (size 2.775 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 37 "Net-(C23-Pad1)") (pintype "passive") (tstamp 929875cb-e7e7-4b3e-8d38-7a0d262580f1))
    (pad "2" smd roundrect (at 2.0625 0 180) (size 2.775 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 17 "A_OUT") (pintype "passive") (tstamp 32dc14f9-f43f-4eaa-95c3-a71e840a4344))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_5x5.8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp bf6d45f8-8e48-4fb2-a64f-f5d42f63e557)
    (at 257.82 40.46)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/b85eec5f-eca0-403b-a490-6d6cb87aecd9")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 89c4e8da-2e89-4b8c-bc73-3ecc108d3fc8)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d018a57c-6f2f-4ad4-89fa-273597650a7f)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp e1de5f9d-109d-4401-a72d-02762c984322)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 4d7f8832-d67c-490c-b78b-e9f11f3a04ae))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp a53cc6dc-e0ad-4363-86ca-fa58f82c2696))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 12f659ab-bd3b-4ce8-8149-dd2c2f33482e))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 160a829d-b4c8-4cec-8214-a6ca1abb95a0))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 99386515-5d29-4423-a365-aed8114fe75e))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp df0ec0b3-26e2-43ba-bb55-965228dbd753))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 0675678a-273e-441b-9b90-2a3c2fc3673e))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp a5c21a8e-6614-4ba8-8145-4bc903a3731a))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp e544dafa-2628-48f9-bff2-1aa457b14730))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp e9c791b3-eec3-4b1a-9ed4-df5d407ae5c6))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pintype "passive") (tstamp 7378ff3a-6ce2-402a-8f84-47987860bc82))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(C4-Pad1)") (pintype "passive") (tstamp fd9945fb-aee0-4678-b9c6-e890b1ab3458))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp c9b95ecf-c68d-4cc1-babd-fd0c83626337)
    (at 85.09 93.1175 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/6534bd7c-5ff9-4195-80a9-53649104f2b1")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8a9ae691-e1cd-486e-b9f4-1188b5f2eaef)
    )
    (fp_text value "1nF" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5c5e36f0-98a0-41be-af46-3d631f621ee8)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp f745413a-1909-44c0-8916-40da24839f25)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 2ef449e2-12b8-4c04-b389-dbcd72093251))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp ea8ecaf5-b5c7-446c-89dd-70d72b8c2323))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1417060e-b236-4c06-bbe7-e6b8fa7e5317))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1f4b097c-c703-4c40-9611-c917b45a2da3))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 8d7d8ca2-6589-42a9-a571-ab708c136ee4))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 8edcb682-314a-4449-87aa-358c6cb8ca85))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 101e9005-3274-45c0-aac6-4c5901129a29))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 6475ce4d-2b47-4509-b374-3254b61d80e7))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 9184f285-e85d-4e65-ab1b-4f994ab91c94))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp d8506380-e529-4959-9bd8-af21150c7bac))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(C17-Pad1)") (pintype "passive") (tstamp c63b74dd-f6f6-40d1-bfa5-f00d7ac42936))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(C17-Pad2)") (pintype "passive") (tstamp 39c1a846-c1d3-46e9-b407-cda14ecb56a0))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp ca163ac5-22ce-4fbd-a447-321daecf7f57)
    (at 257.16 37.95)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/9e352b0c-8534-4df0-9584-baccc15d7647")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 29f253b7-bfaa-4963-95a2-b974a229dafe)
    )
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d1e34dcb-c052-4d85-9706-27c8d25aa71e)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 75e1a1bb-0e5d-4a2a-af06-60dc8cf3b4b3)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 84764e0a-ed08-46eb-a137-27cf7aad0565))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp dd5c1ed0-2cd4-40e6-87e3-ff8129237900))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 405f4f7c-88ae-46e9-b239-a9df0e85caf4))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp bb89e3ab-6d60-4009-bb2d-d41fc5f184cf))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp db050336-a07c-40b2-9695-4d5b7bdfec3d))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp fc61812f-c4d1-4ec4-a50b-0fd5bdafb4b3))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp b00c13ab-7032-4892-a541-b9dd38988013))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp ced80195-3a1e-4fec-9846-7386c15a6491))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp e3edda4c-b1f0-4077-8b1d-2cd694aa109f))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp e40dcf53-1f60-4cce-9798-24555ad81d7c))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pintype "passive") (tstamp fb096ec5-f699-4fab-89c3-3650d74f4192))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 7c6e73bc-2c72-442f-8994-c1c150b548e6))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "misc:YAAJ_BluePill_2" (layer "F.Cu")
    (tedit 5F81AE11) (tstamp ca3e6fa0-782b-4215-8bd1-03fbae335130)
    (at 132.08 107.315 180)
    (descr "Through hole headers for BluePill module. No SWD breakout. Fancy silkscreen.")
    (tags "module BlluePill Blue Pill header SWD breakout")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/7adaa88d-df55-4493-b328-098067816dd2")
    (attr through_hole)
    (fp_text reference "U6" (at 7.62 -3.81) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bd914e52-ac64-4c50-b8e8-fe5656988404)
    )
    (fp_text value "YAAJ_BluePill" (at 20.32 24.765 90) (layer "F.Fab") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 00877895-49a6-4425-bd58-61d8b2b0408d)
    )
    (fp_text user "Y@@J" (at 2.921 -1.016 270 unlocked) (layer "Dwgs.User")
      (effects (font (size 0.5 0.5) (thickness 0.1)))
      (tstamp e1643047-e41b-4ec9-9e08-e38cbf1479f7)
    )
    (fp_text user "REF**" (at 7.62 24.13 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3c66d7c2-76af-40ce-bc7a-70e877f333c8)
    )
    (fp_line (start 1.33 1.27) (end 1.33 49.59) (layer "F.SilkS") (width 0.12) (tstamp 03c3da2f-f65f-4780-812c-5983ca602ca5))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 1426d9a7-934b-4f20-9312-45b265655e3b))
    (fp_line (start 13.97 -1.27) (end 16.51 -1.27) (layer "F.SilkS") (width 0.12) (tstamp 3bc4614d-b75a-414e-af2e-f1d8dc0f222a))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 90d109e6-1740-4f81-b488-8fb00e3c10bb))
    (fp_line (start 18.995 -2.445) (end 18.995 50.705) (layer "F.SilkS") (width 0.12) (tstamp 90e96106-f273-48ac-8701-a161e6705533))
    (fp_line (start 16.51 49.53) (end 13.97 49.53) (layer "F.SilkS") (width 0.12) (tstamp 9498ec38-005a-4bc5-8a6e-9e0e96a75bbe))
    (fp_line (start -1.33 49.59) (end -1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp b2913903-3dd7-4c23-9981-caab898a96fe))
    (fp_line (start 13.97 49.53) (end 13.97 -1.27) (layer "F.SilkS") (width 0.12) (tstamp b2ce6c30-87ea-4de9-b724-185af3145b4f))
    (fp_line (start 18.995 50.705) (end -3.755 50.705) (layer "F.SilkS") (width 0.12) (tstamp c83a98c7-0b14-4e21-aa27-29116161f872))
    (fp_line (start -3.755 50.705) (end -3.755 -2.445) (layer "F.SilkS") (width 0.12) (tstamp cef9930b-c0f8-4578-958d-3a0ef78b9be2))
    (fp_line (start 1.33 49.59) (end -1.33 49.59) (layer "F.SilkS") (width 0.12) (tstamp e459f3fe-cc60-4258-96b2-92a64cc2d73f))
    (fp_line (start -3.755 -2.445) (end 18.995 -2.445) (layer "F.SilkS") (width 0.12) (tstamp ea69a46c-f9db-4474-b1aa-990057c16f7b))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp eb960089-2bd8-4bae-b911-d9a752ee4245))
    (fp_line (start 16.51 -1.27) (end 16.51 49.53) (layer "F.SilkS") (width 0.12) (tstamp f464eba5-c393-4b98-91a0-771e47d8dff6))
    (fp_line (start 17.04 50.06) (end 13.44 50.06) (layer "F.CrtYd") (width 0.05) (tstamp 025272cf-fb4a-4886-a5f8-510ca87fe8a7))
    (fp_line (start -3.93 -2.62) (end 19.17 -2.62) (layer "F.CrtYd") (width 0.05) (tstamp 049ba09e-900d-4b06-bc43-08ca032ad5eb))
    (fp_line (start 13.44 -1.8) (end 13.44 45.72) (layer "F.CrtYd") (width 0.05) (tstamp 2b0c6f2f-134d-44c0-a0a9-08568ec8c51f))
    (fp_line (start -3.93 50.88) (end -3.93 -2.62) (layer "F.CrtYd") (width 0.05) (tstamp 36c8134e-19b8-4bec-b799-554b3e3aff9f))
    (fp_line (start 13.44 -1.8) (end 17.04 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 49010942-4c47-4a78-837b-8199ebb9b2b8))
    (fp_line (start 17.04 -1.8) (end 17.04 50.06) (layer "F.CrtYd") (width 0.05) (tstamp 5d39283e-3f66-49d9-8ab7-2fc8508ecf6c))
    (fp_line (start 1.8 45.72) (end 1.8 50.06) (layer "F.CrtYd") (width 0.05) (tstamp 5f3b2e73-8a64-42a1-a508-b7994b7ca2e9))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 661c1c9d-f3aa-475c-96b6-4af84256ec46))
    (fp_line (start 19.17 -2.62) (end 19.17 50.88) (layer "F.CrtYd") (width 0.05) (tstamp 6efd1061-063e-49f4-825e-3eb4fd0a0828))
    (fp_line (start -1.8 -1.8) (end -1.8 50.06) (layer "F.CrtYd") (width 0.05) (tstamp 79643167-c2fa-4785-8203-d86754569cee))
    (fp_line (start -1.8 50.06) (end 1.8 50.06) (layer "F.CrtYd") (width 0.05) (tstamp 8ac70570-98ce-4dc5-9907-812f18964cca))
    (fp_line (start 1.8 -1.8) (end 1.8 45.72) (layer "F.CrtYd") (width 0.05) (tstamp 94e15bcc-abe3-44bd-9702-983304d05067))
    (fp_line (start 19.17 50.88) (end -3.93 50.88) (layer "F.CrtYd") (width 0.05) (tstamp ac614fdc-8377-4414-b7f1-79ef33ad4bee))
    (fp_line (start 13.44 45.72) (end 13.44 50.06) (layer "F.CrtYd") (width 0.05) (tstamp fbfa9879-c417-40fe-ba9f-52a676c073c0))
    (fp_line (start 18.92 -2.37) (end 18.92 50.63) (layer "F.Fab") (width 0.12) (tstamp 087c5375-4143-4d8c-8725-6f75c356fa27))
    (fp_line (start 1.27 49.53) (end -1.27 49.53) (layer "F.Fab") (width 0.1) (tstamp 164335ed-0d95-45ce-9f60-6db293b67b1f))
    (fp_line (start -3.68 50.63) (end -3.68 -2.32) (layer "F.Fab") (width 0.12) (tstamp 3492c177-dd65-4dda-a611-c77c30c48b04))
    (fp_line (start 16.51 49.53) (end 13.97 49.53) (layer "F.Fab") (width 0.1) (tstamp 4b0afc34-525c-4fea-9ac3-0df5d3d28d00))
    (fp_line (start 13.97 -1.27) (end 16.51 -1.27) (layer "F.Fab") (width 0.1) (tstamp 5d44a06a-8cab-4848-9102-bf39ce7b7fa0))
    (fp_line (start 13.97 49.53) (end 13.97 -1.27) (layer "F.Fab") (width 0.1) (tstamp 6a366248-4e77-401c-bb75-842ff47d5dc1))
    (fp_line (start 11.52 3.48) (end 11.52 -2.32) (layer "F.Fab") (width 0.1) (tstamp 6c08332b-c463-4e52-975b-6cdfbf9b814c))
    (fp_line (start -1.27 49.53) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 859cc295-a399-43ab-bdcc-31666f2a4c02))
    (fp_line (start 1.27 -1.27) (end 1.27 49.53) (layer "F.Fab") (width 0.1) (tstamp 94306e2c-903d-44a3-8dbe-8a9240bab91f))
    (fp_line (start -3.68 50.63) (end 18.92 50.63) (layer "F.Fab") (width 0.12) (tstamp a6f091ff-7b7c-47a1-a3e7-ea267f08a28d))
    (fp_line (start 3.72 3.48) (end 11.52 3.48) (layer "F.Fab") (width 0.1) (tstamp acf19aa5-d035-4926-9b0d-05920f0e843f))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp bcc78cf0-77fe-47fb-a9d3-9ea7d939a05d))
    (fp_line (start 3.72 3.48) (end 3.72 -2.32) (layer "F.Fab") (width 0.1) (tstamp c2493a59-5bec-45a2-9b20-c78870cdf5f3))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp c47261b0-1e00-4d32-9a31-4190fc72fdc6))
    (fp_line (start 16.51 -1.27) (end 16.51 49.53) (layer "F.Fab") (width 0.1) (tstamp cafbf90d-ed41-4ba1-8fb5-8f6cddb723d3))
    (fp_line (start -3.68 -2.37) (end 18.92 -2.37) (layer "F.Fab") (width 0.12) (tstamp f77010ab-2152-49bf-9e35-ce14b436953b))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J6-Pad2)") (pinfunction "PB12") (pintype "bidirectional") (tstamp 7480f15c-c2c5-49e4-8212-777a90c6c504))
    (pad "2" thru_hole circle locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J6-Pad3)") (pinfunction "PB13") (pintype "bidirectional") (tstamp e7109592-367a-479a-9fa0-0b11c3379839))
    (pad "3" thru_hole circle locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J6-Pad4)") (pinfunction "PB14") (pintype "bidirectional") (tstamp 0cf9adf1-52ab-4ab3-9f29-7cf856891bf9))
    (pad "4" thru_hole circle locked (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J6-Pad5)") (pinfunction "PB15") (pintype "bidirectional") (tstamp 299eeef0-7d56-4635-b020-01ded05170dd))
    (pad "5" thru_hole circle locked (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "unconnected-(U6-Pad5)") (pinfunction "PA8") (pintype "bidirectional") (tstamp 5d985f00-0a29-4042-823a-6e7651ff27c5))
    (pad "6" thru_hole circle locked (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "unconnected-(U6-Pad6)") (pinfunction "PA9") (pintype "bidirectional") (tstamp 6e1a1e20-b466-4cfc-b747-531b3a7b4804))
    (pad "7" thru_hole circle locked (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "unconnected-(U6-Pad7)") (pinfunction "PA10") (pintype "bidirectional") (tstamp b25502f2-2bb5-4de4-9a78-a44f5e195701))
    (pad "8" thru_hole circle locked (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "unconnected-(U6-Pad8)") (pinfunction "PA11") (pintype "bidirectional") (tstamp 83244c00-2de8-4e03-88fd-8efb20155da9))
    (pad "9" thru_hole circle locked (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "unconnected-(U6-Pad9)") (pinfunction "PA12") (pintype "bidirectional") (tstamp 2830768c-d91f-465e-9528-16eeb4230408))
    (pad "10" thru_hole circle locked (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "unconnected-(U6-Pad10)") (pinfunction "PA15") (pintype "bidirectional") (tstamp c0f3da99-8398-4763-8316-8e5656f1c4cd))
    (pad "11" thru_hole circle locked (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "unconnected-(U6-Pad11)") (pinfunction "PB3") (pintype "bidirectional") (tstamp 24e161dd-670f-4bc3-875e-1ef4505a3fa6))
    (pad "12" thru_hole circle locked (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "unconnected-(U6-Pad12)") (pinfunction "PB4") (pintype "bidirectional") (tstamp 522fb391-610b-4bf7-8e27-a02533615dd3))
    (pad "13" thru_hole circle locked (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "RX_EN") (pinfunction "PB5") (pintype "bidirectional") (tstamp b4e25d29-0ab4-4b58-aec8-173cf28ba6dc))
    (pad "14" thru_hole circle locked (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "SCL_PLL") (pinfunction "PB6") (pintype "bidirectional") (tstamp 4559243c-8bb1-4f66-a32a-81fee340a3bd))
    (pad "15" thru_hole circle locked (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "SDA_PLL") (pinfunction "PB7") (pintype "bidirectional") (tstamp 723f14f0-85da-45bc-8f86-b7d2aa0fbad4))
    (pad "16" thru_hole circle locked (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "A_OUT") (pinfunction "PB8") (pintype "bidirectional") (tstamp ae89c82d-ccf7-4919-8e22-79d579f3a911))
    (pad "17" thru_hole circle locked (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "unconnected-(U6-Pad17)") (pinfunction "PB9") (pintype "bidirectional") (tstamp 4c4bbd7a-a2a8-4a6e-bdf1-deb04bf75958))
    (pad "18" thru_hole circle locked (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "+5V") (pinfunction "5V") (pintype "power_in") (tstamp ac69b636-28a3-4665-b38b-15483d7c0c0d))
    (pad "19" thru_hole circle locked (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp e6254c1e-6be8-4cf4-b7b1-e0a15d850699))
    (pad "20" thru_hole circle locked (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3.3V") (pinfunction "3V3") (pintype "power_in") (tstamp 5b67b657-56f2-402a-b4fb-5932bd45cfcf))
    (pad "21" thru_hole circle locked (at 15.24 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "unconnected-(U6-Pad21)") (pinfunction "VBat") (pintype "power_in") (tstamp 486c2427-8734-483c-a8d3-6222a8cf6179))
    (pad "22" thru_hole circle locked (at 15.24 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "unconnected-(U6-Pad22)") (pinfunction "PC13") (pintype "bidirectional") (tstamp 708b6528-f34b-40fc-8290-d62bdacfa1a9))
    (pad "23" thru_hole circle locked (at 15.24 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "unconnected-(U6-Pad23)") (pinfunction "PC14") (pintype "bidirectional") (tstamp 546eec0c-b413-4bf8-8be2-9b2af651a31f))
    (pad "24" thru_hole circle locked (at 15.24 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "unconnected-(U6-Pad24)") (pinfunction "PC15") (pintype "bidirectional") (tstamp a22be040-b616-452a-80bf-ecd99f5b5688))
    (pad "25" thru_hole circle locked (at 15.24 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "ADC_I") (pinfunction "PA0") (pintype "bidirectional") (tstamp b11ece41-5a5f-409a-9a0d-38eab9f917de))
    (pad "26" thru_hole circle locked (at 15.24 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "ADC_Q") (pinfunction "PA1") (pintype "bidirectional") (tstamp 4e214afe-3e53-49e1-a9c7-2bd60b25aead))
    (pad "27" thru_hole circle locked (at 15.24 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "unconnected-(U6-Pad27)") (pinfunction "PA2") (pintype "bidirectional") (tstamp 1ee71046-2c17-43ee-8797-181cfdcfbd4c))
    (pad "28" thru_hole circle locked (at 15.24 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "unconnected-(U6-Pad28)") (pinfunction "PA3") (pintype "bidirectional") (tstamp 5ff5e036-c9f4-414f-ab4e-1ae9dad5a387))
    (pad "29" thru_hole circle locked (at 15.24 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "ADC_MIC") (pinfunction "PA4") (pintype "bidirectional") (tstamp 670f77a6-bbda-4db8-a27a-591b52934533))
    (pad "30" thru_hole circle locked (at 15.24 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "unconnected-(U6-Pad30)") (pinfunction "PA5") (pintype "bidirectional") (tstamp 3d053c59-df51-4089-bfc2-59deda192fd8))
    (pad "31" thru_hole circle locked (at 15.24 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "BIAS_PWM") (pinfunction "PA6") (pintype "bidirectional") (tstamp 2d773f1a-aaff-4b84-80f9-451d032fa5ed))
    (pad "32" thru_hole circle locked (at 15.24 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "unconnected-(U6-Pad32)") (pinfunction "PA7") (pintype "bidirectional") (tstamp c7f35325-3ba4-43f4-a222-7a30b924dc16))
    (pad "33" thru_hole circle locked (at 15.24 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "unconnected-(U6-Pad33)") (pinfunction "PB0") (pintype "bidirectional") (tstamp ea5bd477-ccf4-48be-be8c-36434a16e00d))
    (pad "34" thru_hole circle locked (at 15.24 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "unconnected-(U6-Pad34)") (pinfunction "PB1") (pintype "bidirectional") (tstamp a7dab6bb-bf7f-4c15-862e-2e4ee1d26d52))
    (pad "35" thru_hole circle locked (at 15.24 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "SCL_DISP") (pinfunction "PB10") (pintype "bidirectional") (tstamp 4c94973a-8ee8-4fe3-bcdf-84ea37f5068d))
    (pad "36" thru_hole circle locked (at 15.24 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "SDA_DISP") (pinfunction "PB11") (pintype "bidirectional") (tstamp c31be386-676f-44b7-a441-fda1e011d33f))
    (pad "37" thru_hole circle locked (at 15.24 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "unconnected-(U6-Pad37)") (pinfunction "RST") (pintype "input") (tstamp f2e0e4b7-0971-4b74-9f84-277465e68399))
    (pad "38" thru_hole circle locked (at 15.24 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3.3V") (pinfunction "3V3") (pintype "power_in") (tstamp e7b03bf4-a5c2-467a-956c-3cc5e99f45ff))
    (pad "39" thru_hole circle locked (at 15.24 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 8b97a150-fa47-4295-9e88-adabc8a04ced))
    (pad "40" thru_hole circle locked (at 15.24 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 389e9c83-7a93-449e-b842-dd13126c729f))
    (model "D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinHeaders_H_SWD_cp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinHeaders_No_SWD_cp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinHeaders_V_SWD_cp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinSockets_H_SWD_cp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinSockets_No_SWD_cp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Blue_Pill/YAAJ_BluePill_PinSockets_V_SWD_cp.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp cca7da8c-04d5-41dc-b261-bc0008566fb2)
    (at 266.52 43.65)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/51683a91-0e42-41b5-8295-ce0c9db18f2f")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 58780d9f-0780-433a-b8e7-f9810a4cf1b0)
    )
    (fp_text value "1k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2ce7488a-c693-4eb8-984d-d314c47823d5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 4e81abcd-2f60-4358-b33e-0b43b651e12d)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 9e8c121e-91ce-4fb4-ba8e-d2021bcf9973))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp de288ace-3d82-4a4a-ab65-b5751424794a))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 00e3a722-07e0-4f2e-b424-5d2942812cd1))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 7ed135df-43dc-42af-b4c3-e8d9d8af2f21))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp d35c9e59-8937-4f78-81be-7f9c5742f049))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ef047e2c-bca3-4827-b225-94294c866900))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 34b1ddec-3986-4413-9bd9-4bb3db34a393))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 5688a857-c404-4500-8919-fc71283561e5))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 9377a82b-0cd0-465c-8a63-9d7473a20f83))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp d0fc2987-08a8-4cf3-a5db-5aad36b5606e))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "RX_EN") (pintype "passive") (tstamp f88afe3d-0b76-49da-a0cd-97ebd8d4b2ea))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(Q1-Pad2)") (pintype "passive") (tstamp e1512baf-495a-4040-8f13-a64e1a1bf72e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp d68e7495-ee08-486a-b1b5-264836a91492)
    (at 66.04 93.1175 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/43204522-6598-46fe-b406-3f97da5aee5e")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 886d49a1-8138-4456-917e-4741d0e6667f)
    )
    (fp_text value "470nF" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0d7583a0-0771-4d28-81db-52cd5d7d1a45)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 0e53633d-e402-4390-bdca-73ce6f891549)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 355d4d01-4ded-42b0-8bb1-cb0164f694cc))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp ef8812b9-633e-4046-8e96-bf0399e97db3))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 54a436b3-5445-4280-bf8b-2e15cdc9b3b2))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 5c649af1-64f7-4000-8a54-7531d08087a7))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 60133e98-68a5-4248-9543-b4cf46247671))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 761cb538-b8a8-4257-ad38-1906ebf00ad3))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 9bea39aa-7b98-4f62-91b5-18a6a5cae4fc))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp d49a6568-04b7-4a94-b4b6-498907084b7e))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp f1abac94-5dda-4858-8815-34f8c13781b6))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp f9ee2bda-5cdf-49f9-b29d-6ca789014709))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C9-Pad1)") (pintype "passive") (tstamp 9b420c80-e736-4034-9048-c0a7191f0060))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 66fa4145-b553-45c9-af6e-f5814a31b4f0))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp d8760442-9243-43cc-bd2a-2eecaf3b428f)
    (at 71.755 97.79)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/c2227004-7a20-4569-81af-beac94841cde")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 14e51ae5-a86e-4b9b-bbb8-010a5da959a6)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 896bc49c-8442-4bcb-9505-a710f8a05919)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a6e0cdbc-abcc-46e5-a6de-f073ab3e004f)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 8ef89a4f-e456-45e6-a9db-14867eabfcac))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 0a461664-2d89-4c0a-9024-a3fd9d0c5a7e))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(C13-Pad1)") (pinfunction "1") (pintype "passive") (tstamp dbb09a1d-9c10-4f15-852b-28f2983e21bf))
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp db32c4e8-81c3-4ce1-bfa5-82de72c25a40)
    (at 270.87 36.12)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/0e181ed0-8de2-4f1e-9ee6-edeaac8ca954")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 917b0b46-eb5f-41fb-b70c-f3a3d06a289a)
    )
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cf1bac66-3a76-400c-baed-78c024c278c5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 0243b81b-15dc-4e0e-940a-c01e45e52948)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 4f4d3480-b21b-4333-9389-743acb147b18))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 9cf95596-49a5-400f-8c29-203b32d0f609))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 807246b9-3487-4c2d-b873-cf8159bc6c37))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp b5da3989-fab2-4cae-8ed3-6979dc193295))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp e448b21a-764c-46e2-90d6-3814b5b4a52a))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ff4c7020-e907-4029-9515-8b05103fc61f))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 10eca808-1fc9-4905-9b9f-8c16bd9c36ec))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 23ad2289-e9c9-4787-91a9-9da1810180de))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 889fcb90-6130-4962-a62a-ca44b29783b0))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 8fb1d60c-e7b8-4aec-b070-a519661b5659))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pintype "passive") (tstamp 6959f5bb-ddc8-4928-99eb-522040436b02))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 2470c3b4-1b0c-4e16-a859-90799b020bc2))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp db5cde42-88a5-430f-83c7-64cc47b4af32)
    (at 262.17 47.99)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/48e29ffa-76cb-4ea8-97ea-fa1619863245")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fb84ea8b-84ac-4e93-bc06-9b4b39c6329c)
    )
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8fb68bb9-cb05-431e-9fb3-7a6ee61a2f6a)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp c257e621-5604-4294-a3ee-1b3c232bd2f0)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 0a720e94-4bef-4bda-8516-86a76b58a12d))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp c9097eee-c848-4ba2-bf0e-327565ab4900))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 241d4d53-279f-4e4a-94f0-6a130bda6867))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 45befde9-39f6-45b9-8714-cad6262218ec))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 83bedc46-07a8-483b-9241-90e3861af4b6))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp ca61abbc-765c-4e80-9633-cd08e4e5cd8f))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 2c2c0c97-b882-49e7-b904-05931437a4fb))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 864fd37d-1a18-45e7-8b02-4ff462276bb8))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 8f8df145-9616-474e-bdc0-456b86921ae8))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp fb08ce95-e0ca-4570-b009-d45fa6a53df9))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pintype "passive") (tstamp 03118d8e-0697-49d9-ab6f-c1960bafc97c))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp f51c99a4-750f-4972-8350-39a0ab6921c4))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp dd31f049-96b6-44f9-b41d-496db876331c)
    (at 243.36 35.06)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/8409de60-b60d-4e11-8047-169212ce9d12")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bc5c740f-9496-49a1-a517-6fb40e07fa55)
    )
    (fp_text value "Conn_01x02" (at 0 4.87) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e1863618-1385-486c-9a54-d355d09bd057)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1f24b0a1-99bd-4f3e-b574-82af3374dbfd)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 2478b628-6237-4739-888e-bb74b67329a7))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 26a68f88-423d-4b55-ba32-ee5a08f5a8b1))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 56c3fc4b-487d-4d0b-99e4-1fcb1424b62b))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp ac5d4caa-8f61-4925-8279-1ab63f1aab74))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp c03c444e-fb90-4777-84cb-323563def378))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp c2770444-70b3-4529-a141-6bf5983ca5b2))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp 1a7c3da5-6fe8-4a39-bab5-dbe79678a38b))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 68ae4e55-7002-4c1e-8d4b-b2550096820a))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp 9ea7b6c1-665f-48f3-8ddf-6856a74ee7b6))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp fd903cdd-46e7-4ff9-9685-71b1ec5d1138))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 00336e5b-e1e6-4be8-ae22-fd32e0092a7c))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 2c139b6e-9a8c-45f6-9893-d4fde0ba277d))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 85f6a2ad-4ec3-41c6-86d8-234d64c442e5))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 914950a6-9925-43f8-97f3-aca67e7aea72))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp fdd8c091-d0a3-4bac-beca-eb8d2ff7ab64))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(C21-Pad2)") (pinfunction "Pin_1") (pintype "passive") (tstamp fafa3975-9584-4d65-b106-c69672c7f4f5))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp 88adc9da-cccc-4ead-85af-0848599d85af))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp e0ea3e14-5867-4094-9261-eb9e1645c369)
    (at 177.855 48.665)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/f73a9ed1-1b51-4f32-b2ae-6f86a9a0ed79")
    (attr exclude_from_pos_files)
    (fp_text reference "TP12" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6401f911-2000-416f-9312-48bd852b339b)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e33c342a-d29a-43bb-9e7d-377f99446842)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9510eab5-64d3-4182-b9df-d3a12e2922ad)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 47236a3f-a1f9-4a63-808a-e90f5224ef0a))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 874bb3da-a83c-4455-9302-679dfa7ff935))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 "A_OUT") (pinfunction "1") (pintype "passive") (tstamp 1b00aa06-577c-4c61-bb0c-b991a5ee1d21))
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp e384b5e0-e24d-4937-9884-1a14e895e877)
    (at 79.815 95.885)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/a350f3a7-14ce-4f94-ae60-bda37ed6775e")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c01d9a5a-1ba9-4ca0-86aa-bf846438b19d)
    )
    (fp_text value "100" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6a536436-d7e7-4101-8870-89088fb6f250)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp c804716c-4218-4e36-9b53-cdec55440179)
    )
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp 0174f2e6-4f20-403a-b71f-e55bf77a66d8))
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 05d6e8bd-ae8a-4cad-8c02-e5f34ee2ff6a))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 1517feed-5a69-49ad-af84-d662766bd898))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 404db52d-ebd3-4e3e-b2ae-b0c8713ad540))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 5766c38b-e4fc-44d1-aa42-c450df01eb3c))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 9c2e91be-53b7-4b3a-b4a7-f68ffa0948e4))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 21fffe65-66dd-45de-ba22-48d67ca50f4f))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 2998cf7c-e3c9-456e-b2a5-b6df90b181d6))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 6a305b85-97d9-41fa-b9c3-73fa8dc9e17d))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp c1b66ec9-15b6-44ff-940b-47b913830702))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C10-Pad1)") (pintype "passive") (tstamp 8d866224-f247-43c6-8287-5109e80a6e32))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(R11-Pad2)") (pintype "passive") (tstamp a7c31a72-52d6-4fea-a051-531852c32f3f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp e80b1ceb-cb95-4d8c-8c9a-8658bf5172c6)
    (at 66.04 97.3825 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/313c0fa0-61d4-4b53-b275-d5ff75cd37cf")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 43c2f996-0836-48bb-a552-89cf7b28c8a5)
    )
    (fp_text value "470nF" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3178bc28-2ee2-4a3b-8079-9ee003dde8b2)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 5f1b5628-4e7d-40f6-a0e8-b1c206945f6d)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 4756e23f-7eac-463b-a717-be902472ffee))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp e5a275c8-e7a3-4246-bc3d-49d33c05fcdb))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 35e004b5-b987-4aa9-a050-9fc587ac3f70))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 50afa8ca-c582-47a4-8999-3c4b04d7e19e))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 8bf78839-4144-429e-9fed-0c18d6c23f81))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp b3d01248-4209-4e1c-ba52-eff58e3c693c))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 2a39a630-f7e7-420e-b4ff-45965d0512aa))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 32b72e78-ce49-4690-83be-3cd0b237b9dc))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 81a65893-7655-486b-89cc-4acf7edb7133))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp ef051686-33ba-4c09-8510-fc4bb0325abf))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C10-Pad1)") (pintype "passive") (tstamp 3783f150-97fb-4152-9c21-0d41c6cee692))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive") (tstamp 52588e7b-b1e7-44e2-a4f0-7060b5ff95b6))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp ea760113-6623-47fa-89e2-65e93e308982)
    (at 101.6 93.5725 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/fe192179-41f0-4802-9dad-b911489e3798")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 18ebec70-a7e4-487e-a110-d71da4823844)
    )
    (fp_text value "1nF" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 92cffdb5-24fb-4347-bc96-9cf07816cbc3)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 8786fecd-fdfc-467a-b85d-386dfeffe725)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 84022c34-8f77-4045-9051-56126312c7ef))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp cfaea74d-6bc3-4668-8aae-090c14d837ce))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 36f60caf-62df-44bf-9c99-10adcd569e90))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 6628dac5-e93d-4ca7-9359-e81f428cfa77))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 96e66f24-aef6-4afe-83fa-ad1765ca36d2))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp a7eddf6b-638d-46ab-82aa-89297708b5f8))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 081e3fa0-fb29-4f39-8c62-167d3efc0720))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 2aecf531-4d02-4a39-9872-31a80981ef04))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 68dd5aed-4930-498b-936b-37e6289816da))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp a531b523-aaf4-400b-8d38-652ac0fc57cc))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(C16-Pad1)") (pintype "passive") (tstamp 97591834-4c78-4ee0-83f8-7c5f5c49e359))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C16-Pad2)") (pintype "passive") (tstamp 732d1a23-3a55-4ba9-b503-572d4847630d))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_Elec_5x5.8" (layer "F.Cu")
    (tedit 5BC8D926) (tstamp ec83e1af-8d52-4c87-ac1d-4a373ec9d3a3)
    (at 123.825 126.365)
    (descr "SMD capacitor, aluminum electrolytic nonpolar, 5.0x5.8mm")
    (tags "capacitor electrolyic nonpolar")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/15e06373-ef72-4bda-bfe2-3c447d1417c6")
    (attr smd)
    (fp_text reference "C24" (at 0 -3.7) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e71f9ee2-ed72-4682-bc28-c28ec7210e27)
    )
    (fp_text value "10uF" (at 0 3.7) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 005770f1-5fc0-4185-8b97-18ffbefc4a24)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b221b348-7d1e-4e03-b012-1fcb4a2754a0)
    )
    (fp_line (start -2.76 1.695563) (end -2.76 1.06) (layer "F.SilkS") (width 0.12) (tstamp 0546284b-fc34-4195-b800-3de16a92435d))
    (fp_line (start 2.76 2.76) (end 2.76 1.06) (layer "F.SilkS") (width 0.12) (tstamp 1503e0db-e48d-4465-b028-5ea9b8b2fce5))
    (fp_line (start -2.76 1.695563) (end -1.695563 2.76) (layer "F.SilkS") (width 0.12) (tstamp 7b245103-a438-40fc-92dd-d21057987500))
    (fp_line (start -2.76 -1.695563) (end -1.695563 -2.76) (layer "F.SilkS") (width 0.12) (tstamp ace31c4c-0d4c-47ee-b04b-473eb8c1f258))
    (fp_line (start -1.695563 2.76) (end 2.76 2.76) (layer "F.SilkS") (width 0.12) (tstamp bdc444de-d4fd-4ee7-aee4-28f1b410204b))
    (fp_line (start -1.695563 -2.76) (end 2.76 -2.76) (layer "F.SilkS") (width 0.12) (tstamp d632191c-0d47-4d70-b4bb-9a11d5fcd97c))
    (fp_line (start 2.76 -2.76) (end 2.76 -1.06) (layer "F.SilkS") (width 0.12) (tstamp d7095964-204f-42d3-8591-8b941325a57e))
    (fp_line (start -2.76 -1.695563) (end -2.76 -1.06) (layer "F.SilkS") (width 0.12) (tstamp f9afc203-ef95-418b-84f5-fc3833723b60))
    (fp_line (start 2.9 1.05) (end 2.9 2.9) (layer "F.CrtYd") (width 0.05) (tstamp 03503975-4393-40b5-af23-f9afd67f79b5))
    (fp_line (start -2.9 -1.05) (end -3.7 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 1339a14c-261b-46a7-920d-a653f8844317))
    (fp_line (start -2.9 1.05) (end -2.9 1.75) (layer "F.CrtYd") (width 0.05) (tstamp 36b20108-e0f8-4e37-b9e2-dd12b695d182))
    (fp_line (start 3.7 1.05) (end 2.9 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 4aba5a85-649e-4702-b451-ef44c8eab37f))
    (fp_line (start -1.75 2.9) (end 2.9 2.9) (layer "F.CrtYd") (width 0.05) (tstamp 5b938bfb-fa76-47fd-a555-e3d7a5a48ce3))
    (fp_line (start 2.9 -1.05) (end 3.7 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 6024753a-5786-49ab-8997-dcc726e78da7))
    (fp_line (start -3.7 -1.05) (end -3.7 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 744eb02c-da5f-41cd-ae9c-9fdaafd68ba5))
    (fp_line (start 3.7 -1.05) (end 3.7 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 775b591d-0f68-48a9-89e6-b0bb879d8586))
    (fp_line (start -2.9 1.75) (end -1.75 2.9) (layer "F.CrtYd") (width 0.05) (tstamp 79e567a5-0a1c-40f0-9a92-27576d25cb47))
    (fp_line (start -3.7 1.05) (end -2.9 1.05) (layer "F.CrtYd") (width 0.05) (tstamp 9cf212f6-d6ed-4c8f-aa2a-36712db12da3))
    (fp_line (start 2.9 -2.9) (end 2.9 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp 9ea45435-4e48-4e7e-84b5-1d86abd9dbaf))
    (fp_line (start -2.9 -1.75) (end -2.9 -1.05) (layer "F.CrtYd") (width 0.05) (tstamp c817eba5-73e6-4992-9a81-0fc0abb787a4))
    (fp_line (start -2.9 -1.75) (end -1.75 -2.9) (layer "F.CrtYd") (width 0.05) (tstamp cac72bc5-0168-4c8a-a290-b6e0d2e8b1b7))
    (fp_line (start -1.75 -2.9) (end 2.9 -2.9) (layer "F.CrtYd") (width 0.05) (tstamp d809bffe-329c-4181-b746-987306e199db))
    (fp_line (start -1.65 -2.65) (end 2.65 -2.65) (layer "F.Fab") (width 0.1) (tstamp 17a76d58-25b1-4618-9177-610f027b50c9))
    (fp_line (start -2.65 -1.65) (end -2.65 1.65) (layer "F.Fab") (width 0.1) (tstamp 2fd927eb-3f83-4271-aaa4-7af6e772e543))
    (fp_line (start -2.65 1.65) (end -1.65 2.65) (layer "F.Fab") (width 0.1) (tstamp 7fff0f28-8c33-4979-8810-ac41a4177896))
    (fp_line (start 2.65 -2.65) (end 2.65 2.65) (layer "F.Fab") (width 0.1) (tstamp ad6ed826-a00c-46a4-b404-8f33dba8975f))
    (fp_line (start -1.65 2.65) (end 2.65 2.65) (layer "F.Fab") (width 0.1) (tstamp aff567cd-c19a-4efb-a238-b6e9efd3ee89))
    (fp_line (start -2.65 -1.65) (end -1.65 -2.65) (layer "F.Fab") (width 0.1) (tstamp fd5edcb7-bb62-4e60-98b2-8bf3522730ba))
    (fp_circle (center 0 0) (end 2.5 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 37a17ca2-39fd-4d6e-bd29-34826e63dce1))
    (pad "1" smd roundrect (at -2.0625 0) (size 2.775 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 18 "ADC_MIC") (pintype "passive") (tstamp 11447e35-e67e-4588-afc5-d2e8d57dd1cc))
    (pad "2" smd roundrect (at 2.0625 0) (size 2.775 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 35 "Net-(C24-Pad2)") (pintype "passive") (tstamp 0a2005c1-a767-4efb-a7fc-758b61ff7e37))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_5x5.8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp f078d555-3c48-4baf-9d76-5d605808989f)
    (at 68.58 118.11)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/075f8f3d-671e-4a44-9ba9-6fe5bba64202")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9ea8cd9f-1387-40ea-b07a-7119581089ef)
    )
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 86c800f6-90e0-4255-9cf8-d42b63156097)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 2dfc13d9-0c63-4920-a02a-e04f93d45ae1)
    )
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp 0cd0fa46-9cdf-446b-b433-ac8dd89d225a))
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 0f95c2cc-0bcd-4a73-9d3a-859faffd22ae))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 0e05dd7a-7988-429c-bd35-8b725417f3f7))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 129162e6-7821-4168-9d05-3dbc3fd225bd))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 213fabda-9b76-414c-b7fb-cf20418ec820))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 8f570875-5f10-4749-be03-1eecfce68464))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 3917556f-2b9a-4da9-8fe7-ebcf48b626c7))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp 74be337c-8708-4767-b1b8-4d2d891c3015))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp c11ed4b0-addd-44eb-ae36-1a6ccb38eec3))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp edf9e9f6-3f6f-4831-857b-98b7b0ac25e7))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "RF") (pintype "passive") (tstamp 0ac4d329-ecfb-4c88-ab74-a707ee6bb50a))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C5-Pad2)") (pintype "passive") (tstamp be22ffa9-b8c8-496c-895a-80fc5e63fbbd))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_SO:SO-14_3.9x8.65mm_P1.27mm" (layer "F.Cu")
    (tedit 5F427CE7) (tstamp f4a587e5-d3d6-46d0-88d1-d138fb655806)
    (at 80.645 69.85 90)
    (descr "SO, 14 Pin (https://www.st.com/resource/en/datasheet/l6491.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/65db4226-33a8-4398-b56e-b036b9a920b2")
    (attr smd)
    (fp_text reference "U1" (at 0 -5.28 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7e42ba22-fe8a-4c48-a03c-3223c45c4d9a)
    )
    (fp_text value "74HC14" (at 0 5.28 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dc016b67-3819-4be1-a99f-4534096979a8)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.98 0.98) (thickness 0.15)))
      (tstamp 4bc646e7-5265-422c-964a-c79d4fa4ac0d)
    )
    (fp_line (start 0 -4.435) (end 1.95 -4.435) (layer "F.SilkS") (width 0.12) (tstamp 46d152f1-f4cc-4f98-ae67-dfd3db0689d4))
    (fp_line (start 0 -4.435) (end -3.45 -4.435) (layer "F.SilkS") (width 0.12) (tstamp 5162bede-0086-48ca-9294-1b6bd0488a04))
    (fp_line (start 0 4.435) (end 1.95 4.435) (layer "F.SilkS") (width 0.12) (tstamp 6f208e2f-c74d-4334-9d0d-b19b39c147af))
    (fp_line (start 0 4.435) (end -1.95 4.435) (layer "F.SilkS") (width 0.12) (tstamp ce9091ba-7049-4cde-adcd-3a1afe0cb0a1))
    (fp_line (start -3.7 4.58) (end 3.7 4.58) (layer "F.CrtYd") (width 0.05) (tstamp 12109e7d-a81b-4b3c-8f5e-d5c402ffb6af))
    (fp_line (start -3.7 -4.58) (end -3.7 4.58) (layer "F.CrtYd") (width 0.05) (tstamp 4cc05254-d44e-4c96-85b9-05036332cc76))
    (fp_line (start 3.7 4.58) (end 3.7 -4.58) (layer "F.CrtYd") (width 0.05) (tstamp ea06ffaa-c50c-4b47-8348-95bb4a30adaa))
    (fp_line (start 3.7 -4.58) (end -3.7 -4.58) (layer "F.CrtYd") (width 0.05) (tstamp ee52e726-62c5-45fd-9661-ecc546ec284d))
    (fp_line (start -0.975 -4.325) (end 1.95 -4.325) (layer "F.Fab") (width 0.1) (tstamp 1dca78c8-933e-4fd6-8f58-79025249c085))
    (fp_line (start -1.95 4.325) (end -1.95 -3.35) (layer "F.Fab") (width 0.1) (tstamp 42f8d183-5c8c-4844-a9a7-06f5e523577d))
    (fp_line (start -1.95 -3.35) (end -0.975 -4.325) (layer "F.Fab") (width 0.1) (tstamp 5b3c2c78-27bb-42cd-bb78-e2f946c51696))
    (fp_line (start 1.95 -4.325) (end 1.95 4.325) (layer "F.Fab") (width 0.1) (tstamp 69542bf5-4c0a-4885-9d29-e6b333c410a1))
    (fp_line (start 1.95 4.325) (end -1.95 4.325) (layer "F.Fab") (width 0.1) (tstamp b26dd315-5c0a-4f04-9659-cd1faede5672))
    (pad "1" smd roundrect (at -2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "CLK0") (pintype "input") (tstamp efb74fe0-3f73-4551-95e0-8b4d57511b5b))
    (pad "2" smd roundrect (at -2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U1-Pad2)") (pintype "output") (tstamp bb3adc70-f568-4b72-ab36-7095a1141c04))
    (pad "3" smd roundrect (at -2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "CLK1") (pintype "input") (tstamp 57333622-222e-4594-a10d-4997468a2a3c))
    (pad "4" smd roundrect (at -2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U1-Pad4)") (pintype "output") (tstamp a2ac5fc0-f161-44bf-b056-5f48382747b5))
    (pad "5" smd roundrect (at -2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1-Pad5)") (pintype "input") (tstamp ee703964-d19f-42cc-98d9-a0a06780bda1))
    (pad "6" smd roundrect (at -2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(Q2-Pad2)") (pintype "output") (tstamp 1ab30531-1840-425d-87fa-e102fd3efe3e))
    (pad "7" smd roundrect (at -2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 7f16fb2b-d1ab-4026-9877-7d3a71c6c769))
    (pad "8" smd roundrect (at 2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(U1-Pad5)") (pintype "output") (tstamp 98e1c611-1088-4d94-af7e-7cd04c022a67))
    (pad "9" smd roundrect (at 2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "CLK0") (pintype "input") (tstamp d6482ddf-ed7c-4f6b-b996-7e207273f6e7))
    (pad "10" smd roundrect (at 2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(R7-Pad2)") (pintype "output") (tstamp 5e0db2c5-3b8e-4d76-b768-14d4be732451))
    (pad "11" smd roundrect (at 2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1-Pad11)") (pintype "input") (tstamp 51620bf6-4ea7-4ffa-b93c-05c8eea481cd))
    (pad "12" smd roundrect (at 2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1-Pad11)") (pintype "output") (tstamp a4fc410e-58d3-4804-a90b-3937319513a9))
    (pad "13" smd roundrect (at 2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "BIAS_PWM") (pintype "input") (tstamp 7f01c570-0f16-4497-a984-4c86cc3fcc64))
    (pad "14" smd roundrect (at 2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "+5V") (pinfunction "VCC") (pintype "power_in") (tstamp a76594ca-783c-407a-a375-cd5250ccaeb2))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-14_3.9x8.65mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp f92c6d62-a5a7-43a0-b9c1-db2f9d8c99b5)
    (at 257.82 35.44)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/9b310a87-67bf-4187-ac22-f61b20b95a6c")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f828cc21-fddc-420f-ab2c-234f032a7565)
    )
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b1038419-643c-4a0f-82c8-125cbad4ad00)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp c6b0b2fe-e5ea-4b48-84f6-05574c508084)
    )
    (fp_line (start -0.254724 -0.5225) (end 0.254724 -0.5225) (layer "F.SilkS") (width 0.12) (tstamp 577e6cf4-a835-4f70-add7-2f733031a375))
    (fp_line (start -0.254724 0.5225) (end 0.254724 0.5225) (layer "F.SilkS") (width 0.12) (tstamp be5ef4d0-0609-4131-901c-a141bb978055))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 056d24bb-127b-4319-8a44-83b85dd10266))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp 07316998-8bb9-485f-b642-f6f69786ce1d))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 7e395f34-ad01-46e9-ba05-dffd92529818))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp cb0b3e99-c1a3-4398-b45d-2f261d049d70))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 11c1136e-0908-40e8-b30a-35aabe297239))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp 6a743e9b-5de4-4603-8d21-75b321ac6ffe))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer "F.Fab") (width 0.1) (tstamp 6b50e9a0-77cc-46e2-a38b-708fee32ee3d))
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer "F.Fab") (width 0.1) (tstamp b06f271a-b096-422c-9938-f942eb958603))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(Q2-Pad2)") (pintype "passive") (tstamp d3fc684b-e4ec-4358-a763-68ffaeca2015))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(C11-Pad1)") (pintype "passive") (tstamp 1d888b1e-8487-46c0-b822-51a4babb52a3))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TestPoint:TestPoint_THTPad_D1.5mm_Drill0.7mm" (layer "F.Cu")
    (tedit 5A0F774F) (tstamp f9550da1-19e5-4d3f-b59f-f94cf14274a6)
    (at 71.755 93.98)
    (descr "THT pad as test Point, diameter 1.5mm, hole diameter 0.7mm")
    (tags "test point THT pad")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/f1eae4af-f502-483e-bd95-2699d20d52ba")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at 0 -1.648) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3dbdf080-b4e0-4a9f-87a1-67e5f0e96692)
    )
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6b6b178b-90da-4e7e-983c-33f93cb1875c)
    )
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9058a024-1cde-479a-9ca1-f160a301e4fd)
    )
    (fp_circle (center 0 0) (end 0 0.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp d99fcf1b-acb3-4e45-bb80-e21e17e7b597))
    (fp_circle (center 0 0) (end 1.25 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 60da2cf9-e33f-4e32-9e0d-95c9c6e612fd))
    (pad "1" thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(C9-Pad1)") (pinfunction "1") (pintype "passive") (tstamp aa336ff8-1b71-4de1-8332-0f7c59df626c))
  )

  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF) (tstamp fdd95d55-6c43-40fe-b004-36b4a88e7622)
    (at 86.995 89.3075 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "File: opensdx.pro.kicad_sch")
    (property "Sheetname" "")
    (path "/64b7680c-f3dc-4bef-a62d-4c365aef8c69")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.43 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 50a52243-1e1b-4554-9011-e6682b49ba4e)
    )
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e4c05158-2c49-4e5e-b0c2-f21202377e84)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 0.4 0.4) (thickness 0.06)))
      (tstamp 58279ea9-79d1-4019-b4a6-c46f57db6373)
    )
    (fp_line (start -0.146267 0.51) (end 0.146267 0.51) (layer "F.SilkS") (width 0.12) (tstamp 1d97d51e-e876-4cca-9c73-2be25f8adf92))
    (fp_line (start -0.146267 -0.51) (end 0.146267 -0.51) (layer "F.SilkS") (width 0.12) (tstamp e65e62db-9412-4d6c-8f08-9eb7a7d0b6e9))
    (fp_line (start 1.65 -0.73) (end 1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 2ab87868-54d4-4a2c-8c49-27cdb98ab2ec))
    (fp_line (start 1.65 0.73) (end -1.65 0.73) (layer "F.CrtYd") (width 0.05) (tstamp 7f1fcbfc-c46f-412d-aba7-9308d38d3d00))
    (fp_line (start -1.65 -0.73) (end 1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp aa96dc06-80aa-4c5d-8f72-f849e64c424a))
    (fp_line (start -1.65 0.73) (end -1.65 -0.73) (layer "F.CrtYd") (width 0.05) (tstamp f944ee9c-e051-4843-8b22-0df14389e385))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp 6837352f-9708-4037-bb5f-b8732eed3e5f))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer "F.Fab") (width 0.1) (tstamp a9bce28f-63a8-445f-9596-63dcb789ffd6))
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp c8c21a7f-fb4a-48e1-a5ad-feeb5eccc2d5))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer "F.Fab") (width 0.1) (tstamp fbcb6767-ed13-4a45-aa7f-f342ca54c870))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(C17-Pad2)") (pintype "passive") (tstamp 7d241ab9-364d-46b2-b03b-b72dd1c44390))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "ADC_I") (pintype "passive") (tstamp 8eb4fa83-d883-405c-b0a1-10d9b472d575))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (segment (start 64.46 94.94) (end 65.42 93.98) (width 0.25) (layer "F.Cu") (net 9) (tstamp 0e4acca7-0d64-4a34-bc12-072d23592dc1))
  (segment (start 66.04 93.98) (end 71.755 93.98) (width 0.25) (layer "F.Cu") (net 9) (tstamp 6d5426c1-1328-4f9c-b6f9-7df0e39624eb))
  (segment (start 65.42 93.98) (end 66.04 93.98) (width 0.25) (layer "F.Cu") (net 9) (tstamp 78b407a5-7e96-44f4-8eb8-fd0c69d69db4))
  (segment (start 63.1875 94.94) (end 64.46 94.94) (width 0.25) (layer "F.Cu") (net 9) (tstamp b9d7b4e6-afc2-41d9-aa4d-bce88b88449a))
  (segment (start 71.755 93.98) (end 78.9025 93.98) (width 0.25) (layer "F.Cu") (net 9) (tstamp d6f231af-aeab-4a5f-bd9b-1df617475264))
  (segment (start 71.755 97.79) (end 78.9025 97.79) (width 0.25) (layer "F.Cu") (net 10) (tstamp 1d178ab6-b431-4105-b8e4-39e49c51c12b))
  (segment (start 63.925 96.24) (end 65.0675 97.3825) (width 0.25) (layer "F.Cu") (net 10) (tstamp 44f8878d-84fd-4bbb-b4d3-a76ef9d80d4d))
  (segment (start 68.58 97.79) (end 67.49 97.79) (width 0.25) (layer "F.Cu") (net 10) (tstamp 46d8174b-bb27-4d62-bcf2-1a00a78151d9))
  (segment (start 68.58 97.79) (end 71.755 97.79) (width 0.25) (layer "F.Cu") (net 10) (tstamp 587fa9d2-3bc4-4398-8077-b6897bab86f3))
  (segment (start 67.49 97.79) (end 67.0825 97.3825) (width 0.25) (layer "F.Cu") (net 10) (tstamp 6bce424f-a8fa-44de-8bfe-210d201fea68))
  (segment (start 65.0675 97.3825) (end 67.0825 97.3825) (width 0.25) (layer "F.Cu") (net 10) (tstamp aea2ad1e-2c62-4c42-a51a-f51e2de7fb3c))
  (segment (start 63.1875 96.24) (end 63.925 96.24) (width 0.25) (layer "F.Cu") (net 10) (tstamp b3d698f3-9664-4fe7-ab03-7c2cbebecc63))
  (segment (start 64.475 95.59) (end 65.405 96.52) (width 0.25) (layer "F.Cu") (net 12) (tstamp 1abe0dc7-8a0e-4585-9ae0-5476bcb6cb05))
  (segment (start 63.1875 95.59) (end 64.475 95.59) (width 0.25) (layer "F.Cu") (net 12) (tstamp 63a09d1c-831d-471c-9ddc-22ff9ddaf183))
  (segment (start 68.58 96.52) (end 69.215 95.885) (width 0.25) (layer "F.Cu") (net 12) (tstamp 66d37adb-e352-4f96-b436-b289b955f3e0))
  (segment (start 74.295 95.885) (end 78.9025 95.885) (width 0.25) (layer "F.Cu") (net 12) (tstamp 81e053bc-7f0b-42d3-a927-3a20ba318655))
  (segment (start 65.405 96.52) (end 66.04 96.52) (width 0.25) (layer "F.Cu") (net 12) (tstamp 8e20b72e-36ea-403c-b2a5-c8afacce81be))
  (segment (start 69.215 95.885) (end 74.295 95.885) (width 0.25) (layer "F.Cu") (net 12) (tstamp e00ac982-64db-4a5f-977d-5d035fd261e7))
  (segment (start 66.04 96.52) (end 68.58 96.52) (width 0.25) (layer "F.Cu") (net 12) (tstamp ee877a55-bcf5-4b8c-8b9b-a14aee6685ac))
  (segment (start 66.510495 93.1175) (end 67.552995 92.075) (width 0.25) (layer "F.Cu") (net 13) (tstamp 0f13b809-fe99-4a44-9c42-64435319b89f))
  (segment (start 63.1875 94.29) (end 64.397005 94.29) (width 0.25) (layer "F.Cu") (net 13) (tstamp 353455d7-7c90-4254-ae0c-de57d0488767))
  (segment (start 67.552995 92.075) (end 68.58 92.075) (width 0.25) (layer "F.Cu") (net 13) (tstamp 407c6125-bf9a-4080-9fec-c771e024bd81))
  (segment (start 64.397005 94.29) (end 65.569505 93.1175) (width 0.25) (layer "F.Cu") (net 13) (tstamp 4ee8bcf9-2b4c-4164-9ee1-3bf92471ddae))
  (segment (start 68.58 92.075) (end 74.295 92.075) (width 0.25) (layer "F.Cu") (net 13) (tstamp a3e67e58-db7f-440d-9f0d-fef3f1e919e8))
  (segment (start 65.569505 93.1175) (end 66.510495 93.1175) (width 0.25) (layer "F.Cu") (net 13) (tstamp c9b48e55-8e13-4a12-83b9-e01f7a4f6df2))
  (segment (start 74.295 92.075) (end 78.9025 92.075) (width 0.25) (layer "F.Cu") (net 13) (tstamp fda27bd7-0bb8-4c8e-a779-7b1794d693e8))
  (segment (start 99.695 89.08) (end 99.695 86.36) (width 0.25) (layer "F.Cu") (net 14) (tstamp 3db566ed-d307-438a-96ba-1482c2c6301b))
  (segment (start 98.425 86.36) (end 99.695 86.36) (width 0.25) (layer "F.Cu") (net 14) (tstamp c3de8737-b68c-4736-9cf2-fc1d1fb2e5a4))
  (segment (start 99.695 86.36) (end 100.965 86.36) (width 0.25) (layer "F.Cu") (net 14) (tstamp cf0a2b9f-9c4a-44f6-bccd-3435c199fcf4))
  (segment (start 86.995 86.36) (end 86.995 84.455) (width 0.25) (layer "F.Cu") (net 15) (tstamp 21ce61fe-5dcf-460a-98cb-0438ec09c061))
  (segment (start 88.265 86.36) (end 86.995 86.36) (width 0.25) (layer "F.Cu") (net 15) (tstamp 8790fa2c-d5d6-4fef-bbc8-076b2b1c9a06))
  (segment (start 86.995 88.445) (end 86.995 86.36) (width 0.25) (layer "F.Cu") (net 15) (tstamp b8797e62-2372-4efe-9f0c-bebef50fbf27))
  (segment (start 85.725 86.36) (end 86.995 86.36) (width 0.25) (layer "F.Cu") (net 15) (tstamp fc67d882-e226-4238-92e3-d296d6fced03))
  (segment (start 88.4275 91.44) (end 87.7125 92.155) (width 0.25) (layer "F.Cu") (net 39) (tstamp 3c747d86-4cd1-4e00-8ad9-a7c24eaae6d7))
  (segment (start 85.19 92.155) (end 85.09 92.255) (width 0.25) (layer "F.Cu") (net 39) (tstamp 4c054a0d-1c91-42e8-a59d-0094f3e8a1cb))
  (segment (start 86.995 92.155) (end 86.995 90.17) (width 0.25) (layer "F.Cu") (net 39) (tstamp 4f83a82d-de8f-472c-9898-5ba6608e61db))
  (segment (start 86.995 92.155) (end 85.19 92.155) (width 0.25) (layer "F.Cu") (net 39) (tstamp 95ba7fa2-cef7-44e5-8b25-647ed3f638a4))
  (segment (start 87.7125 92.155) (end 86.5225 92.155) (width 0.25) (layer "F.Cu") (net 39) (tstamp c2978b5a-c439-44ed-978d-f331d4275dab))
  (segment (start 89.5275 91.44) (end 88.4275 91.44) (width 0.25) (layer "F.Cu") (net 39) (tstamp dc658eff-be30-4ed7-801f-81c4f3c7789d))
  (segment (start 89.5275 92.71) (end 91.1225 92.71) (width 0.25) (layer "F.Cu") (net 40) (tstamp 6977bacf-948c-4d9a-9d55-09cd70b63936))
  (segment (start 83.9825 97.155) (end 82.7125 95.885) (width 0.25) (layer "F.Cu") (net 40) (tstamp 8373b7fa-e712-42be-82c6-4942f5e80428))
  (segment (start 91.7575 93.345) (end 91.7575 96.52) (width 0.25) (layer "F.Cu") (net 40) (tstamp 94b51777-0d12-4bac-a88e-1f3b33fca034))
  (segment (start 91.1225 97.155) (end 83.9825 97.155) (width 0.25) (layer "F.Cu") (net 40) (tstamp 9cf97b92-3a9c-40f0-8d57-1eca061f6348))
  (segment (start 91.7575 96.52) (end 91.1225 97.155) (width 0.25) (layer "F.Cu") (net 40) (tstamp a9773b94-69b1-4746-9525-8177db1bbb83))
  (segment (start 91.1225 92.71) (end 91.7575 93.345) (width 0.25) (layer "F.Cu") (net 40) (tstamp b4e174ab-f8d5-4f3f-9a86-353d760488a5))
  (segment (start 82.7125 95.885) (end 80.7275 95.885) (width 0.25) (layer "F.Cu") (net 40) (tstamp b5010d85-cf02-4e59-b3ca-82a3a8faa556))
  (segment (start 80.7275 93.98) (end 89.5275 93.98) (width 0.25) (layer "F.Cu") (net 41) (tstamp d3b430e9-a47b-463a-8e5c-d7e335ecef16))
  (segment (start 80.7275 97.79) (end 91.6025 97.79) (width 0.25) (layer "F.Cu") (net 56) (tstamp 0b104229-829c-4581-afcb-9ffcb93fa326))
  (segment (start 98.8225 94.535) (end 99.3775 94.535) (width 0.25) (layer "F.Cu") (net 56) (tstamp 13ff7076-6676-4f3b-a841-2ef06ee4f28f))
  (segment (start 99.3775 94.535) (end 101.1825 94.535) (width 0.25) (layer "F.Cu") (net 56) (tstamp 1a89a8a1-f9b5-4298-8c9b-a493eedb3923))
  (segment (start 101.1825 94.535) (end 101.2825 94.435) (width 0.25) (layer "F.Cu") (net 56) (tstamp 95f132b1-d54e-4da9-a83b-89914f60e513))
  (segment (start 98.1075 95.25) (end 98.8225 94.535) (width 0.25) (layer "F.Cu") (net 56) (tstamp 9ae1c980-b029-4afe-a309-fe1618c1cfdd))
  (segment (start 96.5275 95.25) (end 98.1075 95.25) (width 0.25) (layer "F.Cu") (net 56) (tstamp a4d49e6f-ec7e-42c5-abbc-964701f6cde6))
  (segment (start 91.7575 97.79) (end 94.2975 95.25) (width 0.25) (layer "F.Cu") (net 56) (tstamp a79d2547-984e-4f80-885e-dbdaa3703e1b))
  (segment (start 94.2975 95.25) (end 96.5275 95.25) (width 0.25) (layer "F.Cu") (net 56) (tstamp ff018666-6e06-4f3e-8e74-9717edb6fd50))
  (segment (start 83.495 89.3075) (end 80.7275 92.075) (width 0.25) (layer "F.Cu") (net 57) (tstamp 02109497-5654-4e55-9dcd-d88e0959a49a))
  (segment (start 90.105 89.3075) (end 83.495 89.3075) (width 0.25) (layer "F.Cu") (net 57) (tstamp 2145c90b-700c-4fa8-94b1-25efc4795423))
  (segment (start 94.7775 93.98) (end 90.105 89.3075) (width 0.25) (layer "F.Cu") (net 57) (tstamp 3a019da2-4f6b-47c7-9c51-33e73132d8bb))
  (segment (start 96.5275 93.98) (end 94.7775 93.98) (width 0.25) (layer "F.Cu") (net 57) (tstamp 89ed1104-f99a-4f6c-b253-7c299436a2ec))
  (segment (start 99.3775 92.71) (end 96.5275 92.71) (width 0.25) (layer "F.Cu") (net 58) (tstamp 43de8499-0bd4-41b5-8226-28e44bc8dfb7))
  (segment (start 99.695 92.71) (end 99.695 90.805) (width 0.25) (layer "F.Cu") (net 58) (tstamp 9c130fe5-9f3a-4f1d-a23b-263b7a6521aa))
  (segment (start 99.3775 92.71) (end 101.2825 92.71) (width 0.25) (layer "F.Cu") (net 58) (tstamp dfe9cfda-3959-4599-a66f-3360e40580cc))

)
