(footprint "transformer_bifilar" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 621BE484)
  (property "Sheetfile" "File: dart50-pa-prototype.kicad_sch")
  (property "Sheetname" "")
  (attr through_hole)
  (fp_text reference "L4" (at 5.08 -12.7 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 36875dd7-af16-4002-b7b2-db5a067edd91)
  )
  (fp_text value "FT43-37 10t bifilar" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c7732d8c-c345-488b-833a-a0837c779102)
  )
  (fp_line (start -1.27 -2.54) (end 1.27 -2.54) (layer "F.SilkS") (width 0.15) (tstamp 23dd559b-6f8b-41c4-b045-6a1baa59e4ab))
  (fp_line (start -1.27 2.54) (end 1.27 2.54) (layer "F.SilkS") (width 0.15) (tstamp cb6e1c6e-c29b-4503-be9e-1c060c84c66b))
  (fp_rect (start -2.54 -6.35) (end 2.54 6.35) (layer "F.SilkS") (width 0.15) (fill none) (tstamp c7445ff1-564f-46f0-acba-74f1ff9f97e4))
  (pad "1" thru_hole rect (at -3.81 -2.54) (size 3 1.5) (drill 0.762) (layers *.Cu *.Mask) (tstamp 73d60599-f8ce-4985-b797-3dbb7a5fb9ba))
  (pad "2" thru_hole oval (at 3.81 -2.54) (size 3 1.5) (drill 0.762) (layers *.Cu *.Mask) (tstamp 5fecce9d-808e-40dc-bb0b-2b1070fef933))
  (pad "3" thru_hole oval (at -3.81 2.54) (size 3 1.5) (drill 0.762) (layers *.Cu *.Mask) (tstamp 2428b798-3115-4b18-8b7c-3d2bfb42359f))
  (pad "4" thru_hole oval (at 3.81 2.54) (size 3 1.5) (drill 0.762) (layers *.Cu *.Mask) (tstamp c87e1aad-ceb2-4a82-8fa2-e9046052a4a7))
)
