(export (version D)
  (design
    (source /home/sebastian/projects/AS5043-encoder/pcb/sensor-board.sch)
    (date "Mon 07 Dec 2015 11:43:18 AM CET")
    (tool "Eeschema (2015-11-02 BZR 6290)-product")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "AS5043 encoder")
        (company)
        (rev)
        (date 2015-12-07)
        (source sensor-board.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R4)
      (value 10k)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F292BF0))
    (comp (ref C3)
      (value 100pf)
      (footprint smd_capacitors:c_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F242FCD))
    (comp (ref R3)
      (value 47k)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F242F4C))
    (comp (ref R2)
      (value 33k)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F242E8E))
    (comp (ref R1)
      (value 33k)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F242E7F))
    (comp (ref C1)
      (value 5uF)
      (footprint smd_capacitors:c_tant_A)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F242986))
    (comp (ref C2)
      (value 100nF)
      (footprint smd_capacitors:c_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F242939))
    (comp (ref P1)
      (value CONN_5X2)
      (footprint he10-lock:he10-lock)
      (libsource (lib conn) (part CONN_5X2))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F21BD0B))
    (comp (ref U1)
      (value AS5043)
      (footprint lib:SSOP16_WIDE)
      (libsource (lib as5043) (part AS5043))
      (sheetpath (names /) (tstamps /))
      (tstamp 4F21BC93))
    (comp (ref D1)
      (value LED)
      (footprint led:LED-0603)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 4FCB8666))
    (comp (ref R5)
      (value 1k)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4FCB868E))
    (comp (ref D2)
      (value LED)
      (footprint led:LED-0603)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 4FCCEFE9))
    (comp (ref R6)
      (value 1k)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 4FCCEFEF)))
  (libparts
    (libpart (lib as5043) (part AS5043)
      (fields
        (field (name Reference) U)
        (field (name Value) AS5043))
      (pins
        (pin (num 1) (name MAGRNGN) (type input))
        (pin (num 2) (name MODE) (type input))
        (pin (num 3) (name CS) (type input))
        (pin (num 4) (name CLK) (type input))
        (pin (num 6) (name DO) (type input))
        (pin (num 7) (name VSS) (type input))
        (pin (num 8) (name Prog) (type input))
        (pin (num 9) (name DACref) (type input))
        (pin (num 10) (name ADCout) (type input))
        (pin (num 11) (name FB) (type input))
        (pin (num 12) (name Vout) (type input))
        (pin (num 15) (name VDD3V3) (type input))
        (pin (num 16) (name VDD5V) (type input))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib conn) (part CONN_5X2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_5X2))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive)))))
  (libraries
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical as5043)
      (uri /home/sebastian/projects/AS5043-encoder/pcb/lib/as5043.lib))
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib)))
  (nets
    (net (code 1) (name "Net-(C3-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref P1) (pin 10))
      (node (ref U1) (pin 12)))
    (net (code 2) (name GND)
      (node (ref R2) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 7))
      (node (ref C1) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref P1) (pin 4))
      (node (ref P1) (pin 8))
      (node (ref P1) (pin 6)))
    (net (code 3) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref U1) (pin 15)))
    (net (code 4) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R5) (pin 1)))
    (net (code 5) (name "Net-(R5-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref U1) (pin 1)))
    (net (code 6) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R6) (pin 1)))
    (net (code 7) (name +5V)
      (node (ref P1) (pin 2))
      (node (ref D2) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref U1) (pin 16)))
    (net (code 8) (name "Net-(R1-Pad2)")
      (node (ref U1) (pin 11))
      (node (ref R2) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 9) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 10)))
    (net (code 10) (name "Net-(U1-Pad9)")
      (node (ref U1) (pin 9)))
    (net (code 11) (name /CS)
      (node (ref U1) (pin 3))
      (node (ref P1) (pin 7)))
    (net (code 12) (name /PROG)
      (node (ref U1) (pin 8))
      (node (ref P1) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 13) (name /DO)
      (node (ref U1) (pin 6))
      (node (ref P1) (pin 3)))
    (net (code 14) (name /CLK)
      (node (ref U1) (pin 4))
      (node (ref P1) (pin 5)))
    (net (code 15) (name /MODE)
      (node (ref P1) (pin 9))
      (node (ref U1) (pin 2)))))