(export (version D)
  (design
    (source /home/sebastian/projects/7segment_timer/board/driverboard.sch)
    (date "Sun 26 Jan 2014 01:00:54 AM CET")
    (tool "eeschema (2013-may-18)-stable"))
  (components
    (comp (ref J1)
      (value RJ45)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC23CC))
    (comp (ref J2)
      (value RJ45)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC2875))
    (comp (ref P1)
      (value HE10-10)
      (libsource (lib conn) (part HE10-10))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC2924))
    (comp (ref C3)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC346F))
    (comp (ref C2)
      (value 10uF)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC348D))
    (comp (ref C5)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC350A))
    (comp (ref C4)
      (value 10uF)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC3510))
    (comp (ref R2)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC367C))
    (comp (ref D3)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC36E5))
    (comp (ref R1)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC37A6))
    (comp (ref D1)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC37AD))
    (comp (ref U1)
      (value 74HC595)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC3814))
    (comp (ref C1)
      (value 100n)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC3C4B))
    (comp (ref R10)
      (value 200)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC3E80))
    (comp (ref R18)
      (value 470)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC40ED))
    (comp (ref R9)
      (value 200)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41BE))
    (comp (ref R17)
      (value 470)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41CB))
    (comp (ref R8)
      (value 200)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41D9))
    (comp (ref R16)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41E6))
    (comp (ref R7)
      (value 200)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41F4))
    (comp (ref R15)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4201))
    (comp (ref R6)
      (value 200)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC420F))
    (comp (ref R14)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC421C))
    (comp (ref R5)
      (value 200)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC422A))
    (comp (ref R13)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4237))
    (comp (ref R4)
      (value 200)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4245))
    (comp (ref R12)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4252))
    (comp (ref R3)
      (value 200)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4260))
    (comp (ref R11)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC426D))
    (comp (ref D2)
      (value BAT42W)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E410B2))
    (comp (ref U2)
      (value TS2937)
      (libsource (lib ts2937) (part TS2937))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E445FE))
    (comp (ref Q1)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44C4E))
    (comp (ref Q2)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D2E))
    (comp (ref Q3)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D34))
    (comp (ref Q4)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D3A))
    (comp (ref Q5)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D40))
    (comp (ref Q6)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D46))
    (comp (ref Q7)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D4C))
    (comp (ref Q8)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D52)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part DIODE)
      (description "Diode simple")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part HE10-10)
      (fields
        (field (name Reference) P)
        (field (name Value) HE10-10)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))))
    (libpart (lib conn) (part RJ45)
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name SHIELD) (type passive))))
    (libpart (lib 74xx) (part 74HC595)
      (description "8 bits serial in // out Shift Register 3 State Out")
      (docs 74xx/74HC595.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 74HC595)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name QB) (type 3state))
        (pin (num 2) (name QC) (type 3state))
        (pin (num 3) (name QD) (type 3state))
        (pin (num 4) (name QE) (type 3state))
        (pin (num 5) (name QF) (type 3state))
        (pin (num 6) (name QG) (type 3state))
        (pin (num 7) (name QH) (type 3state))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name ~QH) (type output))
        (pin (num 10) (name SRCLR) (type input))
        (pin (num 11) (name SRCLK) (type input))
        (pin (num 12) (name RCLK) (type input))
        (pin (num 13) (name G) (type input))
        (pin (num 14) (name SER) (type input))
        (pin (num 15) (name QA) (type 3state))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib ts2937) (part TS2937)
      (fields
        (field (name Reference) U)
        (field (name Value) TS2937)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VI) (type input))
        (pin (num 2) (name GND) (type input))
        (pin (num 3) (name VO) (type power_out))))
    (libpart (lib nds355) (part NDS355)
      (fields
        (field (name Reference) Q)
        (field (name Value) NDS355)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical nds355)
      (uri lib/nds355.lib))
    (library (logical ts2937)
      (uri lib/ts2937.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref Q4) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 2) (name SEG_3)
      (node (ref R13) (pin 2))
      (node (ref P1) (pin 7)))
    (net (code 3) (name "")
      (node (ref R13) (pin 1))
      (node (ref Q3) (pin 3)))
    (net (code 4) (name "")
      (node (ref R5) (pin 1))
      (node (ref Q3) (pin 1)))
    (net (code 5) (name "")
      (node (ref R14) (pin 1))
      (node (ref Q4) (pin 3)))
    (net (code 6) (name SEG_4)
      (node (ref P1) (pin 8))
      (node (ref R14) (pin 2)))
    (net (code 7) (name "")
      (node (ref R15) (pin 1))
      (node (ref Q5) (pin 3)))
    (net (code 8) (name SEG_5)
      (node (ref R15) (pin 2))
      (node (ref P1) (pin 5)))
    (net (code 9) (name "")
      (node (ref R7) (pin 1))
      (node (ref Q5) (pin 1)))
    (net (code 10) (name "")
      (node (ref R16) (pin 1))
      (node (ref Q6) (pin 3)))
    (net (code 11) (name "")
      (node (ref Q1) (pin 3))
      (node (ref R11) (pin 1)))
    (net (code 12) (name FET_6)
      (node (ref U1) (pin 5))
      (node (ref R8) (pin 2)))
    (net (code 13) (name FET_4)
      (node (ref U1) (pin 3))
      (node (ref R6) (pin 2)))
    (net (code 14) (name FET_2)
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 1)))
    (net (code 15) (name FET_7)
      (node (ref R9) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 16) (name FET_5)
      (node (ref R7) (pin 2))
      (node (ref U1) (pin 4)))
    (net (code 17) (name FET_3)
      (node (ref U1) (pin 2))
      (node (ref R5) (pin 2)))
    (net (code 18) (name FET_1)
      (node (ref R3) (pin 2))
      (node (ref U1) (pin 15)))
    (net (code 19) (name SEG_1)
      (node (ref R11) (pin 2))
      (node (ref P1) (pin 9)))
    (net (code 20) (name +24V)
      (node (ref Q8) (pin 2))
      (node (ref Q7) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref J2) (pin 4))
      (node (ref J2) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref Q4) (pin 2))
      (node (ref Q5) (pin 2))
      (node (ref Q2) (pin 2))
      (node (ref Q6) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref Q3) (pin 2))
      (node (ref U2) (pin 1)))
    (net (code 21) (name "")
      (node (ref R3) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 22) (name "")
      (node (ref Q2) (pin 3))
      (node (ref R12) (pin 1)))
    (net (code 23) (name SEG_2)
      (node (ref R12) (pin 2))
      (node (ref P1) (pin 10)))
    (net (code 24) (name "")
      (node (ref R4) (pin 1))
      (node (ref Q2) (pin 1)))
    (net (code 25) (name SEG_8)
      (node (ref P1) (pin 4))
      (node (ref R18) (pin 2)))
    (net (code 26) (name "")
      (node (ref Q8) (pin 1))
      (node (ref R10) (pin 1)))
    (net (code 27) (name Data_Out)
      (node (ref U1) (pin 9))
      (node (ref J2) (pin 5)))
    (net (code 28) (name GND)
      (node (ref U1) (pin 8))
      (node (ref J1) (pin 6))
      (node (ref J2) (pin 6))
      (node (ref J2) (pin 8))
      (node (ref J2) (pin 9))
      (node (ref C1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref U1) (pin 13))
      (node (ref U2) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref P1) (pin 2))
      (node (ref J1) (pin 9))
      (node (ref J1) (pin 8)))
    (net (code 29) (name +5V)
      (node (ref D2) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 16))
      (node (ref C1) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref C4) (pin 1)))
    (net (code 30) (name Clock)
      (node (ref J2) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref U1) (pin 11)))
    (net (code 31) (name Data_In)
      (node (ref J1) (pin 5))
      (node (ref U1) (pin 14)))
    (net (code 32) (name SEG_6)
      (node (ref P1) (pin 6))
      (node (ref R16) (pin 2)))
    (net (code 33) (name "")
      (node (ref R8) (pin 1))
      (node (ref Q6) (pin 1)))
    (net (code 34) (name "")
      (node (ref R17) (pin 1))
      (node (ref Q7) (pin 3)))
    (net (code 35) (name SEG_7)
      (node (ref P1) (pin 3))
      (node (ref R17) (pin 2)))
    (net (code 36) (name "")
      (node (ref R9) (pin 1))
      (node (ref Q7) (pin 1)))
    (net (code 37) (name "")
      (node (ref Q8) (pin 3))
      (node (ref R18) (pin 1)))
    (net (code 38) (name FET_8)
      (node (ref R10) (pin 2))
      (node (ref U1) (pin 7)))
    (net (code 39) (name Reset)
      (node (ref J1) (pin 7))
      (node (ref J2) (pin 7))
      (node (ref U1) (pin 10)))
    (net (code 40) (name Enable)
      (node (ref J1) (pin 3))
      (node (ref U1) (pin 12))
      (node (ref J2) (pin 3)))
    (net (code 41) (name "")
      (node (ref D1) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 42) (name "")
      (node (ref D3) (pin 1))
      (node (ref R2) (pin 2)))))